IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [ConceptDesignBIM_2010, QuantityTakeOffAddOnView, SpaceBoundary2ndLevelAddOnView]"
Description: "Option [Entire project;Keep GUIDs;Space cont;CustProperty sets;Bounds;All Domain;All elements;All struct.;scale:100.000000;CSG:Extruded;Comp. wall:Extruded;Building element parts;Chained beam:Extruded;Comp. slab:Extruded]"
File name: "SMC Building.ifc"
Time stamp: "2012-10-15T16:41:27"
Author: "Architect"
Organization: "Building Designer Office"
Preprocessor: "PreProc - EDM 5.0"
Originating system: "IFC file generated by Graphisoft ArchiCAD-64 16.0.0 INT FULL Windows version (IFC2x3 add-on version: 3270 INT FULL)."
Authorization: "The authorising person"
Application: "ArchiCAD-64" version "16.0.0" identifier "IFC2x3 add-on version: 3270 INT FULL" by Organization "Graphisoft" id "GS" description "Graphisoft"

People and organizations
  Person "Undefined" of Organization "Undefined"
  Owner history of Person "Undefined" of Organization "Undefined" | application "ArchiCAD-64" version "16.0.0" identifier "IFC2x3 add-on version: 3270 INT FULL" by Organization "Graphisoft" id "GS" description "Graphisoft" | change ADDED | created 1350308450 (2012-10-15T13:40:50Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Default Project"
  IFCSITE "Default Site" | latitude 37° 48′ 0″ | longitude -122° 24′ 0″
    IFCBUILDING "SMC Building" | postal address (none given)
      IFCBUILDINGSTOREY "Ground floor" | long name "Ground floor" | elevation 0.
        contains 89 elements
          2 x IFCSTAIR | names: "Stair-01", "Stair-02" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Stair_Spiral_16, Pset_StairCommon, AC_Pset_Stair_U-Shape_16
          1 x IFCSLAB | FLOOR | names: "Slab-01" | material: layers "FS-1" ("Solid Fill" 300.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          9 x IFCCOVERING | CEILING | names: "Slab-7" | material: materials ("steel") | property sets: AC_Pset_Name, Pset_CoveringCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCSLAB | ROOF | names: "Roof-03" | material: materials ("Solid Fill") | property sets: AC_Pset_Name, Pset_SlabCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IW-5 30" | names: "EW-3" | material: layers "IW-5" ("Solid Fill" 30.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "D200" | object type "D200" | names: "Column-01", "Column-07", "Column-09" (+2 more) | material: "C-4" | property sets: AC_Pset_Name, Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          5 x IFCCOLUMN | type IFCCOLUMNTYPE "D300" | object type "C-2" | names: "Column-02", "Column-03", "Column-04" (+2 more) | material: "C-2" | property sets: AC_Pset_Name, Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "240X240" | object type "240X240" | names: "Column-08" | material: "C-1" | property sets: AC_Pset_Name, Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "D350" | object type "C-2" | names: "Column-12", "Column-13" | material: "C-2" | property sets: AC_Pset_Name, Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "EW-1 240" | names: "Wall-01", "Wall-02", "Wall-06" (+2 more) | material: layers "EW-1" ("face brick" 100., "Solid Fill" 140.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          13 x IFCWINDOW | type IFCWINDOWSTYLE "W1 14" | names: "Window-01", "Window-02", "Window-03" (+10 more) | material: "Solid Fill" | property sets: Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_W1_14, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "EW-5 100" | names: "Wall-03", "Wall-05", "Wall-04" | material: layers "EW-5" ("Solid Fill" 100.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          5 x IFCWINDOW | type IFCWINDOWSTYLE "Window 16" | names: "Window-26", "Window-07", "Window-08" (+2 more) | material: "Solid Fill" | property sets: Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Window_16, BaseQuantities
          7 x IFCWINDOW | type IFCWINDOWSTYLE "Double Sash Window 16" | names: "Window-24", "Window-23", "Window-25" (+4 more) | material: "Solid Fill" | property sets: Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Double_Sash_Window_16, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Entrance Door 16" | names: "Door-02" | material: "Solid Fill" | property sets: Pset_DoorCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Entrance_Door_16, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IW-2 150" | names: "Wall-09", "Wall-14", "Wall-15" | material: layers "IW-2" ("Solid Fill" 150.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCDOOR | type IFCDOORSTYLE "Metal Door 16" | names: "Door-03", "D-7" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Metal_Door_16, BaseQuantities
          2 x IFCDOOR | type IFCDOORSTYLE "Double Door with Transom 16" | names: "Door-05", "Door-04" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Double_Door_with_Transom_16, BaseQuantities
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IW-1 100" | names: "Wall-10", "Wall-11", "Wall-12" (+5 more) | material: layers "IW-1" ("Solid Fill" 100.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCDOOR | type IFCDOORSTYLE "Door 16" | names: "Door-06", "Door-07" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Door_16, BaseQuantities
          3 x IFCDOOR | type IFCDOORSTYLE "Door 16" | names: "Door-09", "Door-08", "Door-10" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Door_16, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IW-4 70" | names: "Wall-20", "Wall-21", "Wall-22" (+1 more) | material: layers "IW-4" ("Solid Fill" 70.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Sliding Door 16" | names: "Door-11" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Sliding_Door_16, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Revolving Door 16" | names: "Door-01" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_DoorCommon, AC_Pset_Revolving_Door_16, BaseQuantities
          1 x IFCGRID
        IFCSPACE "111" | long name "Stair" | INTERNAL
        IFCSPACE "125" | long name "Petty Education Inc." | INTERNAL
        IFCSPACE "140" | long name "Corridor" | INTERNAL
        IFCSPACE "102" | long name "Corridor" | INTERNAL
        IFCSPACE "110" | long name "Office" | INTERNAL
        IFCSPACE "109" | long name "Office" | INTERNAL
        IFCSPACE "108" | long name "Conference 2" | INTERNAL
        IFCSPACE "105" | long name "Women" | INTERNAL
          contains 1 element
            1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Basin 02 13" | names: "Obj.-587" | material: "Solid Fill" | property sets: AC_Pset_RenovationAndPhasing, AC_Pset_Basin_02_13
        IFCSPACE "104" | long name "Men" | INTERNAL
          contains 2 elements
            1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "WC with Cistern 13" | names: "Obj.-586" | material: "Solid Fill" | property sets: AC_Pset_RenovationAndPhasing, AC_Pset_WC_with_Cistern_13
            1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Basin 02 13" | names: "Obj.-587" | material: "Solid Fill" | property sets: AC_Pset_RenovationAndPhasing, AC_Pset_Basin_02_13
        IFCSPACE "103" | long name "Security" | INTERNAL
        IFCSPACE "101" | long name "Lobby" | INTERNAL
        IFCSPACE "112" | long name "Elevator" | INTERNAL
        IFCSPACE "127" | long name "Common Area" | INTERNAL
        IFCSPACE "134" | long name "Ground Floor Gross Area" | INTERNAL
        IFCSPACE "107" | long name "Stair" | INTERNAL
        IFCSPACE "106" | long name "Conference 1" | INTERNAL
        IFCSPACE "124" | long name "Education and Conference Area" | INTERNAL
      IFCBUILDINGSTOREY "First floor" | long name "First floor" | elevation 3700.
        contains 111 elements
          2 x IFCRAILING | HANDRAIL | names: "Obj.-581" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Railing_Horizontal
          1 x IFCSLAB | FLOOR | names: "Slab-02" | material: layers "FS-2" ("Solid Fill" 200.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCCOVERING | CEILING | names: "Slab-7" | material: materials ("steel") | property sets: AC_Pset_Name, Pset_CoveringCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IW-5 30" | names: "EW-3" | material: layers "IW-5" ("Solid Fill" 30.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          15 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IW-1 100" | names: "EW-3", "Wall-47", "Wall-46" (+11 more) | material: layers "IW-1" ("Solid Fill" 100.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          9 x IFCCOLUMN | type IFCCOLUMNTYPE "D200" | object type "D200" | names: "Column-22", "Column-23", "Column-21" (+6 more) | material: "C-4" | property sets: AC_Pset_Name, Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "EW-2 100" | names: "Wall-40", "Wall-39" | material: layers "EW-2" ("Solid Fill" 100.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IW-4 70" | names: "Wall-60", "Wall-62", "Wall-61" (+1 more) | material: layers "IW-4" ("Solid Fill" 70.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Sliding Door 16" | names: "Door-27" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Sliding_Door_16, BaseQuantities
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "EW-1 240" | names: "Wall-36", "Wall-38", "Wall-34" (+2 more) | material: layers "EW-1" ("face brick" 100., "Solid Fill" 140.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          5 x IFCWINDOW | type IFCWINDOWSTYLE "Window 16" | names: "Window-30", "Window-31", "Window-154" (+2 more) | material: "Solid Fill" | property sets: Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Window_16, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Storefront 16" | names: "Door-15" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_DoorCommon, AC_Pset_Storefront_16, BaseQuantities
          5 x IFCWINDOW | type IFCWINDOWSTYLE "Double Sash Window 16" | names: "Window-71", "Window-72", "Window-73" (+2 more) | material: "Solid Fill" | property sets: Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Double_Sash_Window_16, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IW-2 150" | names: "Wall-48", "Wall-51", "Wall-41" | material: layers "IW-2" ("Solid Fill" 150.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          7 x IFCDOOR | type IFCDOORSTYLE "Door 16" | names: "Door-22", "Door-23", "Door-21" (+4 more) | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Door_16, BaseQuantities
          3 x IFCDOOR | type IFCDOORSTYLE "Door 16" | names: "Door-26", "Door-24", "Door-25" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Door_16, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Metal Door 16" | names: "Door-16" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Metal_Door_16, BaseQuantities
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "EW-4 100" | names: "Wall-29", "Wall-32", "Wall-30" (+5 more) | material: layers "EW-4" ("Solid Fill" 100.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          35 x IFCWINDOW | type IFCWINDOWSTYLE "W1 14" | names: "Window-48", "Window-46", "Window-45" (+32 more) | material: "Solid Fill" | property sets: Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_W1_14, BaseQuantities
          2 x IFCSTAIR | names: "Stair-01", "Stair-02" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Stair_Spiral_16, Pset_StairCommon, AC_Pset_Stair_U-Shape_16
        IFCSPACE "231" | long name "Arbor Doves, Inc." | INTERNAL
        IFCSPACE "214" | long name "Stair" | INTERNAL
        IFCSPACE "241" | long name "Corridor" | INTERNAL
        IFCSPACE "206" | long name "Gym" | INTERNAL
        IFCSPACE "205" | long name "Kitchen" | INTERNAL
        IFCSPACE "209" | long name "Office" | INTERNAL
        IFCSPACE "210" | long name "Office" | INTERNAL
        IFCSPACE "211" | long name "Office" | INTERNAL
        IFCSPACE "202" | long name "Office" | INTERNAL
        IFCSPACE "203" | long name "Office" | INTERNAL
        IFCSPACE "208" | long name "Office" | INTERNAL
        IFCSPACE "204" | long name "Restroom" | INTERNAL
          contains 2 elements
            1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "WC with Cistern 13" | names: "Obj.-586" | material: "Solid Fill" | property sets: AC_Pset_RenovationAndPhasing, AC_Pset_WC_with_Cistern_13
            1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Basin 02 13" | names: "Obj.-587" | material: "Solid Fill" | property sets: AC_Pset_RenovationAndPhasing, AC_Pset_Basin_02_13
        IFCSPACE "212" | long name "Elevator" | INTERNAL
        IFCSPACE "228" | long name "Tomorrows Lubrication, Inc." | INTERNAL
        IFCSPACE "201" | long name "Lobby" | INTERNAL
        IFCSPACE "207" | long name "Stair" | INTERNAL
        IFCSPACE "235" | long name "First Floor Gross Area" | INTERNAL
        IFCSPACE "240" | long name "Corridor" | INTERNAL
        IFCSPACE "215" | long name "Office" | INTERNAL
        IFCSPACE "231" | long name "Common Area" | INTERNAL
        IFCSPACE "299" | long name "Pipe Shaft" | INTERNAL
      IFCBUILDINGSTOREY "Second floor" | long name "Second floor" | elevation 6750.
        contains 106 elements
          3 x IFCRAILING | HANDRAIL | names: "Obj.-581" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Railing_Horizontal
          1 x IFCSTAIR | names: "Stair-01" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Stair_Spiral_16
          2 x IFCSLAB | FLOOR | names: "Slab-03", "Slab-7" | material: layers "FS-2" ("Solid Fill" 200.); layers "FS-1" ("Solid Fill" 300.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCCOVERING | CEILING | names: "Slab-7" | material: materials ("steel") | property sets: AC_Pset_Name, Pset_CoveringCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          13 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IW-1 100" | names: "EW-3", "Wall-90", "Wall-92" (+9 more) | material: layers "IW-1" ("Solid Fill" 100.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          9 x IFCCOLUMN | type IFCCOLUMNTYPE "D200" | object type "D200" | names: "Column-43", "Column-40", "Column-41" (+6 more) | material: "C-4" | property sets: AC_Pset_Name, Pset_ColumnCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IW-4 70" | names: "Wall-98", "Wall-97", "Wall-99" (+1 more) | material: layers "IW-4" ("Solid Fill" 70.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Sliding Door 16" | names: "Door-43" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Sliding_Door_16, BaseQuantities
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "IW-2 150" | names: "Wall-88", "Wall-80", "Wall-89" | material: layers "IW-2" ("Solid Fill" 150.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "EW-1 240" | names: "Wall-72", "Wall-73", "Wall-74" (+2 more) | material: layers "EW-1" ("face brick" 100., "Solid Fill" 140.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          5 x IFCWINDOW | type IFCWINDOWSTYLE "Double Sash Window 16" | names: "Window-125", "Window-126", "Window-127" (+2 more) | material: "Solid Fill" | property sets: Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Double_Sash_Window_16, BaseQuantities
          5 x IFCWINDOW | type IFCWINDOWSTYLE "Window 16" | names: "Window-80", "Window-81", "Window-152" (+2 more) | material: "Solid Fill" | property sets: Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Window_16, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Metal Door 16" | names: "Door-30" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Metal_Door_16, BaseQuantities
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "EW-4 100" | names: "Wall-71", "Wall-65", "Wall-66" (+5 more) | material: layers "EW-4" ("Solid Fill" 100.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          35 x IFCWINDOW | type IFCWINDOWSTYLE "W1 14" | names: "Window-115", "Window-117", "Window-118" (+32 more) | material: "Solid Fill" | property sets: Pset_WindowCommon, AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_W1_14, BaseQuantities
          7 x IFCDOOR | type IFCDOORSTYLE "Door 16" | names: "Door-38", "Door-37", "Door-36" (+4 more) | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Door_16, BaseQuantities
          3 x IFCDOOR | type IFCDOORSTYLE "Door 16" | names: "Door-39", "Door-41", "Door-40" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, AC_Pset_Door_16, BaseQuantities
        IFCSPACE "336" | long name "Second Floor Gross Area" | INTERNAL
          contains 2 elements
            1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "WC with Cistern 13" | names: "Obj.-586" | material: "Solid Fill" | property sets: AC_Pset_RenovationAndPhasing, AC_Pset_WC_with_Cistern_13
            1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Basin 02 13" | names: "Obj.-587" | material: "Solid Fill" | property sets: AC_Pset_RenovationAndPhasing, AC_Pset_Basin_02_13
        IFCSPACE "333" | long name "Biochemical Startup, Inc." | INTERNAL
        IFCSPACE "320" | long name "Corridor" | INTERNAL
        IFCSPACE "307" | long name "Stair" | INTERNAL
        IFCSPACE "301" | long name "Lobby" | INTERNAL
        IFCSPACE "231" | long name "Common Area" | INTERNAL
        IFCSPACE "313" | long name "Stair" | INTERNAL
        IFCSPACE "342" | long name "Corridor" | INTERNAL
        IFCSPACE "311" | long name "Office" | INTERNAL
        IFCSPACE "310" | long name "Office" | INTERNAL
        IFCSPACE "309" | long name "Office" | INTERNAL
        IFCSPACE "308" | long name "Office" | INTERNAL
        IFCSPACE "315" | long name "Office" | INTERNAL
        IFCSPACE "304" | long name "Restroom" | INTERNAL
        IFCSPACE "305" | long name "Kitchen" | INTERNAL
        IFCSPACE "306" | long name "Office" | INTERNAL
        IFCSPACE "303" | long name "Office" | INTERNAL
        IFCSPACE "302" | long name "Office" | INTERNAL
        IFCSPACE "399" | long name "Pipe Shaft" | INTERNAL
        IFCSPACE "312" | long name "Elevator" | INTERNAL
      IFCBUILDINGSTOREY "Roof" | long name "Roof" | elevation 9800.
        contains 22 elements
          1 x IFCSLAB | FLOOR | names: "Slab-04" | material: layers "FS-2" ("Solid Fill" 200.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, BaseQuantities
          2 x IFCSLAB | ROOF | names: "Roof-01", "Roof-02" | material: materials ("Solid Fill") | property sets: AC_Pset_Name, Pset_SlabCommon, AC_Pset_RenovationAndPhasing, BaseQuantities
          13 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "EW-3 100" | names: "Wall-111", "Wall-113", "Wall-119" (+10 more) | material: layers "EW-3" ("Solid Fill" 100.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          5 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "EW-1 240" | names: "Wall-105", "Wall-106", "Wall-107" (+2 more) | material: layers "EW-1" ("face brick" 100., "Solid Fill" 140.) | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_WallCommon, BaseQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Entrance Door 16" | names: "Door-45" | material: "Solid Fill" | property sets: AC_Pset_Name, AC_Pset_RenovationAndPhasing, Pset_DoorCommon, AC_Pset_Entrance_Door_16, BaseQuantities
        IFCSPACE "142" | long name "Roof Gross Area" | INTERNAL
        IFCSPACE "401" | long name "Technical" | INTERNAL

Types
  IFCWALLTYPE "IW-5 30" | 3 occurrences
  IFCCOLUMNTYPE "D200" | 23 occurrences
  IFCCOLUMNTYPE "D300" | 5 occurrences
  IFCCOLUMNTYPE "240X240" | 1 occurrence
  IFCCOLUMNTYPE "D350" | 2 occurrences
  IFCWALLTYPE "EW-1 240" | 20 occurrences
  IFCWINDOWSTYLE "W1 14" | SINGLE_PANEL | 83 occurrences
  IFCWALLTYPE "EW-5 100" | 3 occurrences
  IFCWINDOWSTYLE "Window 16" | SINGLE_PANEL | 15 occurrences
  IFCWINDOWSTYLE "Double Sash Window 16" | DOUBLE_PANEL_HORIZONTAL | 17 occurrences
  IFCDOORSTYLE "Entrance Door 16" | SINGLE_SWING_LEFT | 1 occurrence
  IFCWALLTYPE "IW-2 150" | 9 occurrences
  IFCDOORSTYLE "Metal Door 16" | SINGLE_SWING_RIGHT | 4 occurrences
  IFCDOORSTYLE "Double Door with Transom 16" | SINGLE_SWING_RIGHT | 2 occurrences
  IFCWALLTYPE "IW-1 100" | 36 occurrences
  IFCDOORSTYLE "Door 16" | SINGLE_SWING_RIGHT | 16 occurrences
  IFCDOORSTYLE "Door 16" | SINGLE_SWING_LEFT | 9 occurrences
  IFCWALLTYPE "IW-4 70" | 12 occurrences
  IFCDOORSTYLE "Sliding Door 16" | SLIDING_TO_LEFT | 3 occurrences
  IFCDOORSTYLE "Revolving Door 16" | REVOLVING | 1 occurrence
  IFCSANITARYTERMINALTYPE "Basin 02 13" | WASHHANDBASIN | 4 occurrences
  IFCSANITARYTERMINALTYPE "WC with Cistern 13" | WCSEAT | 3 occurrences
  IFCWALLTYPE "EW-2 100" | 2 occurrences
  IFCDOORSTYLE "Storefront 16" | SINGLE_SWING_RIGHT | 1 occurrence
  IFCWALLTYPE "EW-4 100" | 16 occurrences
  IFCWALLTYPE "EW-3 100" | 13 occurrences
  IFCDOORSTYLE "Entrance Door 16" | SINGLE_SWING_RIGHT | 1 occurrence

Property sets
  BaseQuantities | quantities | on 32 objects (32 IFCOPENINGELEMENT)
    Area = 1.9125 [SQUARE_METRE]
    Depth = 100. [MILLI METRE]
    Height = 2550. [MILLI METRE]
    Volume = 0.0275625 [CUBIC_METRE]
    Width = 750. [MILLI METRE]
  BaseQuantities | quantities | on 32 objects (32 IFCWINDOW)
    Area = 1.9125 [SQUARE_METRE]
    Depth = 100. [MILLI METRE]
    GrossArea = 1.9125 [SQUARE_METRE]
    Height = 2550. [MILLI METRE]
    Perimeter = 6600. [MILLI METRE]
    Volume = 0.0275625 [CUBIC_METRE]
    Width = 750. [MILLI METRE]
  BaseQuantities | quantities | on 13 objects (13 IFCOPENINGELEMENT)
    Area = 2.1 [SQUARE_METRE]
    Depth = 100. [MILLI METRE]
    Height = 2100. [MILLI METRE]
    Volume = 0.04662528 [CUBIC_METRE]
    Width = 1000. [MILLI METRE]
  BaseQuantities | quantities | on 13 objects (13 IFCDOOR)
    Area = 2.1 [SQUARE_METRE]
    Depth = 100. [MILLI METRE]
    Height = 2100. [MILLI METRE]
    Perimeter = 6200. [MILLI METRE]
    Volume = 0.04662528 [CUBIC_METRE]
    Width = 1000. [MILLI METRE]
  BaseQuantities | quantities | on 12 objects (12 IFCOPENINGELEMENT)
    Area = 2.1 [SQUARE_METRE]
    Depth = 150. [MILLI METRE]
    Height = 2100. [MILLI METRE]
    Volume = 0.04662528 [CUBIC_METRE]
    Width = 1000. [MILLI METRE]
  BaseQuantities | quantities | on 12 objects (12 IFCDOOR)
    Area = 2.1 [SQUARE_METRE]
    Depth = 150. [MILLI METRE]
    Height = 2100. [MILLI METRE]
    Perimeter = 6200. [MILLI METRE]
    Volume = 0.04662528 [CUBIC_METRE]
    Width = 1000. [MILLI METRE]
  BaseQuantities | quantities | on 10 objects (10 IFCOPENINGELEMENT)
    Area = 1.92 [SQUARE_METRE]
    Depth = 240. [MILLI METRE]
    Height = 1600. [MILLI METRE]
    Volume = 0.0304375 [CUBIC_METRE]
    Width = 1200. [MILLI METRE]
  BaseQuantities | quantities | on 10 objects (10 IFCWINDOW)
    Area = 1.92 [SQUARE_METRE]
    Depth = 240. [MILLI METRE]
    GrossArea = 1.92 [SQUARE_METRE]
    Height = 1600. [MILLI METRE]
    Perimeter = 5600. [MILLI METRE]
    Volume = 0.0304375 [CUBIC_METRE]
    Width = 1200. [MILLI METRE]
  BaseQuantities: 270 more contents on 401 objects not shown
  AC_Pset_Name | properties | on 12 objects (11 IFCCOVERING, 1 IFCSLAB)
    Name = "Slab-7" (IFCLABEL)
  AC_Pset_Name | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    Name = "EW-3" (IFCLABEL)
  AC_Pset_Name | properties | on 5 objects (5 IFCRAILING)
    Name = "Obj.-581" (IFCLABEL)
  AC_Pset_Name | properties | on 3 objects (3 IFCSTAIR)
    Name = "Stair-01" (IFCLABEL)
  AC_Pset_Name | properties | on 3 objects (3 IFCSPACE)
    Name = "231" (IFCLABEL)
  AC_Pset_Name | properties | on 2 objects (2 IFCSTAIR)
    Name = "Stair-02" (IFCLABEL)
  AC_Pset_Name | properties | on 1 object (1 IFCSLAB)
    Name = "Slab-01" (IFCLABEL)
  AC_Pset_Name | properties | on 1 object (1 IFCSLAB)
    Name = "Roof-03" (IFCLABEL)
  AC_Pset_Name: 353 more contents on 353 objects not shown
  AC_Pset_RenovationAndPhasing | properties | on 394 objects (115 IFCWINDOW, 114 IFCWALLSTANDARDCASE, 60 IFCSPACE, 38 IFCDOOR)
    Renovation Status = "Existing" (IFCLABEL)
  AC_Pset_Stair_Spiral_16 | properties | on 2 objects (2 IFCSTAIR)
    2D Symbol Type = "Intersect" (IFCLABEL)
    3D = "Detailed" (IFCLABEL)
    AKS Number = "" (IFCLABEL)
    Accessories (gs_list_accessories) = "" (IFCLABEL)
    Additional Information 1 = "" (IFCLABEL)
    Additional Information 2 = "" (IFCLABEL)
    Admission Date = "" (IFCLABEL)
    Angle of Stair = 270. (IFCREAL)
    Baluster Diameter = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Baluster Material = "Pine" (IFCLABEL)
    Bearing Capacity = 0. (IFCREAL)
    Bearing Structure = "" (IFCLABEL)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level Height = "" (IFCLABEL)
    Bottom Level Height Value = "" (IFCLABEL)
    Clear Width between Railing Bars = "" (IFCLABEL)
    Clear Width between Railing Bars Value = "" (IFCLABEL)
    Collection of Specifications ID = "" (IFCLABEL)
    Construction = "" (IFCLABEL)
    Contour Pen = "" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Dashed Line Type = 4 (IFCINTEGER)
    Extra Hotspots = FALSE (IFCBOOLEAN)
    Fill Background Pen = "" (IFCLABEL)
    Fill Pen = "" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Finish 1 = "" (IFCLABEL)
    Finish 1 Value = "" (IFCLABEL)
    First Tread Level = "First Tread at Floor Level" (IFCLABEL)
    Group Type = "Others" (IFCLABEL)
    Handrail Material = "Render" (IFCLABEL)
    Headroom = 0. (IFCREAL)
    Height of Levels = 0. (IFCREAL)
    ID Number = "" (IFCLABEL)
    Inventory Number = "" (IFCLABEL)
    Length of Steps = 0. (IFCREAL)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Material of Footstep = "" (IFCLABEL)
    Material of Handhold = "" (IFCLABEL)
    Material of Stair Railing = "" (IFCLABEL)
    Modification Date = "" (IFCLABEL)
    No. of Risers = 19 (IFCINTEGER)
    Nosing = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Note/Remarks = "" (IFCLABEL)
    Number of Half-Landings = 0. (IFCREAL)
    Number of Persons = "" (IFCLABEL)
    Number of Riser = 19 (IFCINTEGER)
    Number of Stories = 0. (IFCREAL)
    Number of Tread = 20 (IFCINTEGER)
    Number of Treads = "" (IFCLABEL)
    ONORM Description = "" (IFCLABEL)
    ONORM Material 1 = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Onorm Number = "" (IFCLABEL)
    Parameter Type = "No. of Risers" (IFCLABEL)
    Product = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Railing Height = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Railing Style = "Balustrade" (IFCLABEL)
    Real No. of Risers = 19 (IFCINTEGER)
    Real Tread Height = 0.15263158 (IFCLENGTHMEASURE) [MILLI METRE]
    Resolution = 3 (IFCINTEGER)
    Riser Height = 0.15263158 (IFCLENGTHMEASURE) [MILLI METRE]
    Serial Number = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Railing (iShowRailingOn) = 1 (IFCINTEGER)
    Show Railing (strShowRailingOn) = "Both" (IFCLABEL)
    Smoke-free Staircase = FALSE (IFCBOOLEAN)
    Sound Insulation (gs_list_soundinsul) = "" (IFCLABEL)
    Sound Insulation (gs_onorm_soundinsul) = "" (IFCLABEL)
    Stair Base Material = "Concrete" (IFCLABEL)
    Stair Base Type (stairBaseType) = "Concrete" (IFCLABEL)
    Stair Base Type (stairBaseType_m) = 1 (IFCINTEGER)
    Stair Slab Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Stair Type = 11 (IFCINTEGER)
    Stair-Well Diameter = 0.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Structure Cut Contour Pen (penLineStringer) = "" (IFCLABEL)
    Structure Cut Contour Pen (penLineStringer_m) = 1 (IFCINTEGER)
    Structure Cut Fill = "structural concrete" (IFCLABEL)
    Structure Cut Fill Background Pen (penBackFillStringer) = "Transparent" (IFCLABEL)
    Structure Cut Fill Background Pen (penBackFillStringer_m) = 0 (IFCINTEGER)
    Structure Cut Fill Pen (penFillStringer) = "" (IFCLABEL)
    Structure Cut Fill Pen (penFillStringer_m) = 2 (IFCINTEGER)
    To Zone Number = "" (IFCLABEL)
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level Height = "" (IFCLABEL)
    Top Level Height Value = "" (IFCLABEL)
    Top Tread Level = "Top Tread at Floor Level" (IFCLABEL)
    Total Height = 2.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Cut Contour Pen (penLineTread) = "" (IFCLABEL)
    Tread Cut Contour Pen (penLineTread_m) = 1 (IFCINTEGER)
    Tread Cut Fill = "wood" (IFCLABEL)
    Tread Cut Fill Background Pen (penBackFillTread) = "" (IFCLABEL)
    Tread Cut Fill Background Pen (penBackFillTread_m) = 114 (IFCINTEGER)
    Tread Cut Fill Pen (penFillTread) = "" (IFCLABEL)
    Tread Cut Fill Pen (penFillTread_m) = 14 (IFCINTEGER)
    Tread Depth / Tread Height = "" (IFCLABEL)
    Tread Height = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Length = 0.22321843 (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Material = "Pine, shiny" (IFCLABEL)
    Tread Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Under Slab Thickness = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
  AC_Pset_Stair_Spiral_16 | properties | on 1 object (1 IFCSTAIR)
    2D Symbol Type = "Intersect" (IFCLABEL)
    3D = "Detailed" (IFCLABEL)
    AKS Number = "" (IFCLABEL)
    Accessories (gs_list_accessories) = "" (IFCLABEL)
    Additional Information 1 = "" (IFCLABEL)
    Additional Information 2 = "" (IFCLABEL)
    Admission Date = "" (IFCLABEL)
    Angle of Stair = 270. (IFCREAL)
    Baluster Diameter = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Baluster Material = "Pine" (IFCLABEL)
    Bearing Capacity = 0. (IFCREAL)
    Bearing Structure = "" (IFCLABEL)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level Height = "" (IFCLABEL)
    Bottom Level Height Value = "" (IFCLABEL)
    Clear Width between Railing Bars = "" (IFCLABEL)
    Clear Width between Railing Bars Value = "" (IFCLABEL)
    Collection of Specifications ID = "" (IFCLABEL)
    Construction = "" (IFCLABEL)
    Contour Pen = "" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Dashed Line Type = 4 (IFCINTEGER)
    Extra Hotspots = FALSE (IFCBOOLEAN)
    Fill Background Pen = "" (IFCLABEL)
    Fill Pen = "" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Finish 1 = "" (IFCLABEL)
    Finish 1 Value = "" (IFCLABEL)
    First Tread Level = "First Tread at Floor Level" (IFCLABEL)
    Group Type = "Others" (IFCLABEL)
    Handrail Material = "Render" (IFCLABEL)
    Headroom = 0. (IFCREAL)
    Height of Levels = 0. (IFCREAL)
    ID Number = "" (IFCLABEL)
    Inventory Number = "" (IFCLABEL)
    Length of Steps = 0. (IFCREAL)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Material of Footstep = "" (IFCLABEL)
    Material of Handhold = "" (IFCLABEL)
    Material of Stair Railing = "" (IFCLABEL)
    Modification Date = "" (IFCLABEL)
    No. of Risers = 19 (IFCINTEGER)
    Nosing = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Note/Remarks = "" (IFCLABEL)
    Number of Half-Landings = 0. (IFCREAL)
    Number of Persons = "" (IFCLABEL)
    Number of Riser = 19 (IFCINTEGER)
    Number of Stories = 0. (IFCREAL)
    Number of Tread = 20 (IFCINTEGER)
    Number of Treads = "" (IFCLABEL)
    ONORM Description = "" (IFCLABEL)
    ONORM Material 1 = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Onorm Number = "" (IFCLABEL)
    Parameter Type = "No. of Risers" (IFCLABEL)
    Product = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Railing Height = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Railing Style = "Balustrade" (IFCLABEL)
    Real No. of Risers = 19 (IFCINTEGER)
    Real Tread Height = 0.18421053 (IFCLENGTHMEASURE) [MILLI METRE]
    Resolution = 3 (IFCINTEGER)
    Riser Height = 0.18421053 (IFCLENGTHMEASURE) [MILLI METRE]
    Serial Number = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Railing (iShowRailingOn) = 1 (IFCINTEGER)
    Show Railing (strShowRailingOn) = "Both" (IFCLABEL)
    Smoke-free Staircase = FALSE (IFCBOOLEAN)
    Sound Insulation (gs_list_soundinsul) = "" (IFCLABEL)
    Sound Insulation (gs_onorm_soundinsul) = "" (IFCLABEL)
    Stair Base Material = "Concrete" (IFCLABEL)
    Stair Base Type (stairBaseType) = "Concrete" (IFCLABEL)
    Stair Base Type (stairBaseType_m) = 1 (IFCINTEGER)
    Stair Slab Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Stair Type = 11 (IFCINTEGER)
    Stair-Well Diameter = 0.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Structure Cut Contour Pen (penLineStringer) = "" (IFCLABEL)
    Structure Cut Contour Pen (penLineStringer_m) = 1 (IFCINTEGER)
    Structure Cut Fill = "structural concrete" (IFCLABEL)
    Structure Cut Fill Background Pen (penBackFillStringer) = "Transparent" (IFCLABEL)
    Structure Cut Fill Background Pen (penBackFillStringer_m) = 0 (IFCINTEGER)
    Structure Cut Fill Pen (penFillStringer) = "" (IFCLABEL)
    Structure Cut Fill Pen (penFillStringer_m) = 2 (IFCINTEGER)
    To Zone Number = "" (IFCLABEL)
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level Height = "" (IFCLABEL)
    Top Level Height Value = "" (IFCLABEL)
    Top Tread Level = "Top Tread at Floor Level" (IFCLABEL)
    Total Height = 3.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Cut Contour Pen (penLineTread) = "" (IFCLABEL)
    Tread Cut Contour Pen (penLineTread_m) = 1 (IFCINTEGER)
    Tread Cut Fill = "wood" (IFCLABEL)
    Tread Cut Fill Background Pen (penBackFillTread) = "" (IFCLABEL)
    Tread Cut Fill Background Pen (penBackFillTread_m) = 114 (IFCINTEGER)
    Tread Cut Fill Pen (penFillTread) = "" (IFCLABEL)
    Tread Cut Fill Pen (penFillTread_m) = 14 (IFCINTEGER)
    Tread Depth / Tread Height = "" (IFCLABEL)
    Tread Height = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Length = 0.22321843 (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Material = "Pine, shiny" (IFCLABEL)
    Tread Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Under Slab Thickness = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    Reference = "U-shape Stair" (IFCIDENTIFIER)
  AC_Pset_Stair_U-Shape_16 | properties | on 1 object (1 IFCSTAIR)
    2*Tread Height+Tread Depth = 0.62222222 (IFCLENGTHMEASURE) [MILLI METRE]
    2D Detail Level (gs_detlevel_2D) = "Scale Sensitive" (IFCLABEL)
    2D Detail Level (gs_detlevel_2D_m) = 1 (IFCINTEGER)
    2D Symbol Type (gs_SymbolType) = "Type 11" (IFCLABEL)
    2D Symbol Type (gs_SymbolType_m) = 11 (IFCINTEGER)
    3D = "Detailed" (IFCLABEL)
    3D Representation (gs_detlevel_3D_m) = 2 (IFCINTEGER)
    Arrowhead Fill Type = "100 %1" (IFCLABEL)
    Arrowhead Style (arrow_style) = "Style 3" (IFCLABEL)
    Background Fill Type = "Solid Fill" (IFCLABEL)
    Bar Depth (leftRailBarDepth) = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Bar Depth (rightRailBarDepth) = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Bar Material = "Render" (IFCLABEL)
    Bar Thickness (leftRailBarThk) = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bar Thickness (rightRailBarThk) = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Breakline = TRUE (IFCBOOLEAN)
    Breakline Position (Height) = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Breakline Style (breakline_style) = "Straight" (IFCLABEL)
    Breakline Width = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Custom Text_1 = "Custom Text_1" (IFCLABEL)
    Custom Text_2 = "Custom Text_2" (IFCLABEL)
    Description = "" (IFCLABEL)
    Dimension Definition = 1 (IFCINTEGER)
    Distance From Stair = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Distance from Slab/Stair = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Down Text = "DOWN" (IFCLABEL)
    Enable Simple ZigZag Breakline = FALSE (IFCBOOLEAN)
    Fill Above Breakline = FALSE (IFCBOOLEAN)
    Fill Background Pen = "" (IFCLABEL)
    Fill Pen (0-No Fill) (gs_ArrowFillPen) = "" (IFCLABEL)
    Fill Pen (0-No Fill) (gs_StartEndFillPen) = "Transparent" (IFCLABEL)
    Fill Pen = "" (IFCLABEL)
    Fill Pen Above (0-No Fill) = "Transparent" (IFCLABEL)
    Flight Width = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Flights Offset = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Font Pen = "" (IFCLABEL)
    Font Size (mm) (fontsize) = 1. (IFCREAL)
    Font Size (mm) (gs_NumTextSize) = 1. (IFCREAL)
    Font Size (mm) (gs_desc_text_size) = 1. (IFCREAL)
    Font Size (point) (gs_desc_text_size_pt) = 2.8346457 (IFCREAL)
    Font Size (point) (gs_text_size_pt) = 2.8346457 (IFCREAL)
    Font Size (point) (gs_text_size_pt_num) = 2.8346457 (IFCREAL)
    Font Type = "Arial" (IFCLABEL)
    Frame Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame/Bar Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Half Height of Symbol = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Half Width of Arrowhead = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Half Width of Symbol = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Material = "Render" (IFCLABEL)
    Height of Arrowhead = 0.25 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Rail (leftRailHeight) = 0.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Rail (rightRailHeight) = 0.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Invisible Line Type = 6 (IFCINTEGER)
    Invisible Structures Lines Pen = "" (IFCLABEL)
    Invisible Structures Lines Type = 4 (IFCINTEGER)
    Left Rail (leftRailType) = "Same as Right" (IFCLABEL)
    Line Pen (gs_LinePenStUp) = "" (IFCLABEL)
    Line Pen (gs_wLinePen) = "" (IFCLABEL)
    Line Type (gs_LineTypeStUp) = 1 (IFCINTEGER)
    Line Type (gs_wLineType2) = 6 (IFCINTEGER)
    Line Type Above Break (lineTypeAboveBreak) = "Intersect" (IFCLABEL)
    Lower Landing Thickness = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Part = FALSE (IFCBOOLEAN)
    Middle/Detailed Scale Change at = 50 (IFCINTEGER)
    No. of Bars (nBarsLeftRail) = 4 (IFCINTEGER)
    No. of Bars (nBarsRightRail) = 4 (IFCINTEGER)
    No. of Risers = 18 (IFCINTEGER)
    No. of Risers in the 1st Run = 9 (IFCINTEGER)
    No. of Risers in the 2nd Run = 9 (IFCINTEGER)
    Nosing = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Numbering Position X = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Numbering Position Y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Parameter Type = "Tread Height" (IFCLABEL)
    Post Material = "Render" (IFCLABEL)
    Post Size (leftRailPostSize) = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Post Size (rightRailPostSize) = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Preferred Tread Height = 0.19444444 (IFCLENGTHMEASURE) [MILLI METRE]
    Radius of Circle = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Rail (rail) = "Both" (IFCLABEL)
    Rail (rail_m) = 1 (IFCINTEGER)
    Rail Axis Line Pen = "" (IFCLABEL)
    Rail Axis Line Type = 6 (IFCINTEGER)
    Rail Bottom Overhang (leftRailOvhgBottom) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Bottom Overhang (rightRailOvhgBottom) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Elements Dimensions (sgl) = "" (IFCLABEL)
    Rail Elements Dimensions (sgr) = "" (IFCLABEL)
    Rail Left Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Line Type = 1 (IFCINTEGER)
    Rail Pen = "" (IFCLABEL)
    Rail Right Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Top Overhang (leftRailOvhgTop) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Top Overhang (rightRailOvhgTop) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Real Tread Height = 0.19444444 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Rail (rightRailType) = "Rail Balustrade" (IFCLABEL)
    Rise Text = "R" (IFCLABEL)
    Rise and Run Text (bShowRiseAndRunText) = FALSE (IFCBOOLEAN)
    Rise and Run Text (gs_txStUp) = FALSE (IFCBOOLEAN)
    Rise and Run Text Position X = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rise and Run Text Position Y = 0.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Rise and Run Text Rotation Angle = 0. (IFCREAL)
    Riser Cover = TRUE (IFCBOOLEAN)
    Riser Cover Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Riser Cut Contour Pen (penLineRiser) = "" (IFCLABEL)
    Riser Cut Contour Pen (penLineRiser_m) = 1 (IFCINTEGER)
    Riser Cut Fill = "Solid Fill" (IFCLABEL)
    Riser Cut Fill Background Pen (penBackFillRiser) = "Transparent" (IFCLABEL)
    Riser Cut Fill Background Pen (penBackFillRiser_m) = 0 (IFCINTEGER)
    Riser Cut Fill Pen (penFillRiser) = "" (IFCLABEL)
    Riser Cut Fill Pen (penFillRiser_m) = 2 (IFCINTEGER)
    Riser Material = "Pine" (IFCLABEL)
    Same as Right Rail = TRUE (IFCBOOLEAN)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Show Numbering (bShowNumbering) = TRUE (IFCBOOLEAN)
    Show Numbering (gs_numaStUp) = TRUE (IFCBOOLEAN)
    Show Rail Axis = FALSE (IFCBOOLEAN)
    Show Rail on Floor Plan = FALSE (IFCBOOLEAN)
    Show Treads = TRUE (IFCBOOLEAN)
    Show Walking Line = TRUE (IFCBOOLEAN)
    Show Walking Line Above Breakline = TRUE (IFCBOOLEAN)
    Simple/Middle Scale Change at = 100 (IFCINTEGER)
    Stair Base Material = "Concrete" (IFCLABEL)
    Stair Base Type (stairBaseType) = "Concrete" (IFCLABEL)
    Stair Base Type (stairBaseType_m) = 1 (IFCINTEGER)
    Stair Slab Thickness = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Start Num. From <Num.> = 1 (IFCINTEGER)
    Story Sensitive = FALSE (IFCBOOLEAN)
    Structural Dimensions (ggl) = "" (IFCLABEL)
    Structural Dimensions (ggr) = "" (IFCLABEL)
    Structure Cut Contour Pen (penLineStringer) = "" (IFCLABEL)
    Structure Cut Contour Pen (penLineStringer_m) = 1 (IFCINTEGER)
    Structure Cut Fill = "structural concrete" (IFCLABEL)
    Structure Cut Fill Background Pen (penBackFillStringer) = "Transparent" (IFCLABEL)
    Structure Cut Fill Background Pen (penBackFillStringer_m) = 0 (IFCINTEGER)
    Structure Cut Fill Pen (penFillStringer) = "" (IFCLABEL)
    Structure Cut Fill Pen (penFillStringer_m) = 2 (IFCINTEGER)
    Surface Material = "Pine" (IFCLABEL)
    Symbol Fill Type = "100 %1" (IFCLABEL)
    Symbol at Start End (gs_StartEndStyle) = "Style 1" (IFCLABEL)
    Symbol at Start End (gs_StartEndStyle_m) = 1 (IFCINTEGER)
    Text (gs_RiseRunText) = "Number x Rise = Run Height" (IFCLABEL)
    Text (iRiseRunText) = 1 (IFCINTEGER)
    Text Horiz. Displacement (DirUPDN_X) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Text Horiz. Displacement (DirUPDN_X_top) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Text Orientation on Symbol (typeTextRotation_Num) = "Align with Symbol" (IFCLABEL)
    Text Orientation on Symbol (typeTextRotation_Num_m) = 0 (IFCINTEGER)
    Text Orientation on Symbol (typeTextRotation_RiseRun) = "Readable" (IFCLABEL)
    Text Orientation on Symbol (typeTextRotation_RiseRun_m) = 2 (IFCINTEGER)
    Text Orientation on Symbol (typeTextRotation_UpDn) = "Align with Symbol" (IFCLABEL)
    Text Orientation on Symbol (typeTextRotation_UpDn_m) = 0 (IFCINTEGER)
    Text Pen (gs_NumTextPen) = "" (IFCLABEL)
    Text Pen (gs_desc_text_pen) = "" (IFCLABEL)
    Text Vert. Displacement (DirUPDN_Y) = -0.25 (IFCLENGTHMEASURE) [MILLI METRE]
    Text Vert. Displacement (DirUPDN_Y_top) = -0.25 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Total Depth = 4.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Total Height = 3.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Total Width = 3.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Cut Contour Pen (penLineTread) = "" (IFCLABEL)
    Tread Cut Contour Pen (penLineTread_m) = 1 (IFCINTEGER)
    Tread Cut Fill = "wood" (IFCLABEL)
    Tread Cut Fill Background Pen (penBackFillTread) = "" (IFCLABEL)
    Tread Cut Fill Background Pen (penBackFillTread_m) = 114 (IFCINTEGER)
    Tread Cut Fill Pen (penFillTread) = "" (IFCLABEL)
    Tread Cut Fill Pen (penFillTread_m) = 14 (IFCINTEGER)
    Tread Depth = 0.23333333 (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Material = "Pine" (IFCLABEL)
    Tread Thickness (0-None) = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    UP/DOWN Font Size (mm) = 2. (IFCREAL)
    UP/DOWN Font Size (point) = 5.6692913 (IFCREAL)
    UP/DOWN Text (walkingDirUPDN) = "None" (IFCLABEL)
    UP/DOWN Text (walkingDirUPDN_m) = 1 (IFCINTEGER)
    UP/DOWN Text Angle (AngUPDN) = 0. (IFCREAL)
    UP/DOWN Text Angle (AngUPDN_top) = 0. (IFCREAL)
    UP/DOWN Text Pen = "" (IFCLABEL)
    Upper Junction Type = "" (IFCLABEL)
    Upper Landing Thickness = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Part = TRUE (IFCBOOLEAN)
    Use Units from Project Preferences = TRUE (IFCBOOLEAN)
    Visible Line Type = 1 (IFCINTEGER)
    Visible Structures Lines Pen = "" (IFCLABEL)
    Visible Structures Lines Type = 1 (IFCINTEGER)
    Walking Line Type = 1 (IFCINTEGER)
    Wire Depth (leftRailWireDepth) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Wire Depth (rightRailWireDepth) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Wire Diameter (leftRailWireDiam) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Wire Diameter (rightRailWireDiam) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Wire Thickness (leftRailWireThk) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Wire Thickness (rightRailWireThk) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Wire Type (leftWireType) = "Rectangular" (IFCLABEL)
    Wire Type (rightWireType) = "Rectangular" (IFCLABEL)
    Wood Base Offset = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    will be developed later (bShowCarriage) = FALSE (IFCBOOLEAN)
    will be developed later (carriageLineType) = 4 (IFCINTEGER)
    will be developed later (carriagePen) = "" (IFCLABEL)
    will be developed later (iPostSymbolType) = 1 (IFCINTEGER)
    will be developed later (postLineType) = 1 (IFCINTEGER)
    will be developed later (postPen) = "" (IFCLABEL)
    will be developed later (postSymbolType) = "Type 1" (IFCLABEL)
  AC_Pset_Stair_U-Shape_16 | properties | on 1 object (1 IFCSTAIR)
    2*Tread Height+Tread Depth = 0.55 (IFCLENGTHMEASURE) [MILLI METRE]
    2D Detail Level (gs_detlevel_2D) = "Scale Sensitive" (IFCLABEL)
    2D Detail Level (gs_detlevel_2D_m) = 1 (IFCINTEGER)
    2D Symbol Type (gs_SymbolType) = "Type 11" (IFCLABEL)
    2D Symbol Type (gs_SymbolType_m) = 11 (IFCINTEGER)
    3D = "Detailed" (IFCLABEL)
    3D Representation (gs_detlevel_3D_m) = 2 (IFCINTEGER)
    Arrowhead Fill Type = "100 %1" (IFCLABEL)
    Arrowhead Style (arrow_style) = "Style 3" (IFCLABEL)
    Background Fill Type = "Solid Fill" (IFCLABEL)
    Bar Depth (leftRailBarDepth) = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Bar Depth (rightRailBarDepth) = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Bar Material = "Render" (IFCLABEL)
    Bar Thickness (leftRailBarThk) = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bar Thickness (rightRailBarThk) = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Breakline = TRUE (IFCBOOLEAN)
    Breakline Position (Height) = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Breakline Style (breakline_style) = "Straight" (IFCLABEL)
    Breakline Width = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Custom Text_1 = "Custom Text_1" (IFCLABEL)
    Custom Text_2 = "Custom Text_2" (IFCLABEL)
    Description = "" (IFCLABEL)
    Dimension Definition = 1 (IFCINTEGER)
    Distance From Stair = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Distance from Slab/Stair = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Down Text = "DOWN" (IFCLABEL)
    Enable Simple ZigZag Breakline = FALSE (IFCBOOLEAN)
    Fill Above Breakline = FALSE (IFCBOOLEAN)
    Fill Background Pen = "" (IFCLABEL)
    Fill Pen (0-No Fill) (gs_ArrowFillPen) = "" (IFCLABEL)
    Fill Pen (0-No Fill) (gs_StartEndFillPen) = "Transparent" (IFCLABEL)
    Fill Pen = "" (IFCLABEL)
    Fill Pen Above (0-No Fill) = "Transparent" (IFCLABEL)
    Flight Width = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Flights Offset = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Font Pen = "" (IFCLABEL)
    Font Size (mm) (fontsize) = 1. (IFCREAL)
    Font Size (mm) (gs_NumTextSize) = 1. (IFCREAL)
    Font Size (mm) (gs_desc_text_size) = 1. (IFCREAL)
    Font Size (point) (gs_desc_text_size_pt) = 2.8346457 (IFCREAL)
    Font Size (point) (gs_text_size_pt) = 2.8346457 (IFCREAL)
    Font Size (point) (gs_text_size_pt_num) = 2.8346457 (IFCREAL)
    Font Type = "Arial" (IFCLABEL)
    Frame Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame/Bar Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Half Height of Symbol = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Half Width of Arrowhead = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Half Width of Symbol = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Material = "Render" (IFCLABEL)
    Height of Arrowhead = 0.25 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Rail (leftRailHeight) = 0.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Rail (rightRailHeight) = 0.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Invisible Line Type = 6 (IFCINTEGER)
    Invisible Structures Lines Pen = "" (IFCLABEL)
    Invisible Structures Lines Type = 4 (IFCINTEGER)
    Left Rail (leftRailType) = "Same as Right" (IFCLABEL)
    Line Pen (gs_LinePenStUp) = "" (IFCLABEL)
    Line Pen (gs_wLinePen) = "" (IFCLABEL)
    Line Type (gs_LineTypeStUp) = 1 (IFCINTEGER)
    Line Type (gs_wLineType2) = 6 (IFCINTEGER)
    Line Type Above Break (lineTypeAboveBreak) = "Intersect" (IFCLABEL)
    Lower Landing Thickness = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Part = FALSE (IFCBOOLEAN)
    Middle/Detailed Scale Change at = 50 (IFCINTEGER)
    No. of Bars (nBarsLeftRail) = 4 (IFCINTEGER)
    No. of Bars (nBarsRightRail) = 4 (IFCINTEGER)
    No. of Risers = 18 (IFCINTEGER)
    No. of Risers in the 1st Run = 9 (IFCINTEGER)
    No. of Risers in the 2nd Run = 9 (IFCINTEGER)
    Nosing = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Numbering Position X = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Numbering Position Y = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Parameter Type = "Tread Height" (IFCLABEL)
    Post Material = "Render" (IFCLABEL)
    Post Size (leftRailPostSize) = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Post Size (rightRailPostSize) = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Preferred Tread Height = 0.15833333 (IFCLENGTHMEASURE) [MILLI METRE]
    Radius of Circle = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Rail (rail) = "Both" (IFCLABEL)
    Rail (rail_m) = 1 (IFCINTEGER)
    Rail Axis Line Pen = "" (IFCLABEL)
    Rail Axis Line Type = 6 (IFCINTEGER)
    Rail Bottom Overhang (leftRailOvhgBottom) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Bottom Overhang (rightRailOvhgBottom) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Elements Dimensions (sgl) = "" (IFCLABEL)
    Rail Elements Dimensions (sgr) = "" (IFCLABEL)
    Rail Left Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Line Type = 1 (IFCINTEGER)
    Rail Pen = "" (IFCLABEL)
    Rail Right Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Top Overhang (leftRailOvhgTop) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail Top Overhang (rightRailOvhgTop) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Real Tread Height = 0.15833333 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Rail (rightRailType) = "Rail Balustrade" (IFCLABEL)
    Rise Text = "R" (IFCLABEL)
    Rise and Run Text (bShowRiseAndRunText) = FALSE (IFCBOOLEAN)
    Rise and Run Text (gs_txStUp) = FALSE (IFCBOOLEAN)
    Rise and Run Text Position X = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rise and Run Text Position Y = 0.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Rise and Run Text Rotation Angle = 0. (IFCREAL)
    Riser Cover = TRUE (IFCBOOLEAN)
    Riser Cover Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Riser Cut Contour Pen (penLineRiser) = "" (IFCLABEL)
    Riser Cut Contour Pen (penLineRiser_m) = 1 (IFCINTEGER)
    Riser Cut Fill = "Solid Fill" (IFCLABEL)
    Riser Cut Fill Background Pen (penBackFillRiser) = "Transparent" (IFCLABEL)
    Riser Cut Fill Background Pen (penBackFillRiser_m) = 0 (IFCINTEGER)
    Riser Cut Fill Pen (penFillRiser) = "" (IFCLABEL)
    Riser Cut Fill Pen (penFillRiser_m) = 2 (IFCINTEGER)
    Riser Material = "Pine" (IFCLABEL)
    Same as Right Rail = TRUE (IFCBOOLEAN)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Show Numbering (bShowNumbering) = TRUE (IFCBOOLEAN)
    Show Numbering (gs_numaStUp) = TRUE (IFCBOOLEAN)
    Show Rail Axis = FALSE (IFCBOOLEAN)
    Show Rail on Floor Plan = FALSE (IFCBOOLEAN)
    Show Treads = TRUE (IFCBOOLEAN)
    Show Walking Line = TRUE (IFCBOOLEAN)
    Show Walking Line Above Breakline = TRUE (IFCBOOLEAN)
    Simple/Middle Scale Change at = 100 (IFCINTEGER)
    Stair Base Material = "Concrete" (IFCLABEL)
    Stair Base Type (stairBaseType) = "Concrete" (IFCLABEL)
    Stair Base Type (stairBaseType_m) = 1 (IFCINTEGER)
    Stair Slab Thickness = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Start Num. From <Num.> = 1 (IFCINTEGER)
    Story Sensitive = FALSE (IFCBOOLEAN)
    Structural Dimensions (ggl) = "" (IFCLABEL)
    Structural Dimensions (ggr) = "" (IFCLABEL)
    Structure Cut Contour Pen (penLineStringer) = "" (IFCLABEL)
    Structure Cut Contour Pen (penLineStringer_m) = 1 (IFCINTEGER)
    Structure Cut Fill = "structural concrete" (IFCLABEL)
    Structure Cut Fill Background Pen (penBackFillStringer) = "Transparent" (IFCLABEL)
    Structure Cut Fill Background Pen (penBackFillStringer_m) = 0 (IFCINTEGER)
    Structure Cut Fill Pen (penFillStringer) = "" (IFCLABEL)
    Structure Cut Fill Pen (penFillStringer_m) = 2 (IFCINTEGER)
    Surface Material = "Pine" (IFCLABEL)
    Symbol Fill Type = "100 %1" (IFCLABEL)
    Symbol at Start End (gs_StartEndStyle) = "Style 1" (IFCLABEL)
    Symbol at Start End (gs_StartEndStyle_m) = 1 (IFCINTEGER)
    Text (gs_RiseRunText) = "Number x Rise = Run Height" (IFCLABEL)
    Text (iRiseRunText) = 1 (IFCINTEGER)
    Text Horiz. Displacement (DirUPDN_X) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Text Horiz. Displacement (DirUPDN_X_top) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Text Orientation on Symbol (typeTextRotation_Num) = "Align with Symbol" (IFCLABEL)
    Text Orientation on Symbol (typeTextRotation_Num_m) = 0 (IFCINTEGER)
    Text Orientation on Symbol (typeTextRotation_RiseRun) = "Readable" (IFCLABEL)
    Text Orientation on Symbol (typeTextRotation_RiseRun_m) = 2 (IFCINTEGER)
    Text Orientation on Symbol (typeTextRotation_UpDn) = "Align with Symbol" (IFCLABEL)
    Text Orientation on Symbol (typeTextRotation_UpDn_m) = 0 (IFCINTEGER)
    Text Pen (gs_NumTextPen) = "" (IFCLABEL)
    Text Pen (gs_desc_text_pen) = "" (IFCLABEL)
    Text Vert. Displacement (DirUPDN_Y) = -0.25 (IFCLENGTHMEASURE) [MILLI METRE]
    Text Vert. Displacement (DirUPDN_Y_top) = -0.25 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Total Depth = 4.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Total Height = 2.85 (IFCLENGTHMEASURE) [MILLI METRE]
    Total Width = 3.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Cut Contour Pen (penLineTread) = "" (IFCLABEL)
    Tread Cut Contour Pen (penLineTread_m) = 1 (IFCINTEGER)
    Tread Cut Fill = "wood" (IFCLABEL)
    Tread Cut Fill Background Pen (penBackFillTread) = "" (IFCLABEL)
    Tread Cut Fill Background Pen (penBackFillTread_m) = 114 (IFCINTEGER)
    Tread Cut Fill Pen (penFillTread) = "" (IFCLABEL)
    Tread Cut Fill Pen (penFillTread_m) = 14 (IFCINTEGER)
    Tread Depth = 0.23333333 (IFCLENGTHMEASURE) [MILLI METRE]
    Tread Material = "Pine" (IFCLABEL)
    Tread Thickness (0-None) = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    UP/DOWN Font Size (mm) = 2. (IFCREAL)
    UP/DOWN Font Size (point) = 5.6692913 (IFCREAL)
    UP/DOWN Text (walkingDirUPDN) = "None" (IFCLABEL)
    UP/DOWN Text (walkingDirUPDN_m) = 1 (IFCINTEGER)
    UP/DOWN Text Angle (AngUPDN) = 0. (IFCREAL)
    UP/DOWN Text Angle (AngUPDN_top) = 0. (IFCREAL)
    UP/DOWN Text Pen = "" (IFCLABEL)
    Upper Junction Type = "" (IFCLABEL)
    Upper Landing Thickness = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Part = TRUE (IFCBOOLEAN)
    Use Units from Project Preferences = TRUE (IFCBOOLEAN)
    Visible Line Type = 1 (IFCINTEGER)
    Visible Structures Lines Pen = "" (IFCLABEL)
    Visible Structures Lines Type = 1 (IFCINTEGER)
    Walking Line Type = 1 (IFCINTEGER)
    Wire Depth (leftRailWireDepth) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Wire Depth (rightRailWireDepth) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Wire Diameter (leftRailWireDiam) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Wire Diameter (rightRailWireDiam) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Wire Thickness (leftRailWireThk) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Wire Thickness (rightRailWireThk) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Wire Type (leftWireType) = "Rectangular" (IFCLABEL)
    Wire Type (rightWireType) = "Rectangular" (IFCLABEL)
    Wood Base Offset = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    will be developed later (bShowCarriage) = FALSE (IFCBOOLEAN)
    will be developed later (carriageLineType) = 4 (IFCINTEGER)
    will be developed later (carriagePen) = "" (IFCLABEL)
    will be developed later (iPostSymbolType) = 1 (IFCINTEGER)
    will be developed later (postLineType) = 1 (IFCINTEGER)
    will be developed later (postPen) = "" (IFCLABEL)
    will be developed later (postSymbolType) = "Type 1" (IFCLABEL)
  Pset_CoveringCommon | properties | on 11 objects (11 IFCCOVERING)
    Reference = "FS-3" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    Reference = "RS-2" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    Reference = "RS-1" (IFCIDENTIFIER)
  AC_Pset_Basic_Zone_Stamp | properties | on 1 object (1 IFCSPACE)
    Back Surface of Wall Insets = 0. (IFCREAL)
    Beam Surface at the Bottom = 0. (IFCREAL)
    Beam Surface at the Top = 0. (IFCREAL)
    Bottom Surface = 13.2 (IFCREAL)
    Boundary Surface = 76.22 (IFCREAL)
    Calculated Area = 13.2 (IFCREAL)
    Combined Width of Doors = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Combined Width of Windows = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Extracted Area Total = 0. (IFCREAL)
    Extracted Column Area = 0. (IFCREAL)
    Extracted Fill Area = 0. (IFCREAL)
    Extracted Low Areas = 0. (IFCREAL)
    Extracted Wall Area = 0. (IFCREAL)
    Fill Background Pen = "Transparent" (IFCLABEL)
    Fill Pen = "Transparent" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Floor Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 3.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Length of Perimeter Walls = 13.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Letter Size [mm] = 1. (IFCREAL)
    Measured Area [m2] = 13.2 (IFCREAL)
    Measured Net Area = 13.2 (IFCREAL)
    Net Perimeter = 20.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Number of All Corners = 8 (IFCINTEGER)
    Number of Concave Corners = 2 (IFCINTEGER)
    Perimeter = 20.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter of Holes = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Reduced Area = 13.2 (IFCREAL)
    Roof Surface at the Bottom = 0. (IFCREAL)
    Roof Surface at the Top = 0. (IFCREAL)
    Side Surface of Wall Insets = 0. (IFCREAL)
    Slab Surface at the Bottom = 0. (IFCREAL)
    Slab Surface at the Top = 0. (IFCREAL)
    Subfloor Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Surface Area of Doors = 0. (IFCREAL)
    Surface Area of Perimeter Walls = 50.885 (IFCREAL)
    Surface Area of Windows = 0. (IFCREAL)
    Text Font 1 = "Arial" (IFCLABEL)
    Top Surface = 13.2 (IFCREAL)
    Top Surface of Wall Insets = 0. (IFCREAL)
    Volume = 48.84 (IFCREAL)
    Zone Area Factor = 1. (IFCREAL)
    Zone Name = "Stair" (IFCLABEL)
    Zone Number = "111" (IFCLABEL)
    Zone Polygon (Gross, Net) = 0 (IFCINTEGER)
  AC_Pset_Basic_Zone_Stamp | properties | on 1 object (1 IFCSPACE)
    Back Surface of Wall Insets = 0. (IFCREAL)
    Beam Surface at the Bottom = 0. (IFCREAL)
    Beam Surface at the Top = 0. (IFCREAL)
    Bottom Surface = 16.685 (IFCREAL)
    Boundary Surface = 57.75 (IFCREAL)
    Calculated Area = 16.685 (IFCREAL)
    Combined Width of Doors = 2. (IFCLENGTHMEASURE) [MILLI METRE]
    Combined Width of Windows = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Extracted Area Total = 0. (IFCREAL)
    Extracted Column Area = 0. (IFCREAL)
    Extracted Fill Area = 0. (IFCREAL)
    Extracted Low Areas = 0. (IFCREAL)
    Extracted Wall Area = 0. (IFCREAL)
    Fill Background Pen = "Transparent" (IFCLABEL)
    Fill Pen = "Transparent" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Floor Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 3.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Length of Perimeter Walls = 16.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Letter Size [mm] = 1. (IFCREAL)
    Measured Area [m2] = 16.685 (IFCREAL)
    Measured Net Area = 16.685 (IFCREAL)
    Net Perimeter = 16.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Number of All Corners = 4 (IFCINTEGER)
    Number of Concave Corners = 0 (IFCINTEGER)
    Perimeter = 16.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter of Holes = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Reduced Area = 16.685 (IFCREAL)
    Roof Surface at the Bottom = 0. (IFCREAL)
    Roof Surface at the Top = 0. (IFCREAL)
    Side Surface of Wall Insets = 0. (IFCREAL)
    Slab Surface at the Bottom = 0. (IFCREAL)
    Slab Surface at the Top = 0. (IFCREAL)
    Subfloor Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Surface Area of Doors = 4.2 (IFCREAL)
    Surface Area of Perimeter Walls = 49.0075 (IFCREAL)
    Surface Area of Windows = 5.4825 (IFCREAL)
    Text Font 1 = "Arial" (IFCLABEL)
    Top Surface = 16.685 (IFCREAL)
    Top Surface of Wall Insets = 0. (IFCREAL)
    Volume = 58.3975 (IFCREAL)
    Zone Area Factor = 1. (IFCREAL)
    Zone Name = "Petty Education Inc." (IFCLABEL)
    Zone Number = "125" (IFCLABEL)
    Zone Polygon (Gross, Net) = 0 (IFCINTEGER)
  AC_Pset_Basic_Zone_Stamp | properties | on 1 object (1 IFCSPACE)
    Back Surface of Wall Insets = 0. (IFCREAL)
    Beam Surface at the Bottom = 0. (IFCREAL)
    Beam Surface at the Top = 0. (IFCREAL)
    Bottom Surface = 6.6375 (IFCREAL)
    Boundary Surface = 41.825 (IFCREAL)
    Calculated Area = 6.6375 (IFCREAL)
    Combined Width of Doors = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Combined Width of Windows = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Extracted Area Total = 0. (IFCREAL)
    Extracted Column Area = 0. (IFCREAL)
    Extracted Fill Area = 0. (IFCREAL)
    Extracted Low Areas = 0. (IFCREAL)
    Extracted Wall Area = 0. (IFCREAL)
    Fill Background Pen = "Transparent" (IFCLABEL)
    Fill Pen = "Transparent" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Floor Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 3.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Length of Perimeter Walls = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Letter Size [mm] = 1. (IFCREAL)
    Measured Area [m2] = 6.6375 (IFCREAL)
    Measured Net Area = 6.6375 (IFCREAL)
    Net Perimeter = 11.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Number of All Corners = 4 (IFCINTEGER)
    Number of Concave Corners = 0 (IFCINTEGER)
    Perimeter = 11.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter of Holes = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Reduced Area = 6.6375 (IFCREAL)
    Roof Surface at the Bottom = 0. (IFCREAL)
    Roof Surface at the Top = 0. (IFCREAL)
    Side Surface of Wall Insets = 0. (IFCREAL)
    Slab Surface at the Bottom = 0. (IFCREAL)
    Slab Surface at the Top = 0. (IFCREAL)
    Subfloor Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Surface Area of Doors = 2.1 (IFCREAL)
    Surface Area of Perimeter Walls = 3.45 (IFCREAL)
    Surface Area of Windows = 0. (IFCREAL)
    Text Font 1 = "Arial" (IFCLABEL)
    Top Surface = 6.6375 (IFCREAL)
    Top Surface of Wall Insets = 0. (IFCREAL)
    Volume = 23.23125 (IFCREAL)
    Zone Area Factor = 1. (IFCREAL)
    Zone Name = "Corridor" (IFCLABEL)
    Zone Number = "140" (IFCLABEL)
    Zone Polygon (Gross, Net) = 0 (IFCINTEGER)
  AC_Pset_Basic_Zone_Stamp | properties | on 1 object (1 IFCSPACE)
    Back Surface of Wall Insets = 0. (IFCREAL)
    Beam Surface at the Bottom = 0. (IFCREAL)
    Beam Surface at the Top = 0. (IFCREAL)
    Bottom Surface = 10.69375 (IFCREAL)
    Boundary Surface = 50.0815 (IFCREAL)
    Calculated Area = 10.69375 (IFCREAL)
    Combined Width of Doors = 7.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Combined Width of Windows = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Extracted Area Total = 0. (IFCREAL)
    Extracted Column Area = 0. (IFCREAL)
    Extracted Fill Area = 0. (IFCREAL)
    Extracted Low Areas = 0. (IFCREAL)
    Extracted Wall Area = 0. (IFCREAL)
    Fill Background Pen = "Transparent" (IFCLABEL)
    Fill Pen = "Transparent" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Floor Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.87 (IFCLENGTHMEASURE) [MILLI METRE]
    Length of Perimeter Walls = 15.975 (IFCLENGTHMEASURE) [MILLI METRE]
    Letter Size [mm] = 1. (IFCREAL)
    Measured Area [m2] = 10.69375 (IFCREAL)
    Measured Net Area = 10.69375 (IFCREAL)
    Net Perimeter = 17.45 (IFCLENGTHMEASURE) [MILLI METRE]
    Number of All Corners = 5 (IFCINTEGER)
    Number of Concave Corners = 0 (IFCINTEGER)
    Perimeter = 17.45 (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter of Holes = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Reduced Area = 10.69375 (IFCREAL)
    Roof Surface at the Bottom = 0. (IFCREAL)
    Roof Surface at the Top = 0. (IFCREAL)
    Side Surface of Wall Insets = 0. (IFCREAL)
    Slab Surface at the Bottom = 0. (IFCREAL)
    Slab Surface at the Top = 0. (IFCREAL)
    Subfloor Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Surface Area of Doors = 16.38 (IFCREAL)
    Surface Area of Perimeter Walls = 39.5325 (IFCREAL)
    Surface Area of Windows = 0. (IFCREAL)
    Text Font 1 = "Arial Western" (IFCLABEL)
    Top Surface = 10.69375 (IFCREAL)
    Top Surface of Wall Insets = 0. (IFCREAL)
    Volume = 30.691062 (IFCREAL)
    Zone Area Factor = 1. (IFCREAL)
    Zone Name = "Corridor" (IFCLABEL)
    Zone Number = "102" (IFCLABEL)
    Zone Polygon (Gross, Net) = 0 (IFCINTEGER)
  AC_Pset_Basic_Zone_Stamp | properties | on 1 object (1 IFCSPACE)
    Back Surface of Wall Insets = 0. (IFCREAL)
    Beam Surface at the Bottom = 0. (IFCREAL)
    Beam Surface at the Top = 0. (IFCREAL)
    Bottom Surface = 7.9890569 (IFCREAL)
    Boundary Surface = 37.122807 (IFCREAL)
    Calculated Area = 7.9890569 (IFCREAL)
    Combined Width of Doors = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Combined Width of Windows = 1.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Extracted Area Total = 0. (IFCREAL)
    Extracted Column Area = 0. (IFCREAL)
    Extracted Fill Area = 0. (IFCREAL)
    Extracted Low Areas = 0. (IFCREAL)
    Extracted Wall Area = 0. (IFCREAL)
    Fill Background Pen = "Transparent" (IFCLABEL)
    Fill Pen = "Transparent" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Floor Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 3.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Length of Perimeter Walls = 11.600877 (IFCLENGTHMEASURE) [MILLI METRE]
    Letter Size [mm] = 1. (IFCREAL)
    Measured Area [m2] = 7.9890569 (IFCREAL)
    Measured Net Area = 7.9890569 (IFCREAL)
    Net Perimeter = 11.600877 (IFCLENGTHMEASURE) [MILLI METRE]
    Number of All Corners = 4 (IFCINTEGER)
    Number of Concave Corners = 0 (IFCINTEGER)
    Perimeter = 11.600877 (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter of Holes = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Reduced Area = 7.9890569 (IFCREAL)
    Roof Surface at the Bottom = 0. (IFCREAL)
    Roof Surface at the Top = 0. (IFCREAL)
    Side Surface of Wall Insets = 0. (IFCREAL)
    Slab Surface at the Bottom = 0. (IFCREAL)
    Slab Surface at the Top = 0. (IFCREAL)
    Subfloor Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Surface Area of Doors = 2.1 (IFCREAL)
    Surface Area of Perimeter Walls = 36.373243 (IFCREAL)
    Surface Area of Windows = 2.58 (IFCREAL)
    Text Font 1 = "Arial Western" (IFCLABEL)
    Top Surface = 7.9890569 (IFCREAL)
    Top Surface of Wall Insets = 0. (IFCREAL)
    Volume = 25.564982 (IFCREAL)
    Zone Area Factor = 1. (IFCREAL)
    Zone Name = "Office" (IFCLABEL)
    Zone Number = "110" (IFCLABEL)
    Zone Polygon (Gross, Net) = 0 (IFCINTEGER)
  AC_Pset_Basic_Zone_Stamp | properties | on 1 object (1 IFCSPACE)
    Back Surface of Wall Insets = 0. (IFCREAL)
    Beam Surface at the Bottom = 0. (IFCREAL)
    Beam Surface at the Top = 0. (IFCREAL)
    Bottom Surface = 8.340943 (IFCREAL)
    Boundary Surface = 37.757193 (IFCREAL)
    Calculated Area = 8.340943 (IFCREAL)
    Combined Width of Doors = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Combined Width of Windows = 1.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Extracted Area Total = 0. (IFCREAL)
    Extracted Column Area = 0. (IFCREAL)
    Extracted Fill Area = 0. (IFCREAL)
    Extracted Low Areas = 0. (IFCREAL)
    Extracted Wall Area = 0. (IFCREAL)
    Fill Background Pen = "Transparent" (IFCLABEL)
    Fill Pen = "Transparent" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Floor Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 3.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Length of Perimeter Walls = 11.799123 (IFCLENGTHMEASURE) [MILLI METRE]
    Letter Size [mm] = 1. (IFCREAL)
    Measured Area [m2] = 8.340943 (IFCREAL)
    Measured Net Area = 8.340943 (IFCREAL)
    Net Perimeter = 11.799123 (IFCLENGTHMEASURE) [MILLI METRE]
    Number of All Corners = 4 (IFCINTEGER)
    Number of Concave Corners = 0 (IFCINTEGER)
    Perimeter = 11.799123 (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter of Holes = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Reduced Area = 8.340943 (IFCREAL)
    Roof Surface at the Bottom = 0. (IFCREAL)
    Roof Surface at the Top = 0. (IFCREAL)
    Side Surface of Wall Insets = 0. (IFCREAL)
    Slab Surface at the Bottom = 0. (IFCREAL)
    Slab Surface at the Top = 0. (IFCREAL)
    Subfloor Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Surface Area of Doors = 2.1 (IFCREAL)
    Surface Area of Perimeter Walls = 36.764257 (IFCREAL)
    Surface Area of Windows = 2.9025 (IFCREAL)
    Text Font 1 = "Arial Western" (IFCLABEL)
    Top Surface = 8.340943 (IFCREAL)
    Top Surface of Wall Insets = 0. (IFCREAL)
    Volume = 26.691018 (IFCREAL)
    Zone Area Factor = 1. (IFCREAL)
    Zone Name = "Office" (IFCLABEL)
    Zone Number = "109" (IFCLABEL)
    Zone Polygon (Gross, Net) = 0 (IFCINTEGER)
  AC_Pset_Basic_Zone_Stamp | properties | on 1 object (1 IFCSPACE)
    Back Surface of Wall Insets = 0. (IFCREAL)
    Beam Surface at the Bottom = 0. (IFCREAL)
    Beam Surface at the Top = 0. (IFCREAL)
    Bottom Surface = 25.725 (IFCREAL)
    Boundary Surface = 69.44 (IFCREAL)
    Calculated Area = 25.725 (IFCREAL)
    Combined Width of Doors = 1.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Combined Width of Windows = 6. (IFCLENGTHMEASURE) [MILLI METRE]
    Extracted Area Total = 0. (IFCREAL)
    Extracted Column Area = 0. (IFCREAL)
    Extracted Fill Area = 0. (IFCREAL)
    Extracted Low Areas = 0. (IFCREAL)
    Extracted Wall Area = 0. (IFCREAL)
    Fill Background Pen = "Transparent" (IFCLABEL)
    Fill Pen = "Transparent" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Floor Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 3.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Length of Perimeter Walls = 21.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Letter Size [mm] = 1. (IFCREAL)
    Measured Area [m2] = 25.725 (IFCREAL)
    Measured Net Area = 25.725 (IFCREAL)
    Net Perimeter = 21.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Number of All Corners = 4 (IFCINTEGER)
    Number of Concave Corners = 0 (IFCINTEGER)
    Perimeter = 21.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter of Holes = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Reduced Area = 25.725 (IFCREAL)
    Roof Surface at the Bottom = 0. (IFCREAL)
    Roof Surface at the Top = 0. (IFCREAL)
    Side Surface of Wall Insets = 0. (IFCREAL)
    Slab Surface at the Bottom = 0. (IFCREAL)
    Slab Surface at the Top = 0. (IFCREAL)
    Subfloor Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Surface Area of Doors = 2.94 (IFCREAL)
    Surface Area of Perimeter Walls = 61.58 (IFCREAL)
    Surface Area of Windows = 12.9 (IFCREAL)
    Text Font 1 = "Arial Western" (IFCLABEL)
    Top Surface = 25.725 (IFCREAL)
    Top Surface of Wall Insets = 0. (IFCREAL)
    Volume = 82.32 (IFCREAL)
    Zone Area Factor = 1. (IFCREAL)
    Zone Name = "Conference 2" (IFCLABEL)
    Zone Number = "108" (IFCLABEL)
    Zone Polygon (Gross, Net) = 0 (IFCINTEGER)
  AC_Pset_Basic_Zone_Stamp | properties | on 1 object (1 IFCSPACE)
    Back Surface of Wall Insets = 0. (IFCREAL)
    Beam Surface at the Bottom = 0. (IFCREAL)
    Beam Surface at the Top = 0. (IFCREAL)
    Bottom Surface = 7.71975 (IFCREAL)
    Boundary Surface = 36.064 (IFCREAL)
    Calculated Area = 7.71975 (IFCREAL)
    Combined Width of Doors = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Combined Width of Windows = 1.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Extracted Area Total = 0. (IFCREAL)
    Extracted Column Area = 0. (IFCREAL)
    Extracted Fill Area = 0. (IFCREAL)
    Extracted Low Areas = 0. (IFCREAL)
    Extracted Wall Area = 0. (IFCREAL)
    Fill Background Pen = "Transparent" (IFCLABEL)
    Fill Pen = "Transparent" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Floor Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 3.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Length of Perimeter Walls = 11.27 (IFCLENGTHMEASURE) [MILLI METRE]
    Letter Size [mm] = 1. (IFCREAL)
    Measured Area [m2] = 7.71975 (IFCREAL)
    Measured Net Area = 7.71975 (IFCREAL)
    Net Perimeter = 11.27 (IFCLENGTHMEASURE) [MILLI METRE]
    Number of All Corners = 4 (IFCINTEGER)
    Number of Concave Corners = 0 (IFCINTEGER)
    Perimeter = 11.27 (IFCLENGTHMEASURE) [MILLI METRE]
    Perimeter of Holes = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Reduced Area = 7.71975 (IFCREAL)
    Roof Surface at the Bottom = 0. (IFCREAL)
    Roof Surface at the Top = 0. (IFCREAL)
    Side Surface of Wall Insets = 0. (IFCREAL)
    Slab Surface at the Bottom = 0. (IFCREAL)
    Slab Surface at the Top = 0. (IFCREAL)
    Subfloor Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Surface Area of Doors = 2.1 (IFCREAL)
    Surface Area of Perimeter Walls = 37.345 (IFCREAL)
    Surface Area of Windows = 0. (IFCREAL)
    Text Font 1 = "Arial Western" (IFCLABEL)
    Top Surface = 7.71975 (IFCREAL)
    Top Surface of Wall Insets = 0. (IFCREAL)
    Volume = 24.7032 (IFCREAL)
    Zone Area Factor = 1. (IFCREAL)
    Zone Name = "Women" (IFCLABEL)
    Zone Number = "105" (IFCLABEL)
    Zone Polygon (Gross, Net) = 0 (IFCINTEGER)
  AC_Pset_Basic_Zone_Stamp: 52 more contents on 52 objects not shown
  Pset_SpaceCommon | properties | on 15 objects (15 IFCSPACE)
    GrossPlannedArea = 8. (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_SpaceCommon | properties | on 3 objects (3 IFCSPACE)
    GrossPlannedArea = 7. (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_SpaceCommon | properties | on 2 objects (2 IFCSPACE)
    GrossPlannedArea = 15. (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_SpaceCommon | properties | on 2 objects (2 IFCSPACE)
    GrossPlannedArea = 6. (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    GrossPlannedArea = 25. (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "Toimistotiloja" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    GrossPlannedArea = 20. (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    GrossPlannedArea = 35. (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    GrossPlannedArea = 16. (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_SpaceCommon: 4 more contents on 4 objects not shown
  AC_Pset_Basin_02_13 | properties | on 4 objects (4 IFCFLOWTERMINAL)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    3D (gs_detlevel_3D) = "Detailed" (IFCLABEL)
    3D (gs_detlevel_3D_m) = 2 (IFCINTEGER)
    Accessories = "" (IFCLABEL)
    Area = 0. (IFCREAL)
    Basin Depth = 0.45 (IFCLENGTHMEASURE) [MILLI METRE]
    Basin Material = "Ceramics, glazed" (IFCLABEL)
    Basin Width = 0.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Cold Water Connection = TRUE (IFCBOOLEAN)
    Connection Length (ConLength_1) = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Length (ConLength_2) = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Length (ConLength_3) = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Material = "Stainless Steel" (IFCLABEL)
    Connection Position X (ConPosX_1) = -0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position X (ConPosX_2) = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position X (ConPosX_3) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position Y (ConPosY_1) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position Y (ConPosY_2) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position Y (ConPosY_3) = -0.1675 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position Z (ConPosZ_1) = 0.805 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position Z (ConPosZ_2) = 0.805 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position Z (ConPosZ_3) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Resolution = 8 (IFCINTEGER)
    Connection Type (ConConnectorType_1) = "Welded" (IFCLABEL)
    Connection Type (ConConnectorType_2) = "Welded" (IFCLABEL)
    Connection Type (ConConnectorType_3) = "Welded" (IFCLABEL)
    Connector Depth (ConConnectorDepth_1) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Depth (ConConnectorDepth_2) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Depth (ConConnectorDepth_3) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Diameter (ConConnectorWidth_1) = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Diameter (ConConnectorWidth_2) = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Diameter (ConConnectorWidth_3) = 0.042 (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Width (ConConnectorWidth2_1) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Width (ConConnectorWidth2_2) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Width (ConConnectorWidth2_3) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Contour Pen = "" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Current Connection on the UI = 1 (IFCINTEGER)
    Current UI Page = 1 (IFCINTEGER)
    Drain Material = "Stainless Steel" (IFCLABEL)
    Enable Symbol Types = FALSE (IFCBOOLEAN)
    Fill Background Pen = "" (IFCLABEL)
    Fill Pen = "" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Gauge Type = "" (IFCLABEL)
    Group Type = "Sanitation" (IFCLABEL)
    Hot Water Connection = TRUE (IFCBOOLEAN)
    IFC Enumeration = 9 (IFCINTEGER)
    IFC Subtype = 33 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Location = "" (IFCLABEL)
    MEP System (ConSystem_1) = "Undefined" (IFCLABEL)
    MEP System (ConSystem_2) = "Undefined" (IFCLABEL)
    MEP System (ConSystem_3) = "Undefined" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Material = "" (IFCLABEL)
    Minimal Space in Front = 0.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Minimal Space on the Side 1 = 0.17 (IFCLENGTHMEASURE) [MILLI METRE]
    Minimal Space on the Side 2 = 0.22 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Depth (ConNominalDepth_1) = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Depth (ConNominalDepth_2) = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Depth (ConNominalDepth_3) = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size (ConNominalWidth_1) = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_2) = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_3) = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Number of Connections = 3 (IFCINTEGER)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Outer Depth (ConDepth_1) = 0.027 (IFCLENGTHMEASURE) [MILLI METRE]
    Outer Depth (ConDepth_2) = 0.027 (IFCLENGTHMEASURE) [MILLI METRE]
    Outer Depth (ConDepth_3) = 0.042 (IFCLENGTHMEASURE) [MILLI METRE]
    Outer Diameter (ConWidth_1) = 0.027 (IFCLENGTHMEASURE) [MILLI METRE]
    Outer Diameter (ConWidth_2) = 0.027 (IFCLENGTHMEASURE) [MILLI METRE]
    Outer Diameter (ConWidth_3) = 0.042 (IFCLENGTHMEASURE) [MILLI METRE]
    Product ID = "" (IFCLABEL)
    Product Name = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Recipe = "" (IFCLABEL)
    Resolution = 12 (IFCINTEGER)
    Serial Number = "" (IFCLABEL)
    Set Program = FALSE (IFCBOOLEAN)
    Shadow = TRUE (IFCBOOLEAN)
    Shape Type (ConType_1) = "Circle" (IFCLABEL)
    Shape Type (ConType_2) = "Circle" (IFCLABEL)
    Shape Type (ConType_3) = "Circle" (IFCLABEL)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Support Types = "Pedestal" (IFCLABEL)
    Symbol Type = "Symbolic" (IFCLABEL)
    System Material = "" (IFCLABEL)
    Tap Material = "Chrome" (IFCLABEL)
    Tap Styles = "None" (IFCLABEL)
    Tap Symbol Type = "Detailed" (IFCLABEL)
    Tool Type (ConToolType_1) = 2 (IFCINTEGER)
    Tool Type (ConToolType_2) = 2 (IFCINTEGER)
    Tool Type (ConToolType_3) = 2 (IFCINTEGER)
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Total Height = 0.85 (IFCLENGTHMEASURE) [MILLI METRE]
    Use System Material = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Version = 4 (IFCINTEGER)
    Volume = 0. (IFCREAL)
    Wall Thickness (ConWallThickness_1) = 0.001 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Thickness (ConWallThickness_2) = 0.001 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Thickness (ConWallThickness_3) = 0.001 (IFCLENGTHMEASURE) [MILLI METRE]
    Waste Water Connection = TRUE (IFCBOOLEAN)
  AC_Pset_WC_with_Cistern_13 | properties | on 3 objects (3 IFCFLOWTERMINAL)
    2D Detail Level (gs_detlevel_2D) = "Scale Sensitive" (IFCLABEL)
    2D Detail Level (gs_detlevel_2D_LOC) = "Detailed" (IFCLABEL)
    2D Detail Level (gs_detlevel_2D_m) = 0 (IFCINTEGER)
    3D (gs_detlevel_3D) = "Detailed" (IFCLABEL)
    3D (gs_detlevel_3D_m) = 2 (IFCINTEGER)
    Accessories = "" (IFCLABEL)
    Area = 0. (IFCREAL)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Bowl Material = "Ceramics, glazed" (IFCLABEL)
    Connection Length (ConLength_1) = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Length (ConLength_2) = 0.17 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Material = "Stainless Steel" (IFCLABEL)
    Connection Position X (ConPosX_1) = 0.1850085 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position X (ConPosX_2) = 0.1850085 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position Y (ConPosY_1) = 0.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position Y (ConPosY_2) = 0.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position Z (ConPosZ_1) = 0.7803 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Position Z (ConPosZ_2) = 0.107 (IFCLENGTHMEASURE) [MILLI METRE]
    Connection Type (ConConnectorType_1) = "Welded" (IFCLABEL)
    Connection Type (ConConnectorType_2) = "Welded" (IFCLABEL)
    Connector Depth (ConConnectorDepth_1) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Depth (ConConnectorDepth_2) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Diameter (ConConnectorWidth_1) = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Diameter (ConConnectorWidth_2) = 0.12 (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Width (ConConnectorWidth2_1) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Connector Width (ConConnectorWidth2_2) = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Contour Pen = "" (IFCLABEL)
    Contours in Front View = TRUE (IFCBOOLEAN)
    Cost = 0. (IFCREAL)
    Current Connection on the UI = 1 (IFCINTEGER)
    Current UI Page = 1 (IFCINTEGER)
    Depth = 0.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Enable Symbol Types = FALSE (IFCBOOLEAN)
    Fill Background Pen = "" (IFCLABEL)
    Fill Pen = "" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Gauge Type = "" (IFCLABEL)
    Group Type = "Sanitation" (IFCLABEL)
    Height = 0.81 (IFCLENGTHMEASURE) [MILLI METRE]
    IFC Enumeration = 10 (IFCINTEGER)
    IFC Subtype = 33 (IFCINTEGER)
    Inventory Number = "" (IFCLABEL)
    Location = "" (IFCLABEL)
    MEP System (ConSystem_1) = "Undefined" (IFCLABEL)
    MEP System (ConSystem_2) = "Undefined" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    Material = "" (IFCLABEL)
    Minimal Space in Front = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimal Space on the Side 1 = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Minimal Space on the Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Depth (ConNominalDepth_1) = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Depth (ConNominalDepth_2) = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size (ConNominalWidth_1) = "" (IFCLABEL)
    Nominal Size (ConNominalWidth_2) = "" (IFCLABEL)
    Note/Remarks = "" (IFCLABEL)
    Number of Connections = 2 (IFCINTEGER)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Outer Depth (ConDepth_1) = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Outer Depth (ConDepth_2) = 0.114 (IFCLENGTHMEASURE) [MILLI METRE]
    Outer Diameter (ConWidth_1) = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Outer Diameter (ConWidth_2) = 0.114 (IFCLENGTHMEASURE) [MILLI METRE]
    Product ID = "" (IFCLABEL)
    Product Name = "" (IFCLABEL)
    Production Year = "" (IFCLABEL)
    Recipe = "" (IFCLABEL)
    Resolution = 24 (IFCINTEGER)
    Seat Cover Material = "Plastic laminate" (IFCLABEL)
    Serial Number = "" (IFCLABEL)
    Set Program = FALSE (IFCBOOLEAN)
    Shadow = TRUE (IFCBOOLEAN)
    Shape Type (ConType_1) = "Circle" (IFCLABEL)
    Shape Type (ConType_2) = "Circle" (IFCLABEL)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Show 3D = TRUE (IFCBOOLEAN)
    Symbol Type = "Type 3" (IFCLABEL)
    System Material = "" (IFCLABEL)
    Tank Material = "Ceramics, glazed" (IFCLABEL)
    Tool Type (ConToolType_1) = 2 (IFCINTEGER)
    Tool Type (ConToolType_2) = 2 (IFCINTEGER)
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type (gs_showtank) = TRUE (IFCBOOLEAN)
    Type (gs_wc_type) = "Residential" (IFCLABEL)
    Type of Effluent (DirEffluent) = "Back" (IFCLABEL)
    Type of Effluent (DirEffluent_ID) = 1 (IFCINTEGER)
    Use System Material = FALSE (IFCBOOLEAN)
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
    Version = 4 (IFCINTEGER)
    Volume = 0. (IFCREAL)
    Wall Thickness (ConWallThickness_1) = 0.001 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Thickness (ConWallThickness_2) = 0.002 (IFCLENGTHMEASURE) [MILLI METRE]
    Waste Water = TRUE (IFCBOOLEAN)
    Water = TRUE (IFCBOOLEAN)
    Width = 0.370017 (IFCLENGTHMEASURE) [MILLI METRE]
    code = 0 (IFCINTEGER)
  Pset_SpaceFireSafetyRequirements | properties | on 1 object (1 IFCSPACE)
    FireExit = TRUE (IFCBOOLEAN)
  Pset_ColumnCommon | properties | on 23 objects (23 IFCCOLUMN)
    Reference = "C-4" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 7 objects (7 IFCCOLUMN)
    Reference = "C-2" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    Reference = "C-1" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 54 objects (54 IFCWALLSTANDARDCASE)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_WindowCommon | properties | on 115 objects (115 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
  AC_Pset_W1_14 | properties | on 10 objects (10 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Automatic Shutter Height = TRUE (IFCBOOLEAN)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip In Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness (gs_board_thk) = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width (gs_board_width) = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Below Sill = FALSE (IFCBOOLEAN)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Closing Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Cover Type (gs_slidingShutter_cover) = "Z-Profile" (IFCLABEL)
    Custom Panel Name Left = "" (IFCLABEL)
    Custom Panel Name Lower = "" (IFCLABEL)
    Custom Panel Name Main = "" (IFCLABEL)
    Custom Panel Name Sidelight = "" (IFCLABEL)
    Custom Panel Name Upper = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Enabled Sunshade Types = 127 (IFCINTEGER)
    Extra Frame = FALSE (IFCBOOLEAN)
    Extra Frame Thickness = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Extra Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame=Wall Width = FALSE (IFCBOOLEAN)
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Position = "Throughout" (IFCLABEL)
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Inner Offset = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation Below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Panes Number Horizontally = 2 (IFCINTEGER)
    Left Panes Number Vertically = 4 (IFCINTEGER)
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Panes Number Horizontally = 4 (IFCINTEGER)
    Lower Panes Number Vertically = 2 (IFCINTEGER)
    Lower Transom = FALSE (IFCBOOLEAN)
    Lower Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Main Panes Number Horizontally = 4 (IFCINTEGER)
    Main Panes Number Vertically = 3 (IFCINTEGER)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Reaches Bottom = FALSE (IFCBOOLEAN)
    Mullion Reaches Top = FALSE (IFCBOOLEAN)
    Mullion Width = 0.11 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of panels 2 = 1 (IFCINTEGER)
    Number of panels = 2 (IFCINTEGER)
    Opening Angle = 0. (IFCREAL)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type Left = "" (IFCLABEL)
    Opening Type Lower = "" (IFCLABEL)
    Opening Type Right = "Side Hung" (IFCLABEL)
    Opening Type Sidelight = "" (IFCLABEL)
    Opening Type Upper = "" (IFCLABEL)
    Panel Height = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Position (gs_shutter_iPanelPos) = 1 (IFCINTEGER)
    Panel Position (gs_shutter_panelPos) = "Symmetric" (IFCLABEL)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sash/Total Sash Opening(%) = 50 (IFCINTEGER)
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Style = "No Mullions" (IFCLABEL)
    Sash Style Left = "No Mullions" (IFCLABEL)
    Sash Style Lower = "No Mullions" (IFCLABEL)
    Sash Style Sidelight = "No Mullions" (IFCLABEL)
    Sash Style Upper = "No Mullions" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sidelight = FALSE (IFCBOOLEAN)
    Sidelight Panes Number Horizontally = 2 (IFCINTEGER)
    Sidelight Panes Number Vertically = 2 (IFCINTEGER)
    Sidelight Width = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Keep = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Nosing = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height To Current Story = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip In Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Unit Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Panes Number Horizontally = 4 (IFCINTEGER)
    Upper Panes Number Vertically = 2 (IFCINTEGER)
    Upper Transom = FALSE (IFCBOOLEAN)
    Upper Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 1 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_W1_14 | properties | on 10 objects (10 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Automatic Shutter Height = TRUE (IFCBOOLEAN)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip In Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness (gs_board_thk) = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width (gs_board_width) = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Below Sill = FALSE (IFCBOOLEAN)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Closing Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Cover Type (gs_slidingShutter_cover) = "Z-Profile" (IFCLABEL)
    Custom Panel Name Left = "" (IFCLABEL)
    Custom Panel Name Lower = "" (IFCLABEL)
    Custom Panel Name Main = "" (IFCLABEL)
    Custom Panel Name Sidelight = "" (IFCLABEL)
    Custom Panel Name Upper = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Enabled Sunshade Types = 127 (IFCINTEGER)
    Extra Frame = FALSE (IFCBOOLEAN)
    Extra Frame Thickness = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Extra Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame=Wall Width = FALSE (IFCBOOLEAN)
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Position = "Throughout" (IFCLABEL)
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Inner Offset = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation Below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Panes Number Horizontally = 2 (IFCINTEGER)
    Left Panes Number Vertically = 4 (IFCINTEGER)
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Panes Number Horizontally = 4 (IFCINTEGER)
    Lower Panes Number Vertically = 2 (IFCINTEGER)
    Lower Transom = FALSE (IFCBOOLEAN)
    Lower Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Main Panes Number Horizontally = 4 (IFCINTEGER)
    Main Panes Number Vertically = 3 (IFCINTEGER)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Reaches Bottom = FALSE (IFCBOOLEAN)
    Mullion Reaches Top = FALSE (IFCBOOLEAN)
    Mullion Width = 0.11 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of panels 2 = 1 (IFCINTEGER)
    Number of panels = 2 (IFCINTEGER)
    Opening Angle = 0. (IFCREAL)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type Left = "" (IFCLABEL)
    Opening Type Lower = "" (IFCLABEL)
    Opening Type Right = "Side Hung" (IFCLABEL)
    Opening Type Sidelight = "" (IFCLABEL)
    Opening Type Upper = "" (IFCLABEL)
    Panel Height = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Position (gs_shutter_iPanelPos) = 1 (IFCINTEGER)
    Panel Position (gs_shutter_panelPos) = "Symmetric" (IFCLABEL)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sash/Total Sash Opening(%) = 50 (IFCINTEGER)
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Style = "No Mullions" (IFCLABEL)
    Sash Style Left = "No Mullions" (IFCLABEL)
    Sash Style Lower = "No Mullions" (IFCLABEL)
    Sash Style Sidelight = "No Mullions" (IFCLABEL)
    Sash Style Upper = "No Mullions" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sidelight = FALSE (IFCBOOLEAN)
    Sidelight Panes Number Horizontally = 2 (IFCINTEGER)
    Sidelight Panes Number Vertically = 2 (IFCINTEGER)
    Sidelight Width = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Keep = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Nosing = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height To Current Story = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip In Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Unit Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Panes Number Horizontally = 4 (IFCINTEGER)
    Upper Panes Number Vertically = 2 (IFCINTEGER)
    Upper Transom = FALSE (IFCBOOLEAN)
    Upper Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 1 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_W1_14 | properties | on 7 objects (7 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Automatic Shutter Height = TRUE (IFCBOOLEAN)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip In Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness (gs_board_thk) = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width (gs_board_width) = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Below Sill = FALSE (IFCBOOLEAN)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Closing Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Cover Type (gs_slidingShutter_cover) = "Z-Profile" (IFCLABEL)
    Custom Panel Name Left = "" (IFCLABEL)
    Custom Panel Name Lower = "" (IFCLABEL)
    Custom Panel Name Main = "" (IFCLABEL)
    Custom Panel Name Sidelight = "" (IFCLABEL)
    Custom Panel Name Upper = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Enabled Sunshade Types = 127 (IFCINTEGER)
    Extra Frame = FALSE (IFCBOOLEAN)
    Extra Frame Thickness = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Extra Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame=Wall Width = FALSE (IFCBOOLEAN)
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Position = "Throughout" (IFCLABEL)
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 3.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Inner Offset = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation Below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Panes Number Horizontally = 2 (IFCINTEGER)
    Left Panes Number Vertically = 4 (IFCINTEGER)
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Panes Number Horizontally = 4 (IFCINTEGER)
    Lower Panes Number Vertically = 2 (IFCINTEGER)
    Lower Transom = FALSE (IFCBOOLEAN)
    Lower Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Main Panes Number Horizontally = 4 (IFCINTEGER)
    Main Panes Number Vertically = 3 (IFCINTEGER)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Reaches Bottom = FALSE (IFCBOOLEAN)
    Mullion Reaches Top = FALSE (IFCBOOLEAN)
    Mullion Width = 0.11 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of panels 2 = 1 (IFCINTEGER)
    Number of panels = 2 (IFCINTEGER)
    Opening Angle = 0. (IFCREAL)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type Left = "" (IFCLABEL)
    Opening Type Lower = "" (IFCLABEL)
    Opening Type Right = "Side Hung" (IFCLABEL)
    Opening Type Sidelight = "" (IFCLABEL)
    Opening Type Upper = "" (IFCLABEL)
    Panel Height = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Position (gs_shutter_iPanelPos) = 1 (IFCINTEGER)
    Panel Position (gs_shutter_panelPos) = "Symmetric" (IFCLABEL)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 3.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sash/Total Sash Opening(%) = 50 (IFCINTEGER)
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Style = "No Mullions" (IFCLABEL)
    Sash Style Left = "No Mullions" (IFCLABEL)
    Sash Style Lower = "No Mullions" (IFCLABEL)
    Sash Style Sidelight = "No Mullions" (IFCLABEL)
    Sash Style Upper = "No Mullions" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sidelight = FALSE (IFCBOOLEAN)
    Sidelight Panes Number Horizontally = 2 (IFCINTEGER)
    Sidelight Panes Number Vertically = 2 (IFCINTEGER)
    Sidelight Width = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Keep = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Nosing = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height To Current Story = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip In Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Unit Height = 3.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Panes Number Horizontally = 4 (IFCINTEGER)
    Upper Panes Number Vertically = 2 (IFCINTEGER)
    Upper Transom = FALSE (IFCBOOLEAN)
    Upper Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 1 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 3.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_W1_14 | properties | on 6 objects (6 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Automatic Shutter Height = TRUE (IFCBOOLEAN)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip In Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness (gs_board_thk) = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width (gs_board_width) = 0.22 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Below Sill = FALSE (IFCBOOLEAN)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Closing Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Cover Type (gs_slidingShutter_cover) = "Z-Profile" (IFCLABEL)
    Custom Panel Name Left = "" (IFCLABEL)
    Custom Panel Name Lower = "" (IFCLABEL)
    Custom Panel Name Main = "" (IFCLABEL)
    Custom Panel Name Sidelight = "" (IFCLABEL)
    Custom Panel Name Upper = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Enabled Sunshade Types = 127 (IFCINTEGER)
    Extra Frame = FALSE (IFCBOOLEAN)
    Extra Frame Thickness = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Extra Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame=Wall Width = FALSE (IFCBOOLEAN)
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Position = "Throughout" (IFCLABEL)
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 0.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.17 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 0.34 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Inner Offset = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation Below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.24 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Panes Number Horizontally = 2 (IFCINTEGER)
    Left Panes Number Vertically = 4 (IFCINTEGER)
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Panes Number Horizontally = 4 (IFCINTEGER)
    Lower Panes Number Vertically = 1 (IFCINTEGER)
    Lower Transom = FALSE (IFCBOOLEAN)
    Lower Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Main Panes Number Horizontally = 4 (IFCINTEGER)
    Main Panes Number Vertically = 3 (IFCINTEGER)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Reaches Bottom = FALSE (IFCBOOLEAN)
    Mullion Reaches Top = FALSE (IFCBOOLEAN)
    Mullion Width = 0.11 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of panels 2 = 1 (IFCINTEGER)
    Number of panels = 2 (IFCINTEGER)
    Opening Angle = 0. (IFCREAL)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type Left = "" (IFCLABEL)
    Opening Type Lower = "" (IFCLABEL)
    Opening Type Right = "Side Hung" (IFCLABEL)
    Opening Type Sidelight = "" (IFCLABEL)
    Opening Type Upper = "" (IFCLABEL)
    Panel Height = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Position (gs_shutter_iPanelPos) = 1 (IFCINTEGER)
    Panel Position (gs_shutter_panelPos) = "Symmetric" (IFCLABEL)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 0.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.24 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sash/Total Sash Opening(%) = 50 (IFCINTEGER)
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Style = "No Mullions" (IFCLABEL)
    Sash Style Left = "No Mullions" (IFCLABEL)
    Sash Style Lower = "No Mullions" (IFCLABEL)
    Sash Style Sidelight = "No Mullions" (IFCLABEL)
    Sash Style Upper = "No Mullions" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sidelight = FALSE (IFCBOOLEAN)
    Sidelight Panes Number Horizontally = 2 (IFCINTEGER)
    Sidelight Panes Number Vertically = 2 (IFCINTEGER)
    Sidelight Width = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Keep = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Nosing = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height To Current Story = 2.3282719 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip In Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Unit Height = 0.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Panes Number Horizontally = 4 (IFCINTEGER)
    Upper Panes Number Vertically = 2 (IFCINTEGER)
    Upper Transom = FALSE (IFCBOOLEAN)
    Upper Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 1 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 0.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_W1_14 | properties | on 6 objects (6 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Automatic Shutter Height = TRUE (IFCBOOLEAN)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip In Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness (gs_board_thk) = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width (gs_board_width) = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Below Sill = FALSE (IFCBOOLEAN)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Closing Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Cover Type (gs_slidingShutter_cover) = "Z-Profile" (IFCLABEL)
    Custom Panel Name Left = "" (IFCLABEL)
    Custom Panel Name Lower = "" (IFCLABEL)
    Custom Panel Name Main = "" (IFCLABEL)
    Custom Panel Name Sidelight = "" (IFCLABEL)
    Custom Panel Name Upper = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Enabled Sunshade Types = 127 (IFCINTEGER)
    Extra Frame = FALSE (IFCBOOLEAN)
    Extra Frame Thickness = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Extra Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame=Wall Width = FALSE (IFCBOOLEAN)
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Position = "Throughout" (IFCLABEL)
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Inner Offset = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation Below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Panes Number Horizontally = 2 (IFCINTEGER)
    Left Panes Number Vertically = 4 (IFCINTEGER)
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Panes Number Horizontally = 4 (IFCINTEGER)
    Lower Panes Number Vertically = 2 (IFCINTEGER)
    Lower Transom = FALSE (IFCBOOLEAN)
    Lower Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Main Panes Number Horizontally = 4 (IFCINTEGER)
    Main Panes Number Vertically = 3 (IFCINTEGER)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Reaches Bottom = FALSE (IFCBOOLEAN)
    Mullion Reaches Top = FALSE (IFCBOOLEAN)
    Mullion Width = 0.11 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of panels 2 = 1 (IFCINTEGER)
    Number of panels = 2 (IFCINTEGER)
    Opening Angle = 0. (IFCREAL)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type Left = "" (IFCLABEL)
    Opening Type Lower = "" (IFCLABEL)
    Opening Type Right = "Side Hung" (IFCLABEL)
    Opening Type Sidelight = "" (IFCLABEL)
    Opening Type Upper = "" (IFCLABEL)
    Panel Height = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Position (gs_shutter_iPanelPos) = 1 (IFCINTEGER)
    Panel Position (gs_shutter_panelPos) = "Symmetric" (IFCLABEL)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sash/Total Sash Opening(%) = 50 (IFCINTEGER)
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Style = "No Mullions" (IFCLABEL)
    Sash Style Left = "No Mullions" (IFCLABEL)
    Sash Style Lower = "No Mullions" (IFCLABEL)
    Sash Style Sidelight = "No Mullions" (IFCLABEL)
    Sash Style Upper = "No Mullions" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sidelight = FALSE (IFCBOOLEAN)
    Sidelight Panes Number Horizontally = 2 (IFCINTEGER)
    Sidelight Panes Number Vertically = 2 (IFCINTEGER)
    Sidelight Width = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Keep = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Nosing = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height To Current Story = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip In Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Unit Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Panes Number Horizontally = 4 (IFCINTEGER)
    Upper Panes Number Vertically = 2 (IFCINTEGER)
    Upper Transom = FALSE (IFCBOOLEAN)
    Upper Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_W1_14 | properties | on 6 objects (6 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Automatic Shutter Height = TRUE (IFCBOOLEAN)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip In Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness (gs_board_thk) = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width (gs_board_width) = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Below Sill = FALSE (IFCBOOLEAN)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Closing Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Cover Type (gs_slidingShutter_cover) = "Z-Profile" (IFCLABEL)
    Custom Panel Name Left = "" (IFCLABEL)
    Custom Panel Name Lower = "" (IFCLABEL)
    Custom Panel Name Main = "" (IFCLABEL)
    Custom Panel Name Sidelight = "" (IFCLABEL)
    Custom Panel Name Upper = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Enabled Sunshade Types = 127 (IFCINTEGER)
    Extra Frame = FALSE (IFCBOOLEAN)
    Extra Frame Thickness = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Extra Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame=Wall Width = FALSE (IFCBOOLEAN)
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Position = "Throughout" (IFCLABEL)
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Inner Offset = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation Below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Panes Number Horizontally = 2 (IFCINTEGER)
    Left Panes Number Vertically = 4 (IFCINTEGER)
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Panes Number Horizontally = 4 (IFCINTEGER)
    Lower Panes Number Vertically = 2 (IFCINTEGER)
    Lower Transom = FALSE (IFCBOOLEAN)
    Lower Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Main Panes Number Horizontally = 4 (IFCINTEGER)
    Main Panes Number Vertically = 3 (IFCINTEGER)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Reaches Bottom = FALSE (IFCBOOLEAN)
    Mullion Reaches Top = FALSE (IFCBOOLEAN)
    Mullion Width = 0.11 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of panels 2 = 1 (IFCINTEGER)
    Number of panels = 2 (IFCINTEGER)
    Opening Angle = 0. (IFCREAL)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type Left = "" (IFCLABEL)
    Opening Type Lower = "" (IFCLABEL)
    Opening Type Right = "Side Hung" (IFCLABEL)
    Opening Type Sidelight = "" (IFCLABEL)
    Opening Type Upper = "" (IFCLABEL)
    Panel Height = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Position (gs_shutter_iPanelPos) = 1 (IFCINTEGER)
    Panel Position (gs_shutter_panelPos) = "Symmetric" (IFCLABEL)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sash/Total Sash Opening(%) = 50 (IFCINTEGER)
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Style = "No Mullions" (IFCLABEL)
    Sash Style Left = "No Mullions" (IFCLABEL)
    Sash Style Lower = "No Mullions" (IFCLABEL)
    Sash Style Sidelight = "No Mullions" (IFCLABEL)
    Sash Style Upper = "No Mullions" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sidelight = FALSE (IFCBOOLEAN)
    Sidelight Panes Number Horizontally = 2 (IFCINTEGER)
    Sidelight Panes Number Vertically = 2 (IFCINTEGER)
    Sidelight Width = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Keep = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Nosing = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height To Current Story = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip In Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Unit Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Panes Number Horizontally = 4 (IFCINTEGER)
    Upper Panes Number Vertically = 2 (IFCINTEGER)
    Upper Transom = FALSE (IFCBOOLEAN)
    Upper Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_W1_14 | properties | on 1 object (1 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Automatic Shutter Height = TRUE (IFCBOOLEAN)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip In Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness (gs_board_thk) = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width (gs_board_width) = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Below Sill = FALSE (IFCBOOLEAN)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Closing Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Cover Type (gs_slidingShutter_cover) = "Z-Profile" (IFCLABEL)
    Custom Panel Name Left = "" (IFCLABEL)
    Custom Panel Name Lower = "" (IFCLABEL)
    Custom Panel Name Main = "" (IFCLABEL)
    Custom Panel Name Sidelight = "" (IFCLABEL)
    Custom Panel Name Upper = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Enabled Sunshade Types = 127 (IFCINTEGER)
    Extra Frame = FALSE (IFCBOOLEAN)
    Extra Frame Thickness = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Extra Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame=Wall Width = FALSE (IFCBOOLEAN)
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Position = "Throughout" (IFCLABEL)
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 8.451849 (IFCREAL)
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Inner Offset = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation Below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Panes Number Horizontally = 2 (IFCINTEGER)
    Left Panes Number Vertically = 4 (IFCINTEGER)
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Panes Number Horizontally = 4 (IFCINTEGER)
    Lower Panes Number Vertically = 2 (IFCINTEGER)
    Lower Transom = FALSE (IFCBOOLEAN)
    Lower Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Main Panes Number Horizontally = 4 (IFCINTEGER)
    Main Panes Number Vertically = 3 (IFCINTEGER)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Reaches Bottom = FALSE (IFCBOOLEAN)
    Mullion Reaches Top = FALSE (IFCBOOLEAN)
    Mullion Width = 0.11 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of panels 2 = 1 (IFCINTEGER)
    Number of panels = 2 (IFCINTEGER)
    Opening Angle = 0. (IFCREAL)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type Left = "" (IFCLABEL)
    Opening Type Lower = "" (IFCLABEL)
    Opening Type Right = "Side Hung" (IFCLABEL)
    Opening Type Sidelight = "" (IFCLABEL)
    Opening Type Upper = "" (IFCLABEL)
    Panel Height = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Position (gs_shutter_iPanelPos) = 1 (IFCINTEGER)
    Panel Position (gs_shutter_panelPos) = "Symmetric" (IFCLABEL)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sash/Total Sash Opening(%) = 50 (IFCINTEGER)
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Style = "No Mullions" (IFCLABEL)
    Sash Style Left = "No Mullions" (IFCLABEL)
    Sash Style Lower = "No Mullions" (IFCLABEL)
    Sash Style Sidelight = "No Mullions" (IFCLABEL)
    Sash Style Upper = "No Mullions" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sidelight = FALSE (IFCBOOLEAN)
    Sidelight Panes Number Horizontally = 2 (IFCINTEGER)
    Sidelight Panes Number Vertically = 2 (IFCINTEGER)
    Sidelight Width = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Keep = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Nosing = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height To Current Story = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip In Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Unit Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Panes Number Horizontally = 4 (IFCINTEGER)
    Upper Panes Number Vertically = 2 (IFCINTEGER)
    Upper Transom = FALSE (IFCBOOLEAN)
    Upper Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_W1_14 | properties | on 1 object (1 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Automatic Shutter Height = TRUE (IFCBOOLEAN)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip In Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness (gs_board_thk) = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width (gs_board_width) = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Below Sill = FALSE (IFCBOOLEAN)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Closing Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Cover Type (gs_slidingShutter_cover) = "Z-Profile" (IFCLABEL)
    Custom Panel Name Left = "" (IFCLABEL)
    Custom Panel Name Lower = "" (IFCLABEL)
    Custom Panel Name Main = "" (IFCLABEL)
    Custom Panel Name Sidelight = "" (IFCLABEL)
    Custom Panel Name Upper = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Enabled Sunshade Types = 127 (IFCINTEGER)
    Extra Frame = FALSE (IFCBOOLEAN)
    Extra Frame Thickness = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Extra Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame=Wall Width = FALSE (IFCBOOLEAN)
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Position = "Throughout" (IFCLABEL)
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 3.6203064 (IFCREAL)
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Inner Offset = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation Below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Left Panes Number Horizontally = 2 (IFCINTEGER)
    Left Panes Number Vertically = 4 (IFCINTEGER)
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Panes Number Horizontally = 4 (IFCINTEGER)
    Lower Panes Number Vertically = 2 (IFCINTEGER)
    Lower Transom = FALSE (IFCBOOLEAN)
    Lower Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Main Panes Number Horizontally = 4 (IFCINTEGER)
    Main Panes Number Vertically = 3 (IFCINTEGER)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Reaches Bottom = FALSE (IFCBOOLEAN)
    Mullion Reaches Top = FALSE (IFCBOOLEAN)
    Mullion Width = 0.11 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of panels 2 = 1 (IFCINTEGER)
    Number of panels = 2 (IFCINTEGER)
    Opening Angle = 0. (IFCREAL)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type Left = "" (IFCLABEL)
    Opening Type Lower = "" (IFCLABEL)
    Opening Type Right = "Side Hung" (IFCLABEL)
    Opening Type Sidelight = "" (IFCLABEL)
    Opening Type Upper = "" (IFCLABEL)
    Panel Height = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Position (gs_shutter_iPanelPos) = 1 (IFCINTEGER)
    Panel Position (gs_shutter_panelPos) = "Symmetric" (IFCLABEL)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sash/Total Sash Opening(%) = 50 (IFCINTEGER)
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Style = "No Mullions" (IFCLABEL)
    Sash Style Left = "No Mullions" (IFCLABEL)
    Sash Style Lower = "No Mullions" (IFCLABEL)
    Sash Style Sidelight = "No Mullions" (IFCLABEL)
    Sash Style Upper = "No Mullions" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sidelight = FALSE (IFCBOOLEAN)
    Sidelight Panes Number Horizontally = 2 (IFCINTEGER)
    Sidelight Panes Number Vertically = 2 (IFCINTEGER)
    Sidelight Width = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Keep = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Frame Nosing = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height To Current Story = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip In Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Unit Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Panes Number Horizontally = 4 (IFCINTEGER)
    Upper Panes Number Vertically = 2 (IFCINTEGER)
    Upper Transom = FALSE (IFCBOOLEAN)
    Upper Transom Height = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_W1_14: 36 more contents on 36 objects not shown
  AC_Pset_Window_16 | properties | on 6 objects (6 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip-in Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing below Sill = FALSE (IFCBOOLEAN)
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Lower Sash = "" (IFCLABEL)
    Custom Panel Name 2 Main Sash = "" (IFCLABEL)
    Custom Panel Name 2 Transom Sash = "" (IFCLABEL)
    Custom Panel Name Lower Sash = "" (IFCLABEL)
    Custom Panel Name Main Sash = "" (IFCLABEL)
    Custom Panel Name Transom Sash = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Lower Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Main Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Insulation below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Transom = FALSE (IFCBOOLEAN)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mirrored Custom Panel (gs_bMirr_cust_panel2_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_03) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_03) = FALSE (IFCBOOLEAN)
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type (gs_optype_m_01) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_03) = 1 (IFCINTEGER)
    Opening Type Lower Sash = "" (IFCLABEL)
    Opening Type Main Sash = "Side Hung" (IFCLABEL)
    Opening Type Transom Sash = "" (IFCLABEL)
    Panes Number Horizontally 2 Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Transom Sash = 4 (IFCINTEGER)
    Panes Number Vertically 2 Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically 2 Transom Sash = 1 (IFCINTEGER)
    Panes Number Vertically Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically Transom Sash = 1 (IFCINTEGER)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_01) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_03) = 1 (IFCINTEGER)
    Sash Type Lower Sash = "" (IFCLABEL)
    Sash Type Main Sash = "No Mullions" (IFCLABEL)
    Sash Type Transom Sash = "" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height to Current Story = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip-in Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Uniform Frame Width = FALSE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Unit Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Transom = FALSE (IFCBOOLEAN)
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.55 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Window_16 | properties | on 2 objects (2 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip-in Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width = 0.22 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing below Sill = FALSE (IFCBOOLEAN)
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Lower Sash = "" (IFCLABEL)
    Custom Panel Name 2 Main Sash = "" (IFCLABEL)
    Custom Panel Name 2 Transom Sash = "" (IFCLABEL)
    Custom Panel Name Lower Sash = "" (IFCLABEL)
    Custom Panel Name Main Sash = "" (IFCLABEL)
    Custom Panel Name Transom Sash = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Lower Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Main Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Insulation below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.24 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Transom = FALSE (IFCBOOLEAN)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mirrored Custom Panel (gs_bMirr_cust_panel2_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_03) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_03) = FALSE (IFCBOOLEAN)
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type (gs_optype_m_01) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_03) = 1 (IFCINTEGER)
    Opening Type Lower Sash = "" (IFCLABEL)
    Opening Type Main Sash = "Side Hung" (IFCLABEL)
    Opening Type Transom Sash = "" (IFCLABEL)
    Panes Number Horizontally 2 Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Transom Sash = 4 (IFCINTEGER)
    Panes Number Vertically 2 Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically 2 Transom Sash = 1 (IFCINTEGER)
    Panes Number Vertically Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically Transom Sash = 1 (IFCINTEGER)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 1.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.24 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_01) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_03) = 1 (IFCINTEGER)
    Sash Type Lower Sash = "" (IFCLABEL)
    Sash Type Main Sash = "No Mullions" (IFCLABEL)
    Sash Type Transom Sash = "" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height to Current Story = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip-in Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Uniform Frame Width = FALSE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Unit Height = 1.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Transom = FALSE (IFCBOOLEAN)
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 1.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Window_16 | properties | on 2 objects (2 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip-in Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width = 0.22 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing below Sill = FALSE (IFCBOOLEAN)
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Lower Sash = "" (IFCLABEL)
    Custom Panel Name 2 Main Sash = "" (IFCLABEL)
    Custom Panel Name 2 Transom Sash = "" (IFCLABEL)
    Custom Panel Name Lower Sash = "" (IFCLABEL)
    Custom Panel Name Main Sash = "" (IFCLABEL)
    Custom Panel Name Transom Sash = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Lower Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Main Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Insulation below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.24 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Transom = FALSE (IFCBOOLEAN)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mirrored Custom Panel (gs_bMirr_cust_panel2_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_03) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_03) = FALSE (IFCBOOLEAN)
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type (gs_optype_m_01) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_03) = 1 (IFCINTEGER)
    Opening Type Lower Sash = "" (IFCLABEL)
    Opening Type Main Sash = "Side Hung" (IFCLABEL)
    Opening Type Transom Sash = "" (IFCLABEL)
    Panes Number Horizontally 2 Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Transom Sash = 4 (IFCINTEGER)
    Panes Number Vertically 2 Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically 2 Transom Sash = 1 (IFCINTEGER)
    Panes Number Vertically Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically Transom Sash = 1 (IFCINTEGER)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.24 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_01) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_03) = 1 (IFCINTEGER)
    Sash Type Lower Sash = "" (IFCLABEL)
    Sash Type Main Sash = "No Mullions" (IFCLABEL)
    Sash Type Transom Sash = "" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height to Current Story = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip-in Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Uniform Frame Width = FALSE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Unit Height = 2.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Transom = FALSE (IFCBOOLEAN)
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.35 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.7 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Window_16 | properties | on 1 object (1 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip-in Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing below Sill = FALSE (IFCBOOLEAN)
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Lower Sash = "" (IFCLABEL)
    Custom Panel Name 2 Main Sash = "" (IFCLABEL)
    Custom Panel Name 2 Transom Sash = "" (IFCLABEL)
    Custom Panel Name Lower Sash = "" (IFCLABEL)
    Custom Panel Name Main Sash = "" (IFCLABEL)
    Custom Panel Name Transom Sash = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 3.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Lower Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Main Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Insulation below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Transom = FALSE (IFCBOOLEAN)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mirrored Custom Panel (gs_bMirr_cust_panel2_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_03) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_03) = FALSE (IFCBOOLEAN)
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type (gs_optype_m_01) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_03) = 1 (IFCINTEGER)
    Opening Type Lower Sash = "" (IFCLABEL)
    Opening Type Main Sash = "Side Hung" (IFCLABEL)
    Opening Type Transom Sash = "" (IFCLABEL)
    Panes Number Horizontally 2 Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Transom Sash = 4 (IFCINTEGER)
    Panes Number Vertically 2 Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically 2 Transom Sash = 1 (IFCINTEGER)
    Panes Number Vertically Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically Transom Sash = 1 (IFCINTEGER)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 3.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_01) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_03) = 1 (IFCINTEGER)
    Sash Type Lower Sash = "" (IFCLABEL)
    Sash Type Main Sash = "No Mullions" (IFCLABEL)
    Sash Type Transom Sash = "" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height to Current Story = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip-in Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Uniform Frame Width = FALSE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Unit Height = 3.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Transom = FALSE (IFCBOOLEAN)
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 3.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Window_16 | properties | on 1 object (1 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip-in Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing below Sill = FALSE (IFCBOOLEAN)
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Lower Sash = "" (IFCLABEL)
    Custom Panel Name 2 Main Sash = "" (IFCLABEL)
    Custom Panel Name 2 Transom Sash = "" (IFCLABEL)
    Custom Panel Name Lower Sash = "" (IFCLABEL)
    Custom Panel Name Main Sash = "" (IFCLABEL)
    Custom Panel Name Transom Sash = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 1.5098548 (IFCREAL)
    Horizontal Division Height Lower Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Main Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Insulation below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Transom = FALSE (IFCBOOLEAN)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mirrored Custom Panel (gs_bMirr_cust_panel2_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_03) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_03) = FALSE (IFCBOOLEAN)
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type (gs_optype_m_01) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_03) = 1 (IFCINTEGER)
    Opening Type Lower Sash = "" (IFCLABEL)
    Opening Type Main Sash = "Side Hung" (IFCLABEL)
    Opening Type Transom Sash = "" (IFCLABEL)
    Panes Number Horizontally 2 Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Transom Sash = 4 (IFCINTEGER)
    Panes Number Vertically 2 Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically 2 Transom Sash = 1 (IFCINTEGER)
    Panes Number Vertically Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically Transom Sash = 1 (IFCINTEGER)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_01) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_03) = 1 (IFCINTEGER)
    Sash Type Lower Sash = "" (IFCLABEL)
    Sash Type Main Sash = "No Mullions" (IFCLABEL)
    Sash Type Transom Sash = "" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height to Current Story = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip-in Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Uniform Frame Width = FALSE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Unit Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Transom = FALSE (IFCBOOLEAN)
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Window_16 | properties | on 1 object (1 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip-in Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing below Sill = FALSE (IFCBOOLEAN)
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Lower Sash = "" (IFCLABEL)
    Custom Panel Name 2 Main Sash = "" (IFCLABEL)
    Custom Panel Name 2 Transom Sash = "" (IFCLABEL)
    Custom Panel Name Lower Sash = "" (IFCLABEL)
    Custom Panel Name Main Sash = "" (IFCLABEL)
    Custom Panel Name Transom Sash = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = -4.5191994 (IFCREAL)
    Horizontal Division Height Lower Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Main Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Insulation below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Transom = FALSE (IFCBOOLEAN)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mirrored Custom Panel (gs_bMirr_cust_panel2_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_03) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_03) = FALSE (IFCBOOLEAN)
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type (gs_optype_m_01) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_03) = 1 (IFCINTEGER)
    Opening Type Lower Sash = "" (IFCLABEL)
    Opening Type Main Sash = "Side Hung" (IFCLABEL)
    Opening Type Transom Sash = "" (IFCLABEL)
    Panes Number Horizontally 2 Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Transom Sash = 4 (IFCINTEGER)
    Panes Number Vertically 2 Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically 2 Transom Sash = 1 (IFCINTEGER)
    Panes Number Vertically Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically Transom Sash = 1 (IFCINTEGER)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_01) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_03) = 1 (IFCINTEGER)
    Sash Type Lower Sash = "" (IFCLABEL)
    Sash Type Main Sash = "No Mullions" (IFCLABEL)
    Sash Type Transom Sash = "" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height to Current Story = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip-in Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Uniform Frame Width = FALSE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Unit Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Transom = FALSE (IFCBOOLEAN)
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Window_16 | properties | on 1 object (1 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip-in Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing below Sill = FALSE (IFCBOOLEAN)
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Lower Sash = "" (IFCLABEL)
    Custom Panel Name 2 Main Sash = "" (IFCLABEL)
    Custom Panel Name 2 Transom Sash = "" (IFCLABEL)
    Custom Panel Name Lower Sash = "" (IFCLABEL)
    Custom Panel Name Main Sash = "" (IFCLABEL)
    Custom Panel Name Transom Sash = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 18.452148 (IFCREAL)
    Horizontal Division Height Lower Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Main Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Insulation below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Transom = FALSE (IFCBOOLEAN)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mirrored Custom Panel (gs_bMirr_cust_panel2_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_03) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_03) = FALSE (IFCBOOLEAN)
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type (gs_optype_m_01) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_03) = 1 (IFCINTEGER)
    Opening Type Lower Sash = "" (IFCLABEL)
    Opening Type Main Sash = "Side Hung" (IFCLABEL)
    Opening Type Transom Sash = "" (IFCLABEL)
    Panes Number Horizontally 2 Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Transom Sash = 4 (IFCINTEGER)
    Panes Number Vertically 2 Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically 2 Transom Sash = 1 (IFCINTEGER)
    Panes Number Vertically Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically Transom Sash = 1 (IFCINTEGER)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_01) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_03) = 1 (IFCINTEGER)
    Sash Type Lower Sash = "" (IFCLABEL)
    Sash Type Main Sash = "No Mullions" (IFCLABEL)
    Sash Type Transom Sash = "" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height to Current Story = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip-in Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Uniform Frame Width = FALSE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Unit Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Transom = FALSE (IFCBOOLEAN)
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Window_16 | properties | on 1 object (1 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Board = FALSE (IFCBOOLEAN)
    Board Angle = 0. (IFCREAL)
    Board Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Slip-in Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Board Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Board Width = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Board in Polygonal Walls = "Parallel to Window" (IFCLABEL)
    Board is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Bottom Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing below Sill = FALSE (IFCBOOLEAN)
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Lower Sash = "" (IFCLABEL)
    Custom Panel Name 2 Main Sash = "" (IFCLABEL)
    Custom Panel Name 2 Transom Sash = "" (IFCLABEL)
    Custom Panel Name Lower Sash = "" (IFCLABEL)
    Custom Panel Name Main Sash = "" (IFCLABEL)
    Custom Panel Name Transom Sash = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = -21.461492 (IFCREAL)
    Horizontal Division Height Lower Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Main Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Sash = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Insulation below Sill = TRUE (IFCBOOLEAN)
    Left Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Transom = FALSE (IFCBOOLEAN)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mirrored Custom Panel (gs_bMirr_cust_panel2_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel2_03) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_03) = FALSE (IFCBOOLEAN)
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type (gs_optype_m_01) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_03) = 1 (IFCINTEGER)
    Opening Type Lower Sash = "" (IFCLABEL)
    Opening Type Main Sash = "Side Hung" (IFCLABEL)
    Opening Type Transom Sash = "" (IFCLABEL)
    Panes Number Horizontally 2 Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Lower Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Main Sash = 4 (IFCINTEGER)
    Panes Number Horizontally Transom Sash = 4 (IFCINTEGER)
    Panes Number Vertically 2 Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically 2 Transom Sash = 1 (IFCINTEGER)
    Panes Number Vertically Lower Sash = 1 (IFCINTEGER)
    Panes Number Vertically Main Sash = 3 (IFCINTEGER)
    Panes Number Vertically Transom Sash = 1 (IFCINTEGER)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_01) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_03) = 1 (IFCINTEGER)
    Sash Type Lower Sash = "" (IFCLABEL)
    Sash Type Main Sash = "No Mullions" (IFCLABEL)
    Sash Type Transom Sash = "" (IFCLABEL)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sill = FALSE (IFCBOOLEAN)
    Sill Angle = 3. (IFCREAL)
    Sill Drip Overlap = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Drip Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Elevation = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Front Side Thickness = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height to Current Story = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Oversize = FALSE (IFCBOOLEAN)
    Sill Slip from Wall = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip-in Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill is Curved in Curved Walls = TRUE (IFCBOOLEAN)
    Sunshade Type (gs_sunShade_iType) = 0 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "None" (IFCLABEL)
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Type of the Sill = "Timber Sill" (IFCLABEL)
    Uniform Frame Width = FALSE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Unit Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Transom = FALSE (IFCBOOLEAN)
    Use Wall Insulation Skin = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.95 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0.75 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Double_Sash_Window_16 | properties | on 10 objects (10 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Bottom Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing below Sill = FALSE (IFCBOOLEAN)
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Lower Sash 1 = "" (IFCLABEL)
    Custom Panel Name 2 Lower Sash 2 = "" (IFCLABEL)
    Custom Panel Name 2 Main Sash 1 = "" (IFCLABEL)
    Custom Panel Name 2 Main Sash 2 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Sash 1 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Sash 2 = "" (IFCLABEL)
    Custom Panel Name Lower Sash 1 = "" (IFCLABEL)
    Custom Panel Name Lower Sash 2 = "" (IFCLABEL)
    Custom Panel Name Main Sash 1 = "" (IFCLABEL)
    Custom Panel Name Main Sash 2 = "" (IFCLABEL)
    Custom Panel Name Transom Sash 1 = "" (IFCLABEL)
    Custom Panel Name Transom Sash 2 = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Divided Lower Transom = FALSE (IFCBOOLEAN)
    Divided Upper Transom = FALSE (IFCBOOLEAN)
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Lower Sash 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Lower Sash 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Main Sash 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Main Sash 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Sash 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Sash 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Left Connected Wall Thickness = 0.24 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Transom = FALSE (IFCBOOLEAN)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mirrored Custom Panel (gs_bMirr_cust_panel_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_03) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_05) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_06) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_07) = FALSE (IFCBOOLEAN)
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    Mullion Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type (gs_optype_m_01) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_03) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_05) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_06) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_07) = 1 (IFCINTEGER)
    Opening Type Lower Sash 1 = "" (IFCLABEL)
    Opening Type Lower Sash 2 = "" (IFCLABEL)
    Opening Type Main Sash 2 = "Side Hung" (IFCLABEL)
    Opening Type Main Sashes = "Side Hung" (IFCLABEL)
    Opening Type Transom Sash 1 = "" (IFCLABEL)
    Opening Type Transom Sash 2 = "" (IFCLABEL)
    Panes Configuration (gs_PanesConfig) = "Uniform Panes" (IFCLABEL)
    Panes Configuration (gs_iPanesConfig) = 1 (IFCINTEGER)
    Panes Number Horizontally 2 Lower Sash 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Lower Sash 2 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash 2 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Sash 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Sash 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Lower Sash 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Lower Sash 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Sash 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Sash 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Lower Sash 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Lower Sash 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Sash 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Sash 2 = 2 (IFCINTEGER)
    Panes Number Vertically Lower Sash 1 = 2 (IFCINTEGER)
    Panes Number Vertically Lower Sash 2 = 2 (IFCINTEGER)
    Panes Number Vertically Main Sash 1 = 2 (IFCINTEGER)
    Panes Number Vertically Main Sash 2 = 2 (IFCINTEGER)
    Panes Number Vertically Transom Sash 1 = 2 (IFCINTEGER)
    Panes Number Vertically Transom Sash 2 = 2 (IFCINTEGER)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 1.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.24 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_01) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_03) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_05) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_06) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_07) = 1 (IFCINTEGER)
    Sash Type Lower Sash 1 = "" (IFCLABEL)
    Sash Type Lower Sash 2 = "" (IFCLABEL)
    Sash Type Main Sash 1 = "No Mullions" (IFCLABEL)
    Sash Type Main Sash 2 = "No Mullions" (IFCLABEL)
    Sash Type Transom Sash 1 = "" (IFCLABEL)
    Sash Type Transom Sash 2 = "" (IFCLABEL)
    Sash Width Side 1 = 0.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sill Height to Current Story = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Uniform Frame Width = FALSE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Unit Height = 1.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Transom = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 1.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Double_Sash_Window_16 | properties | on 7 objects (7 IFCWINDOW)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    2D Detail Level Enable = 103 (IFCINTEGER)
    3D Detail Level = "Detailed" (IFCLABEL)
    3D Detail Level Enable = 14 (IFCINTEGER)
    Bottom Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing = "Off" (IFCLABEL)
    Casing Offset Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Offset Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Bottom Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Left Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Overhang Top Right Outside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Thickness Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "Rectangular" (IFCLABEL)
    Casing Type Outside = "Rectangular" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Left Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Right Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Top Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Inside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width on Bottom Outside = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing below Sill = FALSE (IFCBOOLEAN)
    Connecting Wall Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Angle = 90. (IFCREAL)
    Corner Column = FALSE (IFCBOOLEAN)
    Corner Column Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Column Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Corner Connection Type = "Frame" (IFCLABEL)
    Corner Window Debug Function = FALSE (IFCBOOLEAN)
    Corner Window Function = TRUE (IFCBOOLEAN)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Lower Sash 1 = "" (IFCLABEL)
    Custom Panel Name 2 Lower Sash 2 = "" (IFCLABEL)
    Custom Panel Name 2 Main Sash 1 = "" (IFCLABEL)
    Custom Panel Name 2 Main Sash 2 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Sash 1 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Sash 2 = "" (IFCLABEL)
    Custom Panel Name Lower Sash 1 = "" (IFCLABEL)
    Custom Panel Name Lower Sash 2 = "" (IFCLABEL)
    Custom Panel Name Main Sash 1 = "" (IFCLABEL)
    Custom Panel Name Main Sash 2 = "" (IFCLABEL)
    Custom Panel Name Transom Sash 1 = "" (IFCLABEL)
    Custom Panel Name Transom Sash 2 = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition line type = 4 (IFCINTEGER)
    Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Divided Lower Transom = FALSE (IFCBOOLEAN)
    Divided Upper Transom = FALSE (IFCBOOLEAN)
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Thickness = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Lower Horiz. Divisions = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Height of Upper Horiz. Divisions = 1.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Lower Sash 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Lower Sash 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Main Sash 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Main Sash 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Sash 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Sash 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Left Connected Wall Thickness = 0.24 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Corner = FALSE (IFCBOOLEAN)
    Left Corner Angle = 90. (IFCREAL)
    Left Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Left Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lower Transom = FALSE (IFCBOOLEAN)
    Maximal Tolerance = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Mirrored Custom Panel (gs_bMirr_cust_panel_01) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_02) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_03) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_05) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_06) = FALSE (IFCBOOLEAN)
    Mirrored Custom Panel (gs_bMirr_cust_panel_07) = FALSE (IFCBOOLEAN)
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    Mullion Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Opening Direction (gs_opening_dir) = "Inside" (IFCLABEL)
    Opening Type (gs_optype_m_01) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_03) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_05) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_06) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_07) = 1 (IFCINTEGER)
    Opening Type Lower Sash 1 = "" (IFCLABEL)
    Opening Type Lower Sash 2 = "" (IFCLABEL)
    Opening Type Main Sash 2 = "Side Hung" (IFCLABEL)
    Opening Type Main Sashes = "Side Hung" (IFCLABEL)
    Opening Type Transom Sash 1 = "" (IFCLABEL)
    Opening Type Transom Sash 2 = "" (IFCLABEL)
    Panes Configuration (gs_PanesConfig) = "Uniform Panes" (IFCLABEL)
    Panes Configuration (gs_iPanesConfig) = 1 (IFCINTEGER)
    Panes Number Horizontally 2 Lower Sash 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Lower Sash 2 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash 2 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Sash 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Sash 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Lower Sash 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Lower Sash 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Sash 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Sash 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Lower Sash 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Lower Sash 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Sash 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Sash 2 = 2 (IFCINTEGER)
    Panes Number Vertically Lower Sash 1 = 2 (IFCINTEGER)
    Panes Number Vertically Lower Sash 2 = 2 (IFCINTEGER)
    Panes Number Vertically Main Sash 1 = 2 (IFCINTEGER)
    Panes Number Vertically Main Sash 2 = 2 (IFCINTEGER)
    Panes Number Vertically Transom Sash 1 = 2 (IFCINTEGER)
    Panes Number Vertically Transom Sash 2 = 2 (IFCINTEGER)
    Parametric Level = "High" (IFCLABEL)
    Placement Type (1=CW,0=W) = FALSE (IFCBOOLEAN)
    Rebate Depth = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Connected Wall Thickness = 0.24 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Corner = FALSE (IFCBOOLEAN)
    Right Corner Angle = 90. (IFCREAL)
    Right Corner Connection Type = "Frame" (IFCLABEL)
    Right Diff. Conn. Wall Thickness = FALSE (IFCBOOLEAN)
    Right Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_01) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_03) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_05) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_06) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_07) = 1 (IFCINTEGER)
    Sash Type Lower Sash 1 = "" (IFCLABEL)
    Sash Type Lower Sash 2 = "" (IFCLABEL)
    Sash Type Main Sash 1 = "No Mullions" (IFCLABEL)
    Sash Type Main Sash 2 = "No Mullions" (IFCLABEL)
    Sash Type Transom Sash 1 = "" (IFCLABEL)
    Sash Type Transom Sash 2 = "" (IFCLABEL)
    Sash Width Side 1 = 0.6 (IFCLENGTHMEASURE) [MILLI METRE]
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sill Height to Current Story = 0.74277127 (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Uniform Frame Width = FALSE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Unit Height = 2.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Division Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Opening Oversize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Transom = FALSE (IFCBOOLEAN)
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_DoorCommon | properties | on 3 objects (3 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    FireExit = TRUE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
  AC_Pset_Entrance_Door_16 | properties | on 1 object (1 IFCDOOR)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    3D Detail Level = "Detailed" (IFCLABEL)
    Bottom Frame Width Side 1 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Frame Width Side 2 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Centered Leaf = TRUE (IFCBOOLEAN)
    Custom Handle Name = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Middle Transom = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 2 = "" (IFCLABEL)
    Custom Panel Name Middle Transom = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name Transom Side 2 = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition Background Pen = "Transparent" (IFCLABEL)
    Demolition Fill Type = "" (IFCLABEL)
    Demolition Pen = "Transparent" (IFCLABEL)
    Demolition line type = 1 (IFCINTEGER)
    Display as Transom = FALSE (IFCBOOLEAN)
    Door Frame (gs_pocket_door_frame) = TRUE (IFCBOOLEAN)
    Door Panel Style (gs_door_typ) = "Style 1" (IFCLABEL)
    Door Panel Style (gs_door_typ_m) = 1 (IFCINTEGER)
    Door Stop Thickness = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Door Stop Width = 0.016 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Height = 2.068 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Width = 0.936 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Style (gs_frame_style) = "Style 3" (IFCLABEL)
    Frame Style (gs_frame_style_m) = 3 (IFCINTEGER)
    Frame Style Changed Automatically = FALSE (IFCBOOLEAN)
    Frame Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness Inside = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness=Wall Thickness = FALSE (IFCBOOLEAN)
    Frame Width = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 1 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Glass Thickness = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Height = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Position = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Middle Transom = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Leaf Frame Width Internal = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Left = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Lower = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Right = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Side = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Upper = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Height = 2.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width = 0.96 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaves Configuration (gs_LeavesConfig) = "Uniform Leaves" (IFCLABEL)
    Leaves Configuration (gs_iLeavesConfig) = 1 (IFCINTEGER)
    Left Sidelight = TRUE (IFCBOOLEAN)
    Middle Frame Width Side 1 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Middle Frame Width Side 2 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos_m) = 3 (IFCINTEGER)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    Mullion Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    New Background Pen = "Transparent" (IFCLABEL)
    New Fill Type = "" (IFCLABEL)
    New Pen = "Transparent" (IFCLABEL)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of Door Leaves - Side 2 = 3 (IFCINTEGER)
    Number of Door Leaves = 4 (IFCINTEGER)
    Opening Direction = 1 (IFCINTEGER)
    Opening Direction Leaf (gs_opening_dir) = "Default" (IFCLABEL)
    Opening Direction Leaf (gs_opening_dir_m) = 1 (IFCINTEGER)
    Opening Direction Sidelight (gs_opening_dir_sl) = "Flipped" (IFCLABEL)
    Opening Direction Sidelight (gs_opening_dir_sl_m) = 2 (IFCINTEGER)
    Opening Handle (gs_handle_type) = "None" (IFCLABEL)
    Opening Handle (gs_handle_type_m) = 0 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_05) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_06) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_09) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_10) = 1 (IFCINTEGER)
    Opening Type Middle Transom = "" (IFCLABEL)
    Opening Type Sidelight = "" (IFCLABEL)
    Opening Type Sidelight Side 1 = "" (IFCLABEL)
    Opening Type Transom Side 1 = "" (IFCLABEL)
    Opening Type Transom Side 2 = "" (IFCLABEL)
    Panes Number Horizontally 2 Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally = 3 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally Side 1 = 3 (IFCINTEGER)
    Panes Number Horizontally Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically Transom Side 2 = 2 (IFCINTEGER)
    Pivot Axis Offset = 0.275 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sidelight = FALSE (IFCBOOLEAN)
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_05) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_06) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_09) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_10) = 1 (IFCINTEGER)
    Sash Type Middle Transom = "" (IFCLABEL)
    Sash Type Sidelight Side 1 = "" (IFCLABEL)
    Sash Type Sidelight Side 2 = "" (IFCLABEL)
    Sash Type Transom Side 1 = "" (IFCLABEL)
    Sash Type Transom Side 2 = "" (IFCLABEL)
    Set Egress Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Leaf Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Shoulder Height = 2.074 (IFCLENGTHMEASURE) [MILLI METRE]
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Chinese Spring Door Symbol = FALSE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Editable Hotspots = TRUE (IFCBOOLEAN)
    Show Handle on Symbol = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show Symbol as Airtight Panel = FALSE (IFCBOOLEAN)
    Show as Glass Panel on Symbol = FALSE (IFCBOOLEAN)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Side 1 Width = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight (gs_SidelightTransomRelation) = "Under Transom" (IFCLABEL)
    Sidelight (gs_SidelightTransomRelation_m) = 1 (IFCINTEGER)
    Sidelight Division Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Division Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Frame Width = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Width (gs_sidelight_width_right_half) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Frame Thickness = 0.044 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Depth = 0.018 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 1 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 2 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_frame_width_transom) = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_sash_width) = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Uniform Frame Thickness = TRUE (IFCBOOLEAN)
    Uniform Frame Width = TRUE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Uniform Tolerances = TRUE (IFCBOOLEAN)
    Unit Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Entrance_Door_16 | properties | on 1 object (1 IFCDOOR)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    3D Detail Level = "Detailed" (IFCLABEL)
    Bottom Frame Width Side 1 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Frame Width Side 2 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Centered Leaf = TRUE (IFCBOOLEAN)
    Custom Handle Name = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Middle Transom = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 2 = "" (IFCLABEL)
    Custom Panel Name Middle Transom = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name Transom Side 2 = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition Background Pen = "Transparent" (IFCLABEL)
    Demolition Fill Type = "" (IFCLABEL)
    Demolition Pen = "Transparent" (IFCLABEL)
    Demolition line type = 1 (IFCINTEGER)
    Display as Transom = FALSE (IFCBOOLEAN)
    Door Frame (gs_pocket_door_frame) = TRUE (IFCBOOLEAN)
    Door Panel Style (gs_door_typ) = "Style 1" (IFCLABEL)
    Door Panel Style (gs_door_typ_m) = 1 (IFCINTEGER)
    Door Stop Thickness = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Door Stop Width = 0.016 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Height = 2.068 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Width = 0.936 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Style (gs_frame_style) = "Style 3" (IFCLABEL)
    Frame Style (gs_frame_style_m) = 3 (IFCINTEGER)
    Frame Style Changed Automatically = FALSE (IFCBOOLEAN)
    Frame Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness Inside = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness=Wall Thickness = FALSE (IFCBOOLEAN)
    Frame Width = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 1 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Glass Thickness = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Height = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Position = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Middle Transom = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Leaf Frame Width Internal = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Left = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Lower = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Right = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Side = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Upper = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Height = 2.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width = 0.96 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaves Configuration (gs_LeavesConfig) = "Uniform Leaves" (IFCLABEL)
    Leaves Configuration (gs_iLeavesConfig) = 1 (IFCINTEGER)
    Left Sidelight = TRUE (IFCBOOLEAN)
    Middle Frame Width Side 1 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Middle Frame Width Side 2 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos_m) = 3 (IFCINTEGER)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    Mullion Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    New Background Pen = "Transparent" (IFCLABEL)
    New Fill Type = "" (IFCLABEL)
    New Pen = "Transparent" (IFCLABEL)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of Door Leaves - Side 2 = 3 (IFCINTEGER)
    Number of Door Leaves = 4 (IFCINTEGER)
    Opening Direction = 1 (IFCINTEGER)
    Opening Direction Leaf (gs_opening_dir) = "Default" (IFCLABEL)
    Opening Direction Leaf (gs_opening_dir_m) = 1 (IFCINTEGER)
    Opening Direction Sidelight (gs_opening_dir_sl) = "Flipped" (IFCLABEL)
    Opening Direction Sidelight (gs_opening_dir_sl_m) = 2 (IFCINTEGER)
    Opening Handle (gs_handle_type) = "None" (IFCLABEL)
    Opening Handle (gs_handle_type_m) = 0 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_05) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_06) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_09) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_10) = 1 (IFCINTEGER)
    Opening Type Middle Transom = "" (IFCLABEL)
    Opening Type Sidelight = "" (IFCLABEL)
    Opening Type Sidelight Side 1 = "" (IFCLABEL)
    Opening Type Transom Side 1 = "" (IFCLABEL)
    Opening Type Transom Side 2 = "" (IFCLABEL)
    Panes Number Horizontally 2 Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally = 3 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally Side 1 = 3 (IFCINTEGER)
    Panes Number Horizontally Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically Transom Side 2 = 2 (IFCINTEGER)
    Pivot Axis Offset = 0.275 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sidelight = FALSE (IFCBOOLEAN)
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_05) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_06) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_09) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_10) = 1 (IFCINTEGER)
    Sash Type Middle Transom = "" (IFCLABEL)
    Sash Type Sidelight Side 1 = "" (IFCLABEL)
    Sash Type Sidelight Side 2 = "" (IFCLABEL)
    Sash Type Transom Side 1 = "" (IFCLABEL)
    Sash Type Transom Side 2 = "" (IFCLABEL)
    Set Egress Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Leaf Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Shoulder Height = 2.074 (IFCLENGTHMEASURE) [MILLI METRE]
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Chinese Spring Door Symbol = FALSE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Editable Hotspots = TRUE (IFCBOOLEAN)
    Show Handle on Symbol = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show Symbol as Airtight Panel = FALSE (IFCBOOLEAN)
    Show as Glass Panel on Symbol = FALSE (IFCBOOLEAN)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Side 1 Width = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight (gs_SidelightTransomRelation) = "Under Transom" (IFCLABEL)
    Sidelight (gs_SidelightTransomRelation_m) = 1 (IFCINTEGER)
    Sidelight Division Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Division Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Frame Width = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Width (gs_sidelight_width_right_half) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Frame Thickness = 0.044 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Depth = 0.018 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 1 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 2 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_frame_width_transom) = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_sash_width) = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Uniform Frame Thickness = TRUE (IFCBOOLEAN)
    Uniform Frame Width = TRUE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Uniform Tolerances = TRUE (IFCBOOLEAN)
    Unit Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 1 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Metal_Door_16 | properties | on 4 objects (4 IFCDOOR)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    3D Detail Level = "Detailed" (IFCLABEL)
    Bottom Frame Width Side 1 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Frame Width Side 2 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Centered Leaf = TRUE (IFCBOOLEAN)
    Custom Handle Name = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Middle Transom = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 2 = "" (IFCLABEL)
    Custom Panel Name Middle Transom = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name Transom Side 2 = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition Background Pen = "Transparent" (IFCLABEL)
    Demolition Fill Type = "" (IFCLABEL)
    Demolition Pen = "Transparent" (IFCLABEL)
    Demolition line type = 1 (IFCINTEGER)
    Display as Transom = FALSE (IFCBOOLEAN)
    Door Frame (gs_pocket_door_frame) = TRUE (IFCBOOLEAN)
    Door Panel Style (gs_door_typ) = "Style 1" (IFCLABEL)
    Door Panel Style (gs_door_typ_m) = 1 (IFCINTEGER)
    Door Stop Thickness = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Door Stop Width = 0.016 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Height = 2.068 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Width = 0.936 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Style (gs_frame_style) = "Style 3" (IFCLABEL)
    Frame Style (gs_frame_style_m) = 3 (IFCINTEGER)
    Frame Style Changed Automatically = FALSE (IFCBOOLEAN)
    Frame Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness Inside = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness=Wall Thickness = FALSE (IFCBOOLEAN)
    Frame Width = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 1 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Glass Thickness = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Height = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Position = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Middle Transom = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Leaf Frame Width Internal = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Left = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Lower = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Right = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Side = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Upper = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Height = 2.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width = 0.96 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaves Configuration (gs_LeavesConfig) = "Uniform Leaves" (IFCLABEL)
    Leaves Configuration (gs_iLeavesConfig) = 1 (IFCINTEGER)
    Left Sidelight = TRUE (IFCBOOLEAN)
    Middle Frame Width Side 1 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Middle Frame Width Side 2 = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos_m) = 3 (IFCINTEGER)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    Mullion Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    New Background Pen = "Transparent" (IFCLABEL)
    New Fill Type = "" (IFCLABEL)
    New Pen = "Transparent" (IFCLABEL)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of Door Leaves - Side 2 = 3 (IFCINTEGER)
    Number of Door Leaves = 4 (IFCINTEGER)
    Opening Direction = 1 (IFCINTEGER)
    Opening Direction Leaf (gs_opening_dir) = "Default" (IFCLABEL)
    Opening Direction Leaf (gs_opening_dir_m) = 1 (IFCINTEGER)
    Opening Direction Sidelight (gs_opening_dir_sl) = "Flipped" (IFCLABEL)
    Opening Direction Sidelight (gs_opening_dir_sl_m) = 2 (IFCINTEGER)
    Opening Handle (gs_handle_type) = "None" (IFCLABEL)
    Opening Handle (gs_handle_type_m) = 0 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_05) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_06) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_09) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_10) = 1 (IFCINTEGER)
    Opening Type Middle Transom = "" (IFCLABEL)
    Opening Type Sidelight = "" (IFCLABEL)
    Opening Type Sidelight Side 1 = "" (IFCLABEL)
    Opening Type Transom Side 1 = "" (IFCLABEL)
    Opening Type Transom Side 2 = "" (IFCLABEL)
    Panes Number Horizontally 2 Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally = 3 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally Side 1 = 3 (IFCINTEGER)
    Panes Number Horizontally Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically Transom Side 2 = 2 (IFCINTEGER)
    Pivot Axis Offset = 0.275 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sidelight = FALSE (IFCBOOLEAN)
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_05) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_06) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_09) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_10) = 1 (IFCINTEGER)
    Sash Type Middle Transom = "" (IFCLABEL)
    Sash Type Sidelight Side 1 = "" (IFCLABEL)
    Sash Type Sidelight Side 2 = "" (IFCLABEL)
    Sash Type Transom Side 1 = "" (IFCLABEL)
    Sash Type Transom Side 2 = "" (IFCLABEL)
    Set Egress Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Leaf Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Shoulder Height = 2.074 (IFCLENGTHMEASURE) [MILLI METRE]
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Chinese Spring Door Symbol = FALSE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Editable Hotspots = TRUE (IFCBOOLEAN)
    Show Handle on Symbol = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show Symbol as Airtight Panel = FALSE (IFCBOOLEAN)
    Show as Glass Panel on Symbol = FALSE (IFCBOOLEAN)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Side 1 Width = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight (gs_SidelightTransomRelation) = "Under Transom" (IFCLABEL)
    Sidelight (gs_SidelightTransomRelation_m) = 1 (IFCINTEGER)
    Sidelight Division Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Division Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Frame Width = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Width (gs_sidelight_width_right_half) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Frame Thickness = 0.044 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Depth = 0.018 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 1 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 2 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_frame_width_transom) = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_sash_width) = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Uniform Frame Thickness = TRUE (IFCBOOLEAN)
    Uniform Frame Width = TRUE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Uniform Tolerances = TRUE (IFCBOOLEAN)
    Unit Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 1 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Double_Door_with_Transom_16 | properties | on 2 objects (2 IFCDOOR)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    3D Detail Level = "Detailed" (IFCLABEL)
    Bottom Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Centered Leaf = TRUE (IFCBOOLEAN)
    Custom Handle Name = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name 2 Transom = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 2 = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name Transom = "" (IFCLABEL)
    Custom Panel Name Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name Transom Side 2 = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition Background Pen = "Transparent" (IFCLABEL)
    Demolition Fill Type = "" (IFCLABEL)
    Demolition Pen = "Transparent" (IFCLABEL)
    Demolition line type = 1 (IFCINTEGER)
    Display as Transom = FALSE (IFCBOOLEAN)
    Door Frame (gs_pocket_door_frame) = TRUE (IFCBOOLEAN)
    Door Panel Style (gs_door_typ) = "No Mullions" (IFCLABEL)
    Door Panel Style (gs_door_typ_m) = 46 (IFCINTEGER)
    Door Stop Thickness = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Door Stop Width = 0.016 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Height = 1.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Width = 1.32 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Style (gs_frame_style) = "Style 3" (IFCLABEL)
    Frame Style (gs_frame_style_m) = 3 (IFCINTEGER)
    Frame Style Changed Automatically = FALSE (IFCBOOLEAN)
    Frame Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness Inside = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness=Wall Thickness = FALSE (IFCBOOLEAN)
    Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Glass Thickness = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Height = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Position = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Sidelight Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Leaf Frame Width Internal = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Left = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Lower = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Right = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Side = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Upper = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Height = 1.812 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width = 1.344 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width Side 1 = 0.672 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaves Configuration (gs_LeavesConfig) = "Uniform Leaves" (IFCLABEL)
    Leaves Configuration (gs_iLeavesConfig) = 1 (IFCINTEGER)
    Left Sidelight = FALSE (IFCBOOLEAN)
    Middle Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Middle Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos_m) = 3 (IFCINTEGER)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    Mullion Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    New Background Pen = "Transparent" (IFCLABEL)
    New Fill Type = "" (IFCLABEL)
    New Pen = "Transparent" (IFCLABEL)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of Door Leaves - Side 2 = 3 (IFCINTEGER)
    Number of Door Leaves = 4 (IFCINTEGER)
    Opening Direction = 1 (IFCINTEGER)
    Opening Direction Leaf (gs_opening_dir) = "Default" (IFCLABEL)
    Opening Direction Leaf (gs_opening_dir_m) = 1 (IFCINTEGER)
    Opening Direction Sidelight (gs_opening_dir_sl) = "Flipped" (IFCLABEL)
    Opening Direction Sidelight (gs_opening_dir_sl_m) = 2 (IFCINTEGER)
    Opening Handle (gs_handle_type) = "None" (IFCLABEL)
    Opening Handle (gs_handle_type_m) = 0 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_05) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_06) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_09) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_10) = 1 (IFCINTEGER)
    Opening Type Sidelight Side 1 = "" (IFCLABEL)
    Opening Type Sidelight Side 2 = "" (IFCLABEL)
    Opening Type Transom = "Fixed Glass" (IFCLABEL)
    Opening Type Transom Side 1 = "" (IFCLABEL)
    Opening Type Transom Side 2 = "" (IFCLABEL)
    Panes Number Horizontally 2 Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Side 1 = 3 (IFCINTEGER)
    Panes Number Horizontally Side 2 = 3 (IFCINTEGER)
    Panes Number Horizontally Transom = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Transom = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically Transom = 2 (IFCINTEGER)
    Panes Number Vertically Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically Transom Side 2 = 2 (IFCINTEGER)
    Pivot Axis Offset = 0.275 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sidelight = FALSE (IFCBOOLEAN)
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_05) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_06) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_09) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_10) = 1 (IFCINTEGER)
    Sash Type Sidelight Side 1 = "" (IFCLABEL)
    Sash Type Sidelight Side 2 = "" (IFCLABEL)
    Sash Type Transom = "No Mullions" (IFCLABEL)
    Sash Type Transom Side 1 = "" (IFCLABEL)
    Sash Type Transom Side 2 = "" (IFCLABEL)
    Set Egress Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Leaf Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Shoulder Height = 2.07 (IFCLENGTHMEASURE) [MILLI METRE]
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Chinese Spring Door Symbol = FALSE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Editable Hotspots = TRUE (IFCBOOLEAN)
    Show Handle on Symbol = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show Symbol as Airtight Panel = FALSE (IFCBOOLEAN)
    Show as Glass Panel on Symbol = FALSE (IFCBOOLEAN)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Side 1 Width = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight (gs_SidelightTransomRelation) = "Under Transom" (IFCLABEL)
    Sidelight (gs_SidelightTransomRelation_m) = 1 (IFCINTEGER)
    Sidelight Division Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Division Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Frame Width = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Width (gs_sidelight_width_right_half) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Depth = 0.018 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 1 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 2 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Thickness = 0.044 (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_frame_width_transom) = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_sash_width) = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Uniform Frame Thickness = TRUE (IFCBOOLEAN)
    Uniform Frame Width = TRUE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Uniform Tolerances = TRUE (IFCBOOLEAN)
    Unit Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 1 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Door_16 | properties | on 14 objects (14 IFCDOOR)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    3D Detail Level = "Detailed" (IFCLABEL)
    Bottom Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Centered Leaf = TRUE (IFCBOOLEAN)
    Custom Handle Name = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Middle Transom = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 2 = "" (IFCLABEL)
    Custom Panel Name Middle Transom = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name Transom Side 2 = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition Background Pen = "Transparent" (IFCLABEL)
    Demolition Fill Type = "" (IFCLABEL)
    Demolition Pen = "Transparent" (IFCLABEL)
    Demolition line type = 1 (IFCINTEGER)
    Display as Transom = FALSE (IFCBOOLEAN)
    Door Frame (gs_pocket_door_frame) = TRUE (IFCBOOLEAN)
    Door Panel Style (gs_door_typ) = "No Mullions" (IFCLABEL)
    Door Panel Style (gs_door_typ_m) = 46 (IFCINTEGER)
    Door Stop Thickness = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Door Stop Width = 0.016 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Height = 2.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Width = 0.92 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Style (gs_frame_style) = "Style 3" (IFCLABEL)
    Frame Style (gs_frame_style_m) = 3 (IFCINTEGER)
    Frame Style Changed Automatically = FALSE (IFCBOOLEAN)
    Frame Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness Inside = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness=Wall Thickness = FALSE (IFCBOOLEAN)
    Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Glass Thickness = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Height = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Position = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Middle Transom = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Leaf Frame Width Internal = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Left = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Lower = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Right = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Side = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Upper = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Height = 2.072 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width = 0.944 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaves Configuration (gs_LeavesConfig) = "Uniform Leaves" (IFCLABEL)
    Leaves Configuration (gs_iLeavesConfig) = 1 (IFCINTEGER)
    Left Sidelight = FALSE (IFCBOOLEAN)
    Middle Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Middle Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos_m) = 3 (IFCINTEGER)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    Mullion Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    New Background Pen = "Transparent" (IFCLABEL)
    New Fill Type = "" (IFCLABEL)
    New Pen = "Transparent" (IFCLABEL)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of Door Leaves - Side 2 = 3 (IFCINTEGER)
    Number of Door Leaves = 4 (IFCINTEGER)
    Opening Direction = 1 (IFCINTEGER)
    Opening Direction Leaf (gs_opening_dir) = "Default" (IFCLABEL)
    Opening Direction Leaf (gs_opening_dir_m) = 1 (IFCINTEGER)
    Opening Direction Sidelight (gs_opening_dir_sl) = "Flipped" (IFCLABEL)
    Opening Direction Sidelight (gs_opening_dir_sl_m) = 2 (IFCINTEGER)
    Opening Handle (gs_handle_type) = "None" (IFCLABEL)
    Opening Handle (gs_handle_type_m) = 0 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_05) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_06) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_09) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_10) = 1 (IFCINTEGER)
    Opening Type Middle Transom = "" (IFCLABEL)
    Opening Type Sidelight Side 1 = "" (IFCLABEL)
    Opening Type Sidelight Side 2 = "" (IFCLABEL)
    Opening Type Transom Side 1 = "" (IFCLABEL)
    Opening Type Transom Side 2 = "" (IFCLABEL)
    Panes Number Horizontally 2 Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally = 3 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally Side 1 = 3 (IFCINTEGER)
    Panes Number Horizontally Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically Transom Side 2 = 2 (IFCINTEGER)
    Pivot Axis Offset = 0.275 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sidelight = FALSE (IFCBOOLEAN)
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_05) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_06) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_09) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_10) = 1 (IFCINTEGER)
    Sash Type Middle Transom = "" (IFCLABEL)
    Sash Type Sidelight Side 1 = "" (IFCLABEL)
    Sash Type Sidelight Side 2 = "" (IFCLABEL)
    Sash Type Transom Side 1 = "" (IFCLABEL)
    Sash Type Transom Side 2 = "" (IFCLABEL)
    Set Egress Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Leaf Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Shoulder Height = 1.84 (IFCLENGTHMEASURE) [MILLI METRE]
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Chinese Spring Door Symbol = FALSE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Editable Hotspots = TRUE (IFCBOOLEAN)
    Show Handle on Symbol = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show Symbol as Airtight Panel = FALSE (IFCBOOLEAN)
    Show as Glass Panel on Symbol = FALSE (IFCBOOLEAN)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Side 1 Width = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight (gs_SidelightTransomRelation) = "Under Transom" (IFCLABEL)
    Sidelight (gs_SidelightTransomRelation_m) = 1 (IFCINTEGER)
    Sidelight Division Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Division Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Frame Width = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Width (gs_sidelight_width_right_half) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Frame Thickness = 0.044 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Depth = 0.018 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 1 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 2 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_frame_width_transom) = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_sash_width) = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Uniform Frame Thickness = TRUE (IFCBOOLEAN)
    Uniform Frame Width = TRUE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Uniform Tolerances = TRUE (IFCBOOLEAN)
    Unit Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 2 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Door_16 | properties | on 10 objects (10 IFCDOOR)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    3D Detail Level = "Detailed" (IFCLABEL)
    Bottom Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Centered Leaf = TRUE (IFCBOOLEAN)
    Custom Handle Name = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Middle Transom = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 2 = "" (IFCLABEL)
    Custom Panel Name Middle Transom = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name Transom Side 2 = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition Background Pen = "Transparent" (IFCLABEL)
    Demolition Fill Type = "" (IFCLABEL)
    Demolition Pen = "Transparent" (IFCLABEL)
    Demolition line type = 1 (IFCINTEGER)
    Display as Transom = FALSE (IFCBOOLEAN)
    Door Frame (gs_pocket_door_frame) = TRUE (IFCBOOLEAN)
    Door Panel Style (gs_door_typ) = "No Mullions" (IFCLABEL)
    Door Panel Style (gs_door_typ_m) = 46 (IFCINTEGER)
    Door Stop Thickness = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Door Stop Width = 0.016 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Height = 2.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Width = 0.92 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Style (gs_frame_style) = "Style 3" (IFCLABEL)
    Frame Style (gs_frame_style_m) = 3 (IFCINTEGER)
    Frame Style Changed Automatically = FALSE (IFCBOOLEAN)
    Frame Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness Inside = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness=Wall Thickness = FALSE (IFCBOOLEAN)
    Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Glass Thickness = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Height = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Position = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Middle Transom = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Leaf Frame Width Internal = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Left = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Lower = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Right = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Side = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Upper = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Height = 2.072 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width = 0.944 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaves Configuration (gs_LeavesConfig) = "Uniform Leaves" (IFCLABEL)
    Leaves Configuration (gs_iLeavesConfig) = 1 (IFCINTEGER)
    Left Sidelight = FALSE (IFCBOOLEAN)
    Middle Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Middle Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos_m) = 3 (IFCINTEGER)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    Mullion Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    New Background Pen = "Transparent" (IFCLABEL)
    New Fill Type = "" (IFCLABEL)
    New Pen = "Transparent" (IFCLABEL)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of Door Leaves - Side 2 = 3 (IFCINTEGER)
    Number of Door Leaves = 4 (IFCINTEGER)
    Opening Direction = 1 (IFCINTEGER)
    Opening Direction Leaf (gs_opening_dir) = "Default" (IFCLABEL)
    Opening Direction Leaf (gs_opening_dir_m) = 1 (IFCINTEGER)
    Opening Direction Sidelight (gs_opening_dir_sl) = "Flipped" (IFCLABEL)
    Opening Direction Sidelight (gs_opening_dir_sl_m) = 2 (IFCINTEGER)
    Opening Handle (gs_handle_type) = "None" (IFCLABEL)
    Opening Handle (gs_handle_type_m) = 0 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_05) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_06) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_09) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_10) = 1 (IFCINTEGER)
    Opening Type Middle Transom = "" (IFCLABEL)
    Opening Type Sidelight Side 1 = "" (IFCLABEL)
    Opening Type Sidelight Side 2 = "" (IFCLABEL)
    Opening Type Transom Side 1 = "" (IFCLABEL)
    Opening Type Transom Side 2 = "" (IFCLABEL)
    Panes Number Horizontally 2 Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally = 3 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally Side 1 = 3 (IFCINTEGER)
    Panes Number Horizontally Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically Transom Side 2 = 2 (IFCINTEGER)
    Pivot Axis Offset = 0.275 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sidelight = FALSE (IFCBOOLEAN)
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_05) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_06) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_09) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_10) = 1 (IFCINTEGER)
    Sash Type Middle Transom = "" (IFCLABEL)
    Sash Type Sidelight Side 1 = "" (IFCLABEL)
    Sash Type Sidelight Side 2 = "" (IFCLABEL)
    Sash Type Transom Side 1 = "" (IFCLABEL)
    Sash Type Transom Side 2 = "" (IFCLABEL)
    Set Egress Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Leaf Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Shoulder Height = 1.84 (IFCLENGTHMEASURE) [MILLI METRE]
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Chinese Spring Door Symbol = FALSE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Editable Hotspots = TRUE (IFCBOOLEAN)
    Show Handle on Symbol = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show Symbol as Airtight Panel = FALSE (IFCBOOLEAN)
    Show as Glass Panel on Symbol = FALSE (IFCBOOLEAN)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Side 1 Width = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight (gs_SidelightTransomRelation) = "Under Transom" (IFCLABEL)
    Sidelight (gs_SidelightTransomRelation_m) = 1 (IFCINTEGER)
    Sidelight Division Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Division Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Frame Width = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Width (gs_sidelight_width_right_half) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Frame Thickness = 0.044 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Depth = 0.018 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 1 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 2 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_frame_width_transom) = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_sash_width) = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Uniform Frame Thickness = TRUE (IFCBOOLEAN)
    Uniform Frame Width = TRUE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Uniform Tolerances = TRUE (IFCBOOLEAN)
    Unit Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Door_16 | properties | on 1 object (1 IFCDOOR)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    3D Detail Level = "Detailed" (IFCLABEL)
    Bottom Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Centered Leaf = TRUE (IFCBOOLEAN)
    Custom Handle Name = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Middle Transom = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 2 = "" (IFCLABEL)
    Custom Panel Name Middle Transom = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name Transom Side 2 = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition Background Pen = "Transparent" (IFCLABEL)
    Demolition Fill Type = "" (IFCLABEL)
    Demolition Pen = "Transparent" (IFCLABEL)
    Demolition line type = 1 (IFCINTEGER)
    Display as Transom = FALSE (IFCBOOLEAN)
    Door Frame (gs_pocket_door_frame) = TRUE (IFCBOOLEAN)
    Door Panel Style (gs_door_typ) = "No Mullions" (IFCLABEL)
    Door Panel Style (gs_door_typ_m) = 46 (IFCINTEGER)
    Door Stop Thickness = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Door Stop Width = 0.016 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Height = 2.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Width = 0.92 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Style (gs_frame_style) = "Style 3" (IFCLABEL)
    Frame Style (gs_frame_style_m) = 3 (IFCINTEGER)
    Frame Style Changed Automatically = FALSE (IFCBOOLEAN)
    Frame Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness Inside = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness=Wall Thickness = FALSE (IFCBOOLEAN)
    Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Glass Thickness = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Height = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Position = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Middle Transom = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Leaf Frame Width Internal = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Left = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Lower = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Right = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Side = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Upper = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Height = 2.072 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width = 0.944 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaves Configuration (gs_LeavesConfig) = "Uniform Leaves" (IFCLABEL)
    Leaves Configuration (gs_iLeavesConfig) = 1 (IFCINTEGER)
    Left Sidelight = FALSE (IFCBOOLEAN)
    Middle Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Middle Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos_m) = 3 (IFCINTEGER)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    Mullion Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    New Background Pen = "Transparent" (IFCLABEL)
    New Fill Type = "" (IFCLABEL)
    New Pen = "Transparent" (IFCLABEL)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of Door Leaves - Side 2 = 3 (IFCINTEGER)
    Number of Door Leaves = 4 (IFCINTEGER)
    Opening Direction = 1 (IFCINTEGER)
    Opening Direction Leaf (gs_opening_dir) = "Default" (IFCLABEL)
    Opening Direction Leaf (gs_opening_dir_m) = 1 (IFCINTEGER)
    Opening Direction Sidelight (gs_opening_dir_sl) = "Flipped" (IFCLABEL)
    Opening Direction Sidelight (gs_opening_dir_sl_m) = 2 (IFCINTEGER)
    Opening Handle (gs_handle_type) = "None" (IFCLABEL)
    Opening Handle (gs_handle_type_m) = 0 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_05) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_06) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_09) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_10) = 1 (IFCINTEGER)
    Opening Type Middle Transom = "" (IFCLABEL)
    Opening Type Sidelight Side 1 = "" (IFCLABEL)
    Opening Type Sidelight Side 2 = "" (IFCLABEL)
    Opening Type Transom Side 1 = "" (IFCLABEL)
    Opening Type Transom Side 2 = "" (IFCLABEL)
    Panes Number Horizontally 2 Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally = 3 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally Side 1 = 3 (IFCINTEGER)
    Panes Number Horizontally Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically Transom Side 2 = 2 (IFCINTEGER)
    Pivot Axis Offset = 0.275 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sidelight = FALSE (IFCBOOLEAN)
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_05) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_06) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_09) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_10) = 1 (IFCINTEGER)
    Sash Type Middle Transom = "" (IFCLABEL)
    Sash Type Sidelight Side 1 = "" (IFCLABEL)
    Sash Type Sidelight Side 2 = "" (IFCLABEL)
    Sash Type Transom Side 1 = "" (IFCLABEL)
    Sash Type Transom Side 2 = "" (IFCLABEL)
    Set Egress Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Leaf Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Shoulder Height = 1.84 (IFCLENGTHMEASURE) [MILLI METRE]
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Chinese Spring Door Symbol = FALSE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Editable Hotspots = TRUE (IFCBOOLEAN)
    Show Handle on Symbol = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show Symbol as Airtight Panel = FALSE (IFCBOOLEAN)
    Show as Glass Panel on Symbol = FALSE (IFCBOOLEAN)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Side 1 Width = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight (gs_SidelightTransomRelation) = "Under Transom" (IFCLABEL)
    Sidelight (gs_SidelightTransomRelation_m) = 1 (IFCINTEGER)
    Sidelight Division Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Division Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Frame Width = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Width (gs_sidelight_width_right_half) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Frame Thickness = 0.044 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Depth = 0.018 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 1 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 2 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_frame_width_transom) = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_sash_width) = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Uniform Frame Thickness = TRUE (IFCBOOLEAN)
    Uniform Frame Width = TRUE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Uniform Tolerances = TRUE (IFCBOOLEAN)
    Unit Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 1 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Sliding_Door_16 | properties | on 3 objects (3 IFCDOOR)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    3D Detail Level = "Detailed" (IFCLABEL)
    Bottom Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Centered Leaf = TRUE (IFCBOOLEAN)
    Custom Handle Name = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel_00) = "" (IFCLABEL)
    Custom Panel Name 2 Middle Transom = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name 2 Transom Side 2 = "" (IFCLABEL)
    Custom Panel Name Middle Transom = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 1 = "" (IFCLABEL)
    Custom Panel Name Sidelight Side 2 = "" (IFCLABEL)
    Custom Panel Name Transom Side 1 = "" (IFCLABEL)
    Custom Panel Name Transom Side 2 = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition Background Pen = "Transparent" (IFCLABEL)
    Demolition Fill Type = "" (IFCLABEL)
    Demolition Pen = "Transparent" (IFCLABEL)
    Demolition line type = 1 (IFCINTEGER)
    Display as Transom = FALSE (IFCBOOLEAN)
    Door Frame (gs_pocket_door_frame) = TRUE (IFCBOOLEAN)
    Door Panel Style (gs_door_typ) = "No Mullions" (IFCLABEL)
    Door Panel Style (gs_door_typ_m) = 46 (IFCINTEGER)
    Door Stop Thickness = 0.032 (IFCLENGTHMEASURE) [MILLI METRE]
    Door Stop Width = 0.016 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Height = 2.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Width = 0.46 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Style (gs_frame_style) = "Style 1" (IFCLABEL)
    Frame Style (gs_frame_style_m) = 1 (IFCINTEGER)
    Frame Style Changed Automatically = FALSE (IFCBOOLEAN)
    Frame Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness Inside = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness=Wall Thickness = FALSE (IFCBOOLEAN)
    Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Side 2 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Glass Thickness = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Grill Width = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Height = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Position = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Division Height Middle Transom = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Sidelight Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Division Height Transom Side 2 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspot Grill Editing = TRUE (IFCBOOLEAN)
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Leaf Frame Width Internal = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Left = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Lower = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Right = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Side = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Upper = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Height = 2.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width = 0.92 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width Side 1 = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaves Configuration (gs_LeavesConfig) = "Uniform Leaves" (IFCLABEL)
    Leaves Configuration (gs_iLeavesConfig) = 1 (IFCINTEGER)
    Left Sidelight = TRUE (IFCBOOLEAN)
    Middle Frame Width Side 1 = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Middle Frame Width Side 2 = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Position (MullionPosition) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos) = "Throughout" (IFCLABEL)
    Mullion Position (gs_grill_pos_m) = 3 (IFCINTEGER)
    Mullion Position (iMullionPosition) = 3 (IFCINTEGER)
    Mullion Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Mullion Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    New Background Pen = "Transparent" (IFCLABEL)
    New Fill Type = "" (IFCLABEL)
    New Pen = "Transparent" (IFCLABEL)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of Door Leaves - Side 2 = 3 (IFCINTEGER)
    Number of Door Leaves = 4 (IFCINTEGER)
    Opening Direction = 1 (IFCINTEGER)
    Opening Direction Leaf (gs_opening_dir) = "Default" (IFCLABEL)
    Opening Direction Leaf (gs_opening_dir_m) = 1 (IFCINTEGER)
    Opening Direction Sidelight (gs_opening_dir_sl) = "Flipped" (IFCLABEL)
    Opening Direction Sidelight (gs_opening_dir_sl_m) = 2 (IFCINTEGER)
    Opening Handle (gs_handle_type) = "None" (IFCLABEL)
    Opening Handle (gs_handle_type_m) = 0 (IFCINTEGER)
    Opening Type (gs_optype_m_02) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_05) = 3 (IFCINTEGER)
    Opening Type (gs_optype_m_06) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_09) = 1 (IFCINTEGER)
    Opening Type (gs_optype_m_10) = 1 (IFCINTEGER)
    Opening Type Middle Transom = "" (IFCLABEL)
    Opening Type Sidelight = "" (IFCLABEL)
    Opening Type Sidelight Side 1 = "" (IFCLABEL)
    Opening Type Transom Side 1 = "" (IFCLABEL)
    Opening Type Transom Side 2 = "" (IFCLABEL)
    Panes Number Horizontally 2 Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally = 3 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Main Sash Side 2 = 2 (IFCINTEGER)
    Panes Number Horizontally Middle Transom = 2 (IFCINTEGER)
    Panes Number Horizontally Side 1 = 3 (IFCINTEGER)
    Panes Number Horizontally Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Horizontally Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically 2 Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically 2 Transom Side 2 = 2 (IFCINTEGER)
    Panes Number Vertically = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Main Sash Side 2 = 4 (IFCINTEGER)
    Panes Number Vertically Middle Transom = 2 (IFCINTEGER)
    Panes Number Vertically Side 1 = 4 (IFCINTEGER)
    Panes Number Vertically Transom Side 1 = 2 (IFCINTEGER)
    Panes Number Vertically Transom Side 2 = 2 (IFCINTEGER)
    Pivot Axis Offset = 0.275 (IFCLENGTHMEASURE) [MILLI METRE]
    Rebate Width = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sidelight = FALSE (IFCBOOLEAN)
    Sash Type (MullionStyle_00) = "No Mullions" (IFCLABEL)
    Sash Type (iMullionStyle_00) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_02) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_05) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_06) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_09) = 1 (IFCINTEGER)
    Sash Type (iMullionStyle_10) = 1 (IFCINTEGER)
    Sash Type Middle Transom = "" (IFCLABEL)
    Sash Type Sidelight Side 1 = "" (IFCLABEL)
    Sash Type Sidelight Side 2 = "" (IFCLABEL)
    Sash Type Transom Side 1 = "" (IFCLABEL)
    Sash Type Transom Side 2 = "" (IFCLABEL)
    Set Egress Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Leaf Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Shoulder Height = 2.07 (IFCLENGTHMEASURE) [MILLI METRE]
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Chinese Spring Door Symbol = FALSE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Editable Hotspots = TRUE (IFCBOOLEAN)
    Show Handle on Symbol = FALSE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show Symbol as Airtight Panel = FALSE (IFCBOOLEAN)
    Show as Glass Panel on Symbol = FALSE (IFCBOOLEAN)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Side 1 Width = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight (gs_SidelightTransomRelation) = "Under Transom" (IFCLABEL)
    Sidelight (gs_SidelightTransomRelation_m) = 1 (IFCINTEGER)
    Sidelight Division Thickness = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Division Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Frame Width = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Width (gs_sidelight_width_right_half) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Frame Thickness = 0.044 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Depth = 0.018 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight and Transom Rebate Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 1 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Side 2 Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 1 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Sidelight 2 Bottom = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_frame_width_transom) = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Frame Width (gs_sash_width) = 0.067 (IFCLENGTHMEASURE) [MILLI METRE]
    Uniform Frame Thickness = TRUE (IFCBOOLEAN)
    Uniform Frame Width = TRUE (IFCBOOLEAN)
    Uniform Sashes = FALSE (IFCBOOLEAN)
    Uniform Tolerances = TRUE (IFCBOOLEAN)
    Unit Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 1 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Revolving_Door_16 | properties | on 1 object (1 IFCDOOR)
    3D Closed Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    3D Closed Length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    3D Opening Angle = 180. (IFCREAL)
    3D Opening Height = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    3D Opening Length 1 = 0.56 (IFCLENGTHMEASURE) [MILLI METRE]
    3D Opening Length 2 = 0.14 (IFCLENGTHMEASURE) [MILLI METRE]
    3D Opening Length = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Automatic Shutter Height = TRUE (IFCBOOLEAN)
    Automatic Shutter Width = TRUE (IFCBOOLEAN)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Box Default Width (gs_shutRoll_boxDefaultSize) = "Reveal Width" (IFCLABEL)
    Box Default Width (gs_shutRoll_iBoxDefaultSize) = 1 (IFCINTEGER)
    Box Depth (gs_shutLam_boxWidth) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Box Depth (gs_shutRoll_boxWidth) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Box Height (gs_shutLam_boxHeight) = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Box Height (gs_shutRoll_boxHeight) = 0.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Box Left Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Box Right Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Box Top Angle = 10. (IFCREAL)
    Box Type (gs_shutRoll_boxType) = "Rectangular" (IFCLABEL)
    Box Type (gs_shutRoll_iBoxType) = 1 (IFCINTEGER)
    Brick Sill 3D Detail Level = "Simple" (IFCLABEL)
    Brick Thickness (gs_brick_sill_br_thk) = 0.065 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Type Inside = "" (IFCLABEL)
    Casing Type Outside = "" (IFCLABEL)
    Casing Width Inside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Casing Width Outside = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Closing Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Cover Type (gs_slidingShutter_cover) = "Z-Profile" (IFCLABEL)
    Cover Type (gs_slidingShutter_iCover) = 1 (IFCINTEGER)
    Custom Panel Name (gs_cust_panel) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_shutterPanel) = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition Background Pen = "Transparent" (IFCLABEL)
    Demolition Fill Type = "" (IFCLABEL)
    Demolition Pen = "Transparent" (IFCLABEL)
    Demolition line type = 1 (IFCINTEGER)
    Depth of Rails = 0.0725 (IFCLENGTHMEASURE) [MILLI METRE]
    Different Bottom Frame Width = FALSE (IFCBOOLEAN)
    Display as Transom = FALSE (IFCBOOLEAN)
    Distance from Header (gs_shutRoll_distFromHead) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Distance from Wall (gs_shutRoll_distFromWall) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Door Sill = FALSE (IFCBOOLEAN)
    Door Sill Type = "Off" (IFCLABEL)
    Egress Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Width = 1.068 (IFCLENGTHMEASURE) [MILLI METRE]
    Enabled Sunshade Types = 0 (IFCINTEGER)
    Extra Frame = FALSE (IFCBOOLEAN)
    Extra Frame Thickness = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Extra Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Style Changed Automatically = FALSE (IFCBOOLEAN)
    Frame Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness=Wall Thickness = FALSE (IFCBOOLEAN)
    Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Bottom = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Left = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Right = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Width Upper = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Fully Editable = TRUE (IFCBOOLEAN)
    Hanging Stick Length = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Hanging Stick Radius = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 11.481088 (IFCREAL)
    Hole Radius = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Resolution = 3 (IFCINTEGER)
    Holes Number Horizontal = 5 (IFCINTEGER)
    Holes Number Vertical = 8 (IFCINTEGER)
    Horizontal Boards Approximate Width = 0.115 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Boards Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Frame Divider Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Inner Offset = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Inner Panel Width = 0.12 (IFCLENGTHMEASURE) [MILLI METRE]
    Insulation behind Box (gs_shutLam_cutWallBehind) = FALSE (IFCBOOLEAN)
    Insulation behind Box (gs_shutRoll_cutWallBehind) = FALSE (IFCBOOLEAN)
    Leaf Frame Width Left = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Right = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Height = 2.112 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width = 1.092 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Sidelight = TRUE (IFCBOOLEAN)
    Louver Angle = 30. (IFCREAL)
    Louver Thickness = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Louver Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 0.015 (IFCLENGTHMEASURE) [MILLI METRE]
    New Background Pen = "Transparent" (IFCLABEL)
    New Fill Type = "" (IFCLABEL)
    New Pen = "Transparent" (IFCLABEL)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number of Panels 2 = 1 (IFCINTEGER)
    Number of Panels = 2 (IFCINTEGER)
    Open in 3D = TRUE (IFCBOOLEAN)
    Opened Box = TRUE (IFCBOOLEAN)
    Opening Direction = -1 (IFCINTEGER)
    Opening Direction Leaf = "Inside" (IFCLABEL)
    Opening Side in Curved Wall = "Parallel" (IFCLABEL)
    Outside Overhang = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Distance = 0.006 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Fill Thickness = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Height = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Position (gs_shutter_iPanelPos) = 1 (IFCINTEGER)
    Panel Position (gs_shutter_panelPos) = "Symmetric" (IFCLABEL)
    Panel Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Panel Type (gs_shutPanel_iType) = 1 (IFCINTEGER)
    Panel Type (gs_shutPanel_type) = "Style 1" (IFCLABEL)
    Panel Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Rail = TRUE (IFCBOOLEAN)
    Rail Position (gs_shutRoll_iRailPos) = 1 (IFCINTEGER)
    Rail Position (gs_shutRoll_railPos) = "On Casing" (IFCLABEL)
    Rail Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Height = 2.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Width = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Right Sidelight = FALSE (IFCBOOLEAN)
    Rolling Shutter Placement (gs_shutRoll_iPlacement) = 1 (IFCINTEGER)
    Rolling Shutter Placement (gs_shutRoll_placement) = "On Facade" (IFCLABEL)
    Set Egress Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Leaf Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show 2D Symbol = TRUE (IFCBOOLEAN)
    Show Casing behind Sunshade (gs_shutRoll_showCasingBehind) = FALSE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Opening Lines on Symbol = FALSE (IFCBOOLEAN)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sidelight Width Left = 0.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Width Right = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Angle = 10. (IFCREAL)
    Sill Front Side Thickness = 0.07 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Nosing = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Overhang Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Slip-in Depth = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Style Changed Automatically = FALSE (IFCBOOLEAN)
    Sill Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Height = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Top Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Type Enable Mask = 0 (IFCINTEGER)
    Slat Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Stacking Direction (gs_foldingShutter_iStacking) = 1 (IFCINTEGER)
    Stacking Direction (gs_foldingShutter_stacking) = "Inside" (IFCLABEL)
    Sunshade Type (gs_sunShade_iType) = -1 (IFCINTEGER)
    Sunshade Type (gs_sunShade_type) = "" (IFCLABEL)
    Threshold = "Off" (IFCLABEL)
    Threshold Angle = 3.1995974 (IFCREAL)
    Threshold Changed Automatically = FALSE (IFCBOOLEAN)
    Threshold External Thickness = 0.0058073777 (IFCLENGTHMEASURE) [MILLI METRE]
    Threshold Nosing Inside = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Threshold Nosing Outside = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Threshold Thickness = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Threshold Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Diameter = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Transom = TRUE (IFCBOOLEAN)
    Transom Height = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Trim = "Off" (IFCLABEL)
    Trim Offset Inside = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Offset Outside = 0.012 (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Thickness Inside = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Thickness Outside = 0.005 (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Width Left Inside = 0.075 (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Width Left Outside = 0.075 (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Width Right Inside = 0.075 (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Width Right Outside = 0.075 (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Width Top Inside = 0.075 (IFCLENGTHMEASURE) [MILLI METRE]
    Trim Width Top Outside = 0.075 (IFCLENGTHMEASURE) [MILLI METRE]
    Uniform Frame Width = TRUE (IFCBOOLEAN)
    Unit Height = 2.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Width = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Venetian Blinds Placement (gs_shutLam_iPlacement) = 1 (IFCINTEGER)
    Venetian Blinds Placement (gs_shutLam_placement) = "Fixed on Facade" (IFCLABEL)
    Vertical Board Width = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Boards Approximate Width = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Boards Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Frame Divider Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 2.25 (IFCLENGTHMEASURE) [MILLI METRE]
    Width of Sill = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Frame Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Z Frame Width = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
  AC_Pset_Railing_Horizontal | properties | on 2 objects (2 IFCRAILING)
    3D = "Detailed" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Axis Line Type = 6 (IFCINTEGER)
    Bar Material = "Zinc" (IFCLABEL)
    Bar Position = "on Posts" (IFCLABEL)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Contour Pen = "" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Cross Section Resolution = 6 (IFCINTEGER)
    Fill Background Pen = "" (IFCLABEL)
    Fill Pen = "" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Group Type = "Others" (IFCLABEL)
    Handrail Diameter = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Material = "Zinc" (IFCLABEL)
    Handrail Overhang (Left) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Overhang (Right) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Overhang = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Radius = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Width = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Horiz. Bar Diameter = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Inventory No. = "" (IFCLABEL)
    Left End Cutting Angle = 90. (IFCREAL)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    No. of Bars (0-None) = 4 (IFCINTEGER)
    No. of Posts (0-None) = 3 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Post Depth = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Post Material = "Zinc" (IFCLABEL)
    Post Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Production Year = "" (IFCLABEL)
    Railing Length = 4.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Right End Cutting Angle = 90. (IFCREAL)
    Serial No. = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Show Axis = FALSE (IFCBOOLEAN)
    Show Posts in 2D = TRUE (IFCBOOLEAN)
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
  AC_Pset_Railing_Horizontal | properties | on 2 objects (2 IFCRAILING)
    3D = "Detailed" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Axis Line Type = 6 (IFCINTEGER)
    Bar Material = "Zinc" (IFCLABEL)
    Bar Position = "on Posts" (IFCLABEL)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Contour Pen = "" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Cross Section Resolution = 6 (IFCINTEGER)
    Fill Background Pen = "" (IFCLABEL)
    Fill Pen = "" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Group Type = "Others" (IFCLABEL)
    Handrail Diameter = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Material = "Zinc" (IFCLABEL)
    Handrail Overhang (Left) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Overhang (Right) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Overhang = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Radius = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Width = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Horiz. Bar Diameter = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Inventory No. = "" (IFCLABEL)
    Left End Cutting Angle = 90. (IFCREAL)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    No. of Bars (0-None) = 4 (IFCINTEGER)
    No. of Posts (0-None) = 3 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Post Depth = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Post Material = "Zinc" (IFCLABEL)
    Post Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Production Year = "" (IFCLABEL)
    Railing Length = 1.515 (IFCLENGTHMEASURE) [MILLI METRE]
    Right End Cutting Angle = 90. (IFCREAL)
    Serial No. = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Show Axis = FALSE (IFCBOOLEAN)
    Show Posts in 2D = TRUE (IFCBOOLEAN)
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
  AC_Pset_Railing_Horizontal | properties | on 1 object (1 IFCRAILING)
    3D = "Detailed" (IFCLABEL)
    Accessories = "" (IFCLABEL)
    Axis Line Type = 6 (IFCINTEGER)
    Bar Material = "Zinc" (IFCLABEL)
    Bar Position = "on Posts" (IFCLABEL)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Contour Pen = "" (IFCLABEL)
    Cost = 0. (IFCREAL)
    Cross Section Resolution = 6 (IFCINTEGER)
    Fill Background Pen = "" (IFCLABEL)
    Fill Pen = "" (IFCLABEL)
    Fill Type = "Solid Fill" (IFCLABEL)
    Group Type = "Others" (IFCLABEL)
    Handrail Diameter = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Material = "Zinc" (IFCLABEL)
    Handrail Overhang (Left) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Overhang (Right) = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Overhang = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Radius = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Handrail Width = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Horiz. Bar Diameter = 0.02 (IFCLENGTHMEASURE) [MILLI METRE]
    Inventory No. = "" (IFCLABEL)
    Left End Cutting Angle = 90. (IFCREAL)
    Location = "" (IFCLABEL)
    Manufacturer = "" (IFCLABEL)
    No. of Bars (0-None) = 4 (IFCINTEGER)
    No. of Posts (0-None) = 3 (IFCINTEGER)
    Note/Remarks = "" (IFCLABEL)
    Object Weight = 0. (IFCREAL)
    Object Weight Unit = "kg" (IFCLABEL)
    Post Depth = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Post Material = "Zinc" (IFCLABEL)
    Post Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Production Year = "" (IFCLABEL)
    Railing Length = 1.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Right End Cutting Angle = 90. (IFCREAL)
    Serial No. = "" (IFCLABEL)
    Shadow = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = FALSE (IFCBOOLEAN)
    Show Axis = FALSE (IFCBOOLEAN)
    Show Posts in 2D = TRUE (IFCBOOLEAN)
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    User Defined 1 = "" (IFCLABEL)
    User Defined 2 = "" (IFCLABEL)
    User Defined 3 = "" (IFCLABEL)
    User Defined 4 = "" (IFCLABEL)
    User Defined 5 = "" (IFCLABEL)
  AC_Pset_Storefront_16 | properties | on 1 object (1 IFCDOOR)
    2D Detail Level = "Scale Sensitive" (IFCLABEL)
    3D Detail Level = "Detailed" (IFCLABEL)
    Angle Side 2 = 20. (IFCREAL)
    Angle Side = 20. (IFCREAL)
    Auto Turn Opposite-Side Plaster = TRUE (IFCBOOLEAN)
    Auto Turn Reference-Side Plaster = TRUE (IFCBOOLEAN)
    Bottom Level = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Rail Width = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Reveal Type (gs_reveal_type_bottom) = "No Reveal" (IFCLABEL)
    Bottom Reveal Type (gs_reveal_type_bottom_int) = 2 (IFCINTEGER)
    Bottom Side Angle = 20. (IFCREAL)
    Bottom Vert. Div. Number = 2 (IFCINTEGER)
    Bottom Vert. Div. Width (0-No) = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Bottom Vert. Mull. Number = 1 (IFCINTEGER)
    Butt Glazed Joint = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Closure Type (gs_closure_type) = "No Closure" (IFCLABEL)
    Closure Type (gs_closure_type_int) = 1 (IFCINTEGER)
    Consider Skin as Plaster = FALSE (IFCBOOLEAN)
    Contour Line Type (gs_ltJoint) = 1 (IFCINTEGER)
    Contour Line Type (gs_ltPlug) = 1 (IFCINTEGER)
    Contour Pen (gs_penJoint) = "" (IFCLABEL)
    Contour Pen (gs_penPlug) = "" (IFCLABEL)
    Custom Handle Inside = "" (IFCLABEL)
    Custom Handle Outside = "" (IFCLABEL)
    Custom Material = FALSE (IFCBOOLEAN)
    Custom Panel Name (gs_cust_p) = "" (IFCLABEL)
    Custom Panel Name (gs_cust_panel) = "" (IFCLABEL)
    Demolition / New construction = "None" (IFCLABEL)
    Demolition Background Pen = "Transparent" (IFCLABEL)
    Demolition Fill Type = "" (IFCLABEL)
    Demolition Pen = "Transparent" (IFCLABEL)
    Demolition line type = 1 (IFCINTEGER)
    Distance of Skin from Closure = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Door Stop = TRUE (IFCBOOLEAN)
    Door Stop Thickness = 0.0254 (IFCLENGTHMEASURE) [MILLI METRE]
    Door Stop Width = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Edited Jamb Side = "Edit Both Jambs" (IFCLABEL)
    Edited Skin Number = "1. Skin" (IFCLABEL)
    Edited Wall Side = "Reference Side" (IFCLABEL)
    Egress Height = 2.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Egress Width = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    End Frame Profile on Left (endFrameLeft) = "Normal" (IFCLABEL)
    End Frame Profile on Left (iEndFrameLeft) = 1 (IFCINTEGER)
    End Frame Profile on Right (endFrameRight) = "Normal" (IFCLABEL)
    End Frame Profile on Right (iEndFrameRight) = 1 (IFCINTEGER)
    Fill Background Pen (gs_penJointBg) = "" (IFCLABEL)
    Fill Background Pen (gs_penPlugBg) = "" (IFCLABEL)
    Fill Pen (gs_penJointFg) = "" (IFCLABEL)
    Fill Pen (gs_penPlugFg) = "" (IFCLABEL)
    Fill Type (gs_fillJoint) = "rigid insulation" (IFCLABEL)
    Fill Type (gs_fillPlug) = "rigid insulation" (IFCLABEL)
    Floor Plan Display Option = 3 (IFCINTEGER)
    Frame Style on Left Side = "Visible Mullions" (IFCLABEL)
    Frame Style on Mullion = "Visible Mullions" (IFCLABEL)
    Frame Style on Right Side = "Visible Mullions" (IFCLABEL)
    Frame Thickness = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Frame Thickness=Wall Thickness = FALSE (IFCBOOLEAN)
    Frame Width = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Fully Editable = TRUE (IFCBOOLEAN)
    Glass Setback = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Glass Thickness = 0.01 (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Distance from Leaf Edge = 0.035 (IFCLENGTHMEASURE) [MILLI METRE]
    Handle Height = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Head Jamb Depth = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Hole Has Wall's Side Material = TRUE (IFCBOOLEAN)
    Hole Material's Split is Curved = FALSE (IFCBOOLEAN)
    Hole Position Angle = 0. (IFCREAL)
    Horizontal Div. Number = 3 (IFCINTEGER)
    Horizontal Div. Width (0-No) = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Mullion Number = 2 (IFCINTEGER)
    Horizontal Mullion Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Horizontal Mullion Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Hotspots 0-None,1-2D,2-3D,3-All = 3 (IFCINTEGER)
    Inner Head Depth (gs_reveal_double_innerTop) = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Inner Reveal Type = "No Reveal" (IFCLABEL)
    Inner Sill Depth (gs_reveal_double_innerBottom) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Insert Insulation Strip = TRUE (IFCBOOLEAN)
    Jamb Depth = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Jamb Depth Side 2 = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Joint Left = FALSE (IFCBOOLEAN)
    Joint Lower = FALSE (IFCBOOLEAN)
    Joint Right = FALSE (IFCBOOLEAN)
    Joint Upper = FALSE (IFCBOOLEAN)
    Leaf Frame Width = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Left = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Lower = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Right = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Frame Width Upper = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Height = 2.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Thickness = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Width = 0.92 (IFCLENGTHMEASURE) [MILLI METRE]
    Left Angle = 90. (IFCREAL)
    Material (gs_cc_dutch_matJoint) = "Pine, shiny" (IFCLABEL)
    Middle Rail (bMiddleRail) = TRUE (IFCBOOLEAN)
    Middle Rail Elevation = 0.9 (IFCLENGTHMEASURE) [MILLI METRE]
    Middle Rail Width = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Middle Vert. Div. Number = 2 (IFCINTEGER)
    Middle Vert. Div. Width (0-No) = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Middle Vert. Mull. Number = 1 (IFCINTEGER)
    New Background Pen = "Transparent" (IFCLABEL)
    New Fill Type = "" (IFCLABEL)
    New Pen = "Transparent" (IFCLABEL)
    New Wall Fill Background Pen = "" (IFCLABEL)
    New Wall Fill Pen = "" (IFCLABEL)
    New Wall Fill Type = "masonry block" (IFCLABEL)
    New Wall Fill Width Left = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    New Wall Fill Width Right = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Nominal Size = 0 (IFCINTEGER)
    Number from = "Reference Side" (IFCLABEL)
    Number of Skins to Turn = 1 (IFCINTEGER)
    Opening Direction = 1 (IFCINTEGER)
    Opening Direction Leaf = "Default" (IFCLABEL)
    Opening Handle Inside (gs_handle_type) = "None" (IFCLABEL)
    Opening Handle Inside (gs_handle_type_m) = 0 (IFCINTEGER)
    Opening Handle Outside (gs_handle_type_out) = "None" (IFCLABEL)
    Opening Handle Outside (gs_handle_type_out_m) = 0 (IFCINTEGER)
    Outer Jamb Depth = 0.08 (IFCLENGTHMEASURE) [MILLI METRE]
    Outer Reveal Type = "No Reveal" (IFCLABEL)
    Panel Division Type (divisionMethod) = "Number of Divisions" (IFCLABEL)
    Panel Division Type (iDivisionMethod) = 1 (IFCINTEGER)
    Panel Style = "Style 1" (IFCLABEL)
    Parametric Level = "High" (IFCLABEL)
    Place Closure from Side (gs_cc_dutch_ClosureToSide) = 1 (IFCINTEGER)
    Place Closure from Side (gs_cc_dutch_ClosureToSide_str) = "" (IFCLABEL)
    Place Closure on Bottom = FALSE (IFCBOOLEAN)
    Place Closure on Side 1 = TRUE (IFCBOOLEAN)
    Place Closure on Side 2 = TRUE (IFCBOOLEAN)
    Place Closure on Top = FALSE (IFCBOOLEAN)
    Place Closure to Skin = 1 (IFCINTEGER)
    Plaster Thickness Limit = 0.04 (IFCLENGTHMEASURE) [MILLI METRE]
    Profile Width = 0.15 (IFCLENGTHMEASURE) [MILLI METRE]
    Retain Nominal Size on Change = FALSE (IFCBOOLEAN)
    Reveal Depth (AC_wido_sill) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Reveal Type (gs_reveal_doubleInnerTypeInt) = 0 (IFCINTEGER)
    Reveal Type (gs_reveal_doubleOuterTypeInt) = 0 (IFCINTEGER)
    Reveal Type (gs_reveal_type_int) = 1 (IFCINTEGER)
    Reveal Type (gs_reveal_type_new) = "No Reveal - Edge" (IFCLABEL)
    Reveal Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Right Angle = 90. (IFCREAL)
    Right Panel/Total Panel Opening = 50 (IFCINTEGER)
    Set Egress Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Leaf Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Reveal Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Unit Size as Nominal Size = FALSE (IFCBOOLEAN)
    Set Wallhole Size as Nominal Size = TRUE (IFCBOOLEAN)
    Show 2D Hotspots in 3D = TRUE (IFCBOOLEAN)
    Show Demolition/New parameter = FALSE (IFCBOOLEAN)
    Show Insulation Strip = TRUE (IFCBOOLEAN)
    Show Reveal on Symbol = "Always" (IFCLABEL)
    Show in 3D = FALSE (IFCBOOLEAN)
    Show new construction on Wall = FALSE (IFCBOOLEAN)
    Sidelight Side 1 = FALSE (IFCBOOLEAN)
    Sidelight Side 2 = FALSE (IFCBOOLEAN)
    Sidelight Width 1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sidelight Width 2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Height to Current Story = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sill Jamb Depth = 0.06 (IFCLENGTHMEASURE) [MILLI METRE]
    Spouwlat Thickness = 0.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Spouwlat Width = 0.038 (IFCLENGTHMEASURE) [MILLI METRE]
    Strip Thickness = 0.025 (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Left = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Lower = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Right = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tolerance Upper = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Tr. Vert. Div. Width (0-No) = 0.3 (IFCLENGTHMEASURE) [MILLI METRE]
    Transom = FALSE (IFCBOOLEAN)
    Transom Height (gs_transom_height) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Height (middlePanelHeight) = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Transom Vert. Div. Number = 2 (IFCINTEGER)
    Transom Vert. Mull. Number = 1 (IFCINTEGER)
    Turn In Skin = FALSE (IFCBOOLEAN)
    Turn Opposite-Side Plaster = 0 (IFCINTEGER)
    Turn Reference-Side Plaster = 0 (IFCINTEGER)
    Turn Skin on Side = "Both" (IFCLABEL)
    Turn Skin to Closure = FALSE (IFCBOOLEAN)
    Uniform Jamb Depth = TRUE (IFCBOOLEAN)
    Unit Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Unit Size = "Custom Size" (IFCLABEL)
    Unit Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Upper Side Angle = 20. (IFCREAL)
    Use Wall Finish Component = FALSE (IFCBOOLEAN)
    Vertical Mullion Thickness = 0.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Vertical Mullion Width = 0.03 (IFCLENGTHMEASURE) [MILLI METRE]
    Wall Contours (0-None,1-Full,2-Side,3-Length) = 0 (IFCINTEGER)
    Wall Direction Type = 0 (IFCINTEGER)
    Wall Type = 1 (IFCINTEGER)
    Wallhole Height = 2.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Wallhole Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Z Dimension = 1. (IFCLENGTHMEASURE) [MILLI METRE]

Other addresses and roles
  postal address (none given)