IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0, SurfaceGeometryAddOnView, QuantityTakeOffAddOnView, SpaceBoundary2ndLevelAddOnView]"
Description: "Option [Drawing Scale: 96.000000]"
Description: "Option [Global Unique Identifiers (GUID): Keep existing]"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Entire Model]"
Description: "Option [IFC Domain: All]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and ARCHICAD 2D elements: Off]"
Description: "Option [Convert 2D symbols of Doors and Windows: Off]"
Description: "Option [Explode Composite and Complex Profile elements into parts: On]"
Description: "Option [Export geometries that Participates in Collision Detection only: On]"
Description: "Option [Use legacy geometric methods as in Coordination View 1.0: Off]"
Description: "Option [IFC Site Geometry: As boundary representation (BRep)]"
Description: "Option [IFC Site Location: At Project Origin]"
Description: "Option [Curtain Wall export mode: Container Element]"
File name: "C:\Users\skari\OneDrive - Graphisoft SE\[1] Solibri Training\FINAL\ENG\IFC FILES\SAC_ARC_2.ifc"
Time stamp: "2018-05-03T13:29:54"
Author: "Architect"
Organization: "Building Designer Office"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.09 : 26 Sep 2013"
Originating system: "IFC file generated by GRAPHISOFT ARCHICAD-64 21.0.0 INT FULL Windows version (IFC add-on version: 5021 INT FULL)."
Authorization: "The authorising person"
Application: "ARCHICAD-64" version "21.0.0" identifier "IFC add-on version: 5021 INT FULL" by Organization "GRAPHISOFT" id "GS" description "GRAPHISOFT"

People and organizations
  Person "Undefined" of Organization "Undefined"
  Owner history of Person "Undefined" of Organization "Undefined" | application "ARCHICAD-64" version "21.0.0" identifier "IFC add-on version: 5021 INT FULL" by Organization "GRAPHISOFT" id "GS" description "GRAPHISOFT" | change ADDED | created 1525346954 (2018-05-03T11:29:14Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  CURRENCY: USD
  TIMEUNIT: Year (conversion based)
  MASSUNIT: GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "The S House"
  IFCSITE "Site" | latitude 38° 53′ 51.61″ | longitude -77° 2′ 11.58″ | elevation above sea level 30480.
    contains 12 elements
      3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Stone: Gravel 1"" | names: "S17" | material: "Stone: Gravel" | property sets: AC_Pset_RenovationAndPhasing, ArchiCADQuantities
      1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Stone: Limestone 1"" | names: "S17" | material: "Stone: Limestone" | property sets: AC_Pset_RenovationAndPhasing, ArchiCADQuantities
      8 x IFCFLOWTERMINAL | type IFCLAMPTYPE "Street Lamp 04 21" | names: "L-001" | material: "Foreground Fill" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Street_Lamp_04_21
    IFCBUILDING "Building"
      IFCBUILDINGSTOREY "BASEMENT" | elevation -914.4
        contains 50 elements
          30 x IFCPILE | names: "S21" | material: "Concrete Cast-in-Place Floor, Beam" | property sets: Pset_ConcreteElementGeneral, AC_Pset_RenovationAndPhasing, ArchiCADQuantities
          19 x IFCFOOTING | STRIP_FOOTING | material: "Concrete Cast-in-Place Floor, Beam"; materials ("Concrete Cast-in-Place Floor, Beam", "Concrete Cast-in-Place Floor, Beam"); materials ("Concrete Cast-in-Place Floor, Beam", "Concrete Cast-in-Place Floor, Beam", "Concrete Cast-in-Place Floor, Beam") | property sets: AC_Pset_RenovationAndPhasing, ArchiCADQuantities
          1 x IFCSLAB | type IFCSLABTYPE "Concrete Cast-in-Place Floor, Beam 20"" | BASESLAB | names: "S21" | material: "Concrete Cast-in-Place Floor, Beam" | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
      IFCBUILDINGSTOREY "1st FLOOR" | elevation 0.
        contains 155 elements
          13 x IFCBEAM | type IFCBEAMTYPE "W18X50 7 1/2" x 18"" | object type "W18X50 7 1/2" x 18"" | names: "Beam-01" | material: materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel") | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          23 x IFCCOLUMN | type IFCCOLUMNTYPE "HP10X57 10 1/4" x 10"" | object type "HP10X57 10 1/4" x 10"" | names: "Column-01" | material: "Metal: Stainless Steel" | property sets: Pset_ColumnCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCRAILING | type IFCRAILINGTYPE "Railing Type" | names: "RAILING - 037" | material: "Metal: Light-Frame" | property sets: AC_Pset_RenovationAndPhasing, Pset_RailingCommon, BaseQuantities, ArchiCADQuantities
          4 x IFCWALL | type IFCWALLTYPE "Demo Staircase Wall 11 1/4"" | parts: 12 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCWALL | type IFCWALLTYPE "Demo Staircase Wall with Insulation 15 1/4"" | parts: 4 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Storefront Window 21" | names: "04" | material: materials ("Background Fill", "Background Fill", "Air Space", "Background Fill", "Background Fill") | property sets: Pset_DoorWindowGlazingType, Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "Demo 1st Floor Slab 20"" | BASESLAB | names: "S19" | parts: 3 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "Storefront Double Door 21" | names: "A" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall Type" | names: "CW24" | parts: 574 IFCBUILDINGELEMENTPROXY, 3 IFCDOOR | property sets: Pset_ConcreteElementGeneral, Pset_CurtainWallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Demo 1st Floor Flooring 4 1/2"" | FLOORING | names: "S32" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCSTAIR | HALF_TURN_STAIR | names: "STAIR - 016" | parts: 38 IFCBUILDINGELEMENTPROXY, 2 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_ConcreteElementGeneral, Pset_StairCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCTRANSPORTELEMENT | type IFCTRANSPORTELEMENTTYPE "Elevator 21" | ELEVATOR | names: "ELEVATOR-026" | material: "Background Fill" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Elevator_21
          1 x IFCBEAM | type IFCBEAMTYPE "Curtain Wall Type" | object type "Curtain Wall Type" | names: "CW23" | parts: 220 IFCBEAM, 96 IFCBUILDINGELEMENTPROXY | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          3 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Mirror 21" | names: "ELEVATOR-009" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Mirror_21
          5 x IFCWALL | type IFCWALLTYPE "Demo Restroom Wall with tiles 6 1/4"" | parts: 25 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          3 x IFCWALL | type IFCWALLTYPE "Demo Restroom Wall 5 3/4"" | parts: 15 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Commercial Bath Stall 21" | names: "ELEVATOR-008" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Commercial_Bath_Stall_21
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Toilet ADA 21" | names: "ELEVATOR-012" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Toilet_ADA_21
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Basin 21" | names: "ELEVATOR-013" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Basin_21
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Urinal 21" | names: "ELEVATOR-009" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Urinal_21
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Multi-Basin Counter 21" | names: "ELEVATOR-010" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Multi-Basin_Counter_21
          1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Sofa Layout 21" | names: "CAB21" | material: "Background Fill" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Sofa_Layout_21
          32 x IFCFLOWTERMINAL | type IFCLAMPTYPE "Pendant Lamp 21" | names: "L-002" | material: "Foreground Fill" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Pendant_Lamp_21
          9 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Dining Table Rectangle 21" | names: "ELEVATOR-014" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Dining_Table_Rectangle_21
          24 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Designer Chair 11 21" | names: "ELEVATOR-015" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Designer_Chair_11_21
          8 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Coffee Table 01 21" | names: "ELEVATOR-016" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Coffee_Table_01_21
          2 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Wood: Plywood" | names: "M12" | material: "Wood: Plywood" | property sets: AC_Pset_RenovationAndPhasing, ArchiCADQuantities
          4 x IFCWALL | type IFCWALLTYPE "Concrete Cast-in-Place Floor, Beam 6"" | material: "Concrete Cast-in-Place Floor, Beam" | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCGRID | names: "Grid"
        IFCSPACE "004" | long name "Elevator" | INTERNAL
        IFCSPACE "002" | long name "Entry" | INTERNAL
        IFCSPACE "004" | long name "Shaft" | INTERNAL
        IFCSPACE "007" | long name "Café" | INTERNAL
        IFCSPACE "002" | long name "Toilette" | INTERNAL
        IFCSPACE "003" | long name "Toilette" | INTERNAL
        IFCSPACE "004" | long name "Toilette" | INTERNAL
        IFCSPACE "005" | long name "Toilette" | INTERNAL
        IFCSPACE "006" | long name "Toilette" | INTERNAL
        IFCSPACE "005" | long name "Staircase" | INTERNAL
        IFCSPACE "002" | long name "Storage" | INTERNAL
        IFCSPACE "002" | long name "Corridor" | INTERNAL
      IFCBUILDINGSTOREY "2nd FLOOR" | elevation 3657.6
        contains 117 elements
          11 x IFCBEAM | type IFCBEAMTYPE "W18X50 7 1/2" x 18"" | object type "W18X50 7 1/2" x 18"" | names: "Beam-01" | material: materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); "Metal: Stainless Steel"; materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel") | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          17 x IFCCOLUMN | type IFCCOLUMNTYPE "HP10X57 10 1/4" x 10"" | object type "HP10X57 10 1/4" x 10"" | names: "Column-01" | material: "Metal: Stainless Steel" | property sets: Pset_ColumnCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          3 x IFCBEAM | type IFCBEAMTYPE "Curved_Beam" | object type "Curved_Beam" | names: "ELEVATOR-025" | material: "Background Fill" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Curved_Beam
          2 x IFCWALL | type IFCWALLTYPE "Demo Staircase Wall 11 1/4"" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          2 x IFCWALL | type IFCWALLTYPE "Demo Staircase Wall with Insulation 15 1/4"" | parts: 8 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Storefront Window 21" | names: "05" | material: materials ("Background Fill", "Background Fill", "Air Space", "Background Fill", "Background Fill") | property sets: Pset_DoorWindowGlazingType, Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Storefront Double Door 21" | names: "A" | material: materials ("Background Fill", "Background Fill-International", "Background Fill", "Air Space", "Background Fill", "Background Fill") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          2 x IFCRAILING | type IFCRAILINGTYPE "Railing Type" | names: "RAILING - 036", "RAILING - 040" | material: "Metal: Light-Frame"; "Metal: Stainless Steel" | property sets: AC_Pset_RenovationAndPhasing, Pset_RailingCommon, BaseQuantities, ArchiCADQuantities
          1 x IFCSLAB | type IFCSLABTYPE "FLR Conc.+Stl Deck; 6": 6"" | names: "S19" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall Type" | names: "CW25" | parts: 419 IFCBUILDINGELEMENTPROXY, 1 IFCDOOR | property sets: Pset_ConcreteElementGeneral, Pset_CurtainWallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Demo Terrace Flooring copy 4 1/2"" | FLOORING | names: "S28" | parts: 3 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Demo Carpet Floor 2"" | FLOORING | names: "S29" | parts: 3 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCSTAIR | HALF_TURN_STAIR | names: "STAIR - 016" | parts: 38 IFCBUILDINGELEMENTPROXY, 2 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_ConcreteElementGeneral, Pset_StairCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Multi-Basin Counter 21" | names: "ELEVATOR-010" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Multi-Basin_Counter_21
          5 x IFCWALL | type IFCWALLTYPE "Demo Restroom Wall with tiles 6 1/4"" | parts: 25 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Commercial Bath Stall 21" | names: "ELEVATOR-008" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Commercial_Bath_Stall_21
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Basin 21" | names: "ELEVATOR-013" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Basin_21
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Toilet ADA 21" | names: "ELEVATOR-012" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Toilet_ADA_21
          3 x IFCWALL | type IFCWALLTYPE "Demo Restroom Wall 5 3/4"" | parts: 15 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Urinal 21" | names: "ELEVATOR-009" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Urinal_21
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | material: materials ("Background Fill", "Background Fill-International", "Air Space", "Background Fill", "Air Space", "Air Space", "Insulation Rigid", "Background Fill-International", "Background Fill-International", "Air Space", "Background Fill-International", "Insulation Batt") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | material: materials ("Background Fill", "Background Fill-International", "Air Space", "Background Fill", "Air Space", "Air Space", "Insulation Rigid", "Background Fill-International", "Background Fill-International", "Air Space", "Background Fill-International", "Insulation Batt") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | material: materials ("Background Fill", "Background Fill-International", "Air Space", "Background Fill", "Air Space", "Air Space", "Insulation Rigid", "Background Fill-International", "Background Fill-International", "Air Space", "Background Fill-International", "Insulation Batt") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | material: materials ("Background Fill", "Background Fill-International", "Air Space", "Background Fill", "Air Space", "Air Space", "Insulation Rigid", "Background Fill-International", "Background Fill-International", "Air Space", "Background Fill-International", "Insulation Batt") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | material: materials ("Background Fill", "Background Fill-International", "Air Space", "Background Fill", "Air Space", "Air Space", "Insulation Rigid", "Background Fill-International", "Background Fill-International", "Air Space", "Background Fill-International", "Insulation Batt") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Demo Tiles Flooring 2"" | FLOORING | names: "S30" | parts: 3 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          12 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Designer Chair 11 21" | names: "ELEVATOR-015" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Designer_Chair_11_21
          4 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Coffee Table 01 21" | names: "ELEVATOR-016" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Coffee_Table_01_21
          1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Kitchen Layout 21" | names: "ELEVATOR-009" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Kitchen_Layout_21
          6 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Office Layout Linear 21" | names: "CAB25", "CAB24" | material: "Background Fill" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Office_Layout_Linear_21
          25 x IFCFLOWTERMINAL | type IFCLAMPTYPE "Pendant Lamp 21" | names: "L-002" | material: "Foreground Fill" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Pendant_Lamp_21
          4 x IFCWALL | type IFCWALLTYPE "Concrete Cast-in-Place Floor, Beam 6"" | material: "Concrete Cast-in-Place Floor, Beam" | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
        IFCSPACE "004" | long name "Staircase" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Demo Tiles Flooring 2"" | FLOORING | names: "S30" | parts: 3 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
        IFCSPACE "004" | long name "Shaft" | INTERNAL
        IFCSPACE "004" | long name "Elevator" | INTERNAL
        IFCSPACE "002" | long name "Office" | INTERNAL
        IFCSPACE "006" | long name "Toilette" | INTERNAL
        IFCSPACE "005" | long name "Toilette" | INTERNAL
        IFCSPACE "002" | long name "Kitchen" | INTERNAL
        IFCSPACE "002" | long name "Toilette" | INTERNAL
        IFCSPACE "003" | long name "Toilette" | INTERNAL
        IFCSPACE "004" | long name "Toilette" | INTERNAL
      IFCBUILDINGSTOREY "3rd FLOOR" | elevation 7315.2
        contains 102 elements
          10 x IFCBEAM | type IFCBEAMTYPE "W18X50 7 1/2" x 18"" | object type "W18X50 7 1/2" x 18"" | names: "Beam-01" | material: materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel") | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          17 x IFCCOLUMN | type IFCCOLUMNTYPE "HP10X57 10 1/4" x 10"" | object type "HP10X57 10 1/4" x 10"" | names: "Column-01" | material: "Metal: Stainless Steel" | property sets: Pset_ColumnCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          2 x IFCWALL | type IFCWALLTYPE "Demo Staircase Wall 11 1/4"" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          2 x IFCWALL | type IFCWALLTYPE "Demo Staircase Wall with Insulation 15 1/4"" | parts: 8 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Storefront Window 21" | names: "06" | material: materials ("Background Fill", "Background Fill", "Air Space", "Background Fill", "Background Fill") | property sets: Pset_DoorWindowGlazingType, Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "Storefront Double Door 21" | names: "A" | material: materials ("Background Fill", "Background Fill-International", "Background Fill", "Air Space", "Background Fill", "Background Fill") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          3 x IFCBEAM | type IFCBEAMTYPE "Curved_Beam" | object type "Curved_Beam" | names: "ELEVATOR-025" | material: "Background Fill" | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Curved_Beam
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Basin 21" | names: "ELEVATOR-013" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Basin_21
          1 x IFCSLAB | type IFCSLABTYPE "FLR Conc.+Stl Deck; 6": 6"" | names: "S19" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall Type" | names: "CW26" | parts: 420 IFCBUILDINGELEMENTPROXY | property sets: Pset_ConcreteElementGeneral, Pset_CurtainWallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Demo Terrace Flooring copy 4 1/2"" | FLOORING | names: "S25" | parts: 3 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          2 x IFCCOVERING | type IFCCOVERINGTYPE "Demo Carpet Floor 2"" | FLOORING | names: "S27" | parts: 6 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCSTAIR | HALF_TURN_STAIR | names: "STAIR - 016" | parts: 38 IFCBUILDINGELEMENTPROXY, 2 IFCSTAIRFLIGHT, 1 IFCSLAB | property sets: Pset_ConcreteElementGeneral, Pset_StairCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          2 x IFCRAILING | type IFCRAILINGTYPE "Railing Type" | names: "RAILING - 035", "RAILING - 038" | material: "Metal: Light-Frame"; "Metal: Stainless Steel" | property sets: AC_Pset_RenovationAndPhasing, Pset_RailingCommon, BaseQuantities, ArchiCADQuantities
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Toilet ADA 21" | names: "ELEVATOR-012" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Toilet_ADA_21
          1 x IFCBEAM | type IFCBEAMTYPE "Curtain Wall Type" | object type "Curtain Wall Type" | names: "CW23" | parts: 256 IFCBEAM | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          5 x IFCWALL | type IFCWALLTYPE "Demo Restroom Wall with tiles 6 1/4"" | parts: 25 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          3 x IFCWALL | type IFCWALLTYPE "Demo Restroom Wall 5 3/4"" | parts: 15 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Multi-Basin Counter 21" | names: "ELEVATOR-010" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Multi-Basin_Counter_21
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Urinal 21" | names: "ELEVATOR-009" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Urinal_21
          2 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Commercial Bath Stall 21" | names: "ELEVATOR-008" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Commercial_Bath_Stall_21
          1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Kitchen Layout 21" | names: "ELEVATOR-009" | material: "Brick" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Kitchen_Layout_21
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | material: materials ("Background Fill", "Background Fill-International", "Air Space", "Background Fill", "Air Space", "Air Space", "Insulation Rigid", "Background Fill-International", "Background Fill-International", "Air Space", "Background Fill-International", "Insulation Batt") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | material: materials ("Background Fill", "Background Fill-International", "Air Space", "Background Fill", "Air Space", "Air Space", "Insulation Rigid", "Background Fill-International", "Background Fill-International", "Air Space", "Background Fill-International", "Insulation Batt") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | material: materials ("Background Fill", "Background Fill-International", "Air Space", "Background Fill", "Air Space", "Air Space", "Insulation Rigid", "Background Fill-International", "Background Fill-International", "Air Space", "Background Fill-International", "Insulation Batt") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | material: materials ("Background Fill", "Background Fill-International", "Air Space", "Background Fill", "Air Space", "Air Space", "Insulation Rigid", "Background Fill-International", "Background Fill-International", "Air Space", "Background Fill-International", "Insulation Batt") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Commercial 21" | names: "A" | material: materials ("Background Fill", "Background Fill-International", "Air Space", "Background Fill", "Air Space", "Air Space", "Insulation Rigid", "Background Fill-International", "Background Fill-International", "Air Space", "Background Fill-International", "Insulation Batt") | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Demo Tiles Flooring 2"" | FLOORING | names: "S27" | parts: 3 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          25 x IFCFLOWTERMINAL | type IFCLAMPTYPE "Pendant Lamp 21" | names: "L-002" | material: "Foreground Fill" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Pendant_Lamp_21
          6 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Office Layout Linear 21" | names: "CAB25", "CAB24" | material: "Background Fill" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Office_Layout_Linear_21
          4 x IFCWALL | type IFCWALLTYPE "Concrete Cast-in-Place Floor, Beam 6"" | material: "Concrete Cast-in-Place Floor, Beam" | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
        IFCSPACE "003" | long name "Staircase" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Demo Tiles Flooring 2"" | FLOORING | names: "S26" | parts: 3 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
        IFCSPACE "004" | long name "Shaft" | INTERNAL
        IFCSPACE "004" | long name "Elevator" | INTERNAL
        IFCSPACE "002" | long name "Toilette" | INTERNAL
        IFCSPACE "003" | long name "Toilette" | INTERNAL
        IFCSPACE "004" | long name "Toilette" | INTERNAL
        IFCSPACE "005" | long name "Toilette" | INTERNAL
        IFCSPACE "006" | long name "Toilette" | INTERNAL
        IFCSPACE "002" | long name "Office" | INTERNAL
        IFCSPACE "002" | long name "Kitchen" | INTERNAL
      IFCBUILDINGSTOREY "4th FLOOR" | elevation 10972.8
        contains 54 elements
          16 x IFCBEAM | type IFCBEAMTYPE "W18X50 7 1/2" x 18"" | object type "W18X50 7 1/2" x 18"" | names: "Beam-01", "Beam-02" | material: materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); "Metal: Stainless Steel"; materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel"); materials ("Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel", "Metal: Stainless Steel") | property sets: Pset_BeamCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          16 x IFCCOLUMN | type IFCCOLUMNTYPE "HP10X57 10 1/4" x 10"" | object type "HP10X57 10 1/4" x 10"" | names: "Column-01" | material: "Metal: Stainless Steel" | property sets: Pset_ColumnCommon, Pset_ConcreteElementGeneral, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCWALL | type IFCWALLTYPE "Demo Staircase Wall 11 1/4"" | parts: 3 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCDOOR | type IFCDOORSTYLE "D1 Combi Commercial 21" | names: "A" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          3 x IFCWALL | type IFCWALLTYPE "Demo Staircase Wall with Insulation 15 1/4"" | parts: 12 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Storefront Window 21" | names: "07" | material: materials ("Background Fill", "Background Fill", "Air Space", "Background Fill", "Background Fill") | property sets: Pset_DoorWindowGlazingType, Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "W Round Pivot 21" | names: "03" | material: materials ("Background Fill", "Background Fill-International", "Air Space", "Background Fill", "Background Fill", "Background Fill-International", "Background Fill-International", "Air Space", "Background Fill-International", "Insulation Batt") | property sets: Pset_DoorWindowGlazingType, Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "FLR Conc.+Stl Deck; 6": 6"" | names: "S19" | parts: 2 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCCURTAINWALL | type IFCCURTAINWALLTYPE "Curtain Wall Type" | names: "CW27" | parts: 230 IFCBUILDINGELEMENTPROXY, 1 IFCDOOR | property sets: Pset_ConcreteElementGeneral, Pset_CurtainWallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Demo Terrace Flooring copy 4 1/2"" | FLOORING | names: "S22" | parts: 3 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Demo Carpet Floor 2"" | FLOORING | names: "S23" | parts: 3 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          1 x IFCRAILING | type IFCRAILINGTYPE "Railing Type" | names: "RAILING - 039" | material: "Metal: Stainless Steel" | property sets: AC_Pset_RenovationAndPhasing, Pset_RailingCommon, BaseQuantities, ArchiCADQuantities
          4 x IFCFLOWTERMINAL | type IFCLAMPTYPE "Pendant Lamp 21" | names: "L-002" | material: "Foreground Fill" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Pendant_Lamp_21
          1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Office Workstation Solo 21" | names: "CAB26" | material: "Background Fill" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Office_Workstation_Solo_21
          1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "Sofa Layout 21" | names: "CAB21" | material: "Background Fill" | property sets: Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing, ArchiCADQuantities, AC_Equantity_Sofa_Layout_21
          4 x IFCWALL | type IFCWALLTYPE "Concrete Cast-in-Place Floor, Beam 6"" | material: "Concrete Cast-in-Place Floor, Beam" | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
        IFCSPACE "006" | long name "Staircase" | INTERNAL
          contains 1 element
            1 x IFCCOVERING | type IFCCOVERINGTYPE "Demo Tiles Flooring 2"" | FLOORING | names: "S24" | parts: 3 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_CoveringCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
        IFCSPACE "004" | long name "Elevator" | INTERNAL
        IFCSPACE "003" | long name "Office" | INTERNAL
      IFCBUILDINGSTOREY "PARAPET" | elevation 14630.4
        contains 7 elements
          1 x IFCSLAB | type IFCSLABTYPE "Demo Project - Flat Roof 11 1/4"" | ROOF | names: "S20" | parts: 5 IFCBUILDINGELEMENTPART | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          4 x IFCWALL | type IFCWALLTYPE "Concrete Cast-in-Place Floor, Beam 6"" | material: "Concrete Cast-in-Place Floor, Beam" | property sets: Pset_ConcreteElementGeneral, Pset_WallCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities
          2 x IFCSLAB | type IFCSLABTYPE "Concrete Cast-in-Place Floor, Beam 6"" | ROOF | names: "S23" | material: "Concrete Cast-in-Place Floor, Beam" | property sets: Pset_ConcreteElementGeneral, Pset_SlabCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing, BaseQuantities, ArchiCADQuantities

Types
  IFCBUILDINGELEMENTPROXYTYPE "Stone: Gravel 1"" | 3 occurrences
  IFCBUILDINGELEMENTPROXYTYPE "Stone: Limestone 1"" | 1 occurrence
  IFCLAMPTYPE "Street Lamp 04 21" | 8 occurrences
  IFCSLABTYPE "Concrete Cast-in-Place Floor, Beam 20"" | FLOOR | 1 occurrence
  IFCBEAMTYPE "W18X50 7 1/2" x 18"" | 50 occurrences
  IFCCOLUMNTYPE "HP10X57 10 1/4" x 10"" | 73 occurrences
  IFCRAILINGTYPE "Railing Type" | 6 occurrences
  IFCWALLTYPE "Demo Staircase Wall 11 1/4"" | 9 occurrences
  IFCWALLTYPE "Demo Staircase Wall with Insulation 15 1/4"" | 8 occurrences
  IFCWINDOWSTYLE "Storefront Window 21" | SINGLE_PANEL | 4 occurrences | property sets: Window Lining Properties, Window Panel Properties - Panel 1
  IFCSLABTYPE "Demo 1st Floor Slab 20"" | FLOOR | 1 occurrence
  IFCDOORSTYLE "Storefront Double Door 21" | DOUBLE_DOOR_SINGLE_SWING | 3 occurrences | property sets: Door Lining Properties, Door Panel Properties - Panel 1, Door Panel Properties - Panel 2
  IFCCURTAINWALLTYPE "Curtain Wall Type" | 4 occurrences
  IFCCOVERINGTYPE "Demo 1st Floor Flooring 4 1/2"" | FLOORING | 2 occurrences
  IFCTRANSPORTELEMENTTYPE "Elevator 21" | 1 occurrence
  IFCBEAMTYPE "Curtain Wall Type" | 2 occurrences
  IFCSANITARYTERMINALTYPE "Mirror 21" | 3 occurrences
  IFCWALLTYPE "Demo Restroom Wall with tiles 6 1/4"" | 15 occurrences
  IFCWALLTYPE "Demo Restroom Wall 5 3/4"" | 9 occurrences
  IFCDOORSTYLE "D1 Commercial 21" | SINGLE_SWING_RIGHT | 3 occurrences | property sets: Door Lining Properties, Door Panel Properties - Panel 1
  IFCDOORSTYLE "D1 Commercial 21" | SINGLE_SWING_LEFT | 3 occurrences | property sets: Door Lining Properties, Door Panel Properties - Panel 1
  IFCDOORSTYLE "D1 Commercial 21" | SINGLE_SWING_LEFT | 3 occurrences | property sets: Door Lining Properties, Door Panel Properties - Panel 1
  IFCDOORSTYLE "D1 Commercial 21" | SINGLE_SWING_RIGHT | 3 occurrences | property sets: Door Lining Properties, Door Panel Properties - Panel 1
  IFCDOORSTYLE "D1 Commercial 21" | SINGLE_SWING_LEFT | 3 occurrences | property sets: Door Lining Properties, Door Panel Properties - Panel 1
  IFCSANITARYTERMINALTYPE "Commercial Bath Stall 21" | 2 occurrences
  IFCSANITARYTERMINALTYPE "Toilet ADA 21" | 1 occurrence
  IFCSANITARYTERMINALTYPE "Basin 21" | 1 occurrence
  IFCSANITARYTERMINALTYPE "Urinal 21" | 1 occurrence
  IFCSANITARYTERMINALTYPE "Multi-Basin Counter 21" | 2 occurrences
  IFCFURNITURETYPE "Sofa Layout 21" | 2 occurrences
  IFCLAMPTYPE "Pendant Lamp 21" | 86 occurrences
  IFCFURNITURETYPE "Dining Table Rectangle 21" | 9 occurrences
  IFCFURNITURETYPE "Designer Chair 11 21" | 36 occurrences
  IFCFURNITURETYPE "Coffee Table 01 21" | 12 occurrences
  IFCFURNITURETYPE "Wood: Plywood" | 2 occurrences
  IFCWALLTYPE "Concrete Cast-in-Place Floor, Beam 6"" | 20 occurrences
  IFCBEAMTYPE "Curved_Beam" | 6 occurrences
  IFCSLABTYPE "FLR Conc.+Stl Deck; 6": 6"" | FLOOR | 3 occurrences
  IFCCOVERINGTYPE "Demo Terrace Flooring copy 4 1/2"" | FLOORING | 3 occurrences
  IFCCOVERINGTYPE "Demo Carpet Floor 2"" | FLOORING | 4 occurrences
  IFCSANITARYTERMINALTYPE "Multi-Basin Counter 21" | 4 occurrences
  IFCSANITARYTERMINALTYPE "Commercial Bath Stall 21" | 4 occurrences
  IFCSANITARYTERMINALTYPE "Basin 21" | 2 occurrences
  IFCSANITARYTERMINALTYPE "Toilet ADA 21" | 2 occurrences
  IFCSANITARYTERMINALTYPE "Urinal 21" | 2 occurrences
  IFCCOVERINGTYPE "Demo Tiles Flooring 2"" | FLOORING | 5 occurrences
  IFCFURNITURETYPE "Kitchen Layout 21" | 2 occurrences
  IFCFURNITURETYPE "Office Layout Linear 21" | 12 occurrences
  IFCDOORSTYLE "D1 Combi Commercial 21" | USERDEFINED | 1 occurrence
  IFCWINDOWSTYLE "W Round Pivot 21" | USERDEFINED | 1 occurrence
  IFCFURNITURETYPE "Office Workstation Solo 21" | 1 occurrence
  IFCSLABTYPE "Demo Project - Flat Roof 11 1/4"" | ROOF | 1 occurrence
  IFCSLABTYPE "Concrete Cast-in-Place Floor, Beam 6"" | ROOF | 2 occurrences

Property sets
  BaseQuantities | quantities | on 73 objects (73 IFCCOLUMN)
    CrossSectionArea = 0.010668651 [SQUARE_METRE]
    Depth = 254. [MILLI METRE]
    GrossSurfaceArea = 5.564869014 [SQUARE_METRE]
    GrossVolume = 0.0390216578976 [CUBIC_METRE]
    Length = 3657.6 [MILLI METRE]
    NetVolume = 0.0390216578976 [CUBIC_METRE]
    OuterSurfaceArea = 5.543531712 [SQUARE_METRE]
    TotalSurfaceArea = 5.564869014 [SQUARE_METRE]
    Width = 259.08 [MILLI METRE]
  BaseQuantities | quantities | on 15 objects (15 IFCBEAM)
    CrossSectionArea = 0.0093796048 [SQUARE_METRE]
    GrossSurfaceArea = 11.5058788536 [SQUARE_METRE]
    GrossVolume = 0.065175694965 [CUBIC_METRE]
    Length = 7124.7 [MILLI METRE]
    NetSurfaceAreaExtrudedSides = 11.487119644 [SQUARE_METRE]
    NetVolume = 0.065175694965 [CUBIC_METRE]
    OuterSurfaceArea = 11.487119644 [SQUARE_METRE]
    TotalSurfaceArea = 11.5058788536 [SQUARE_METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCDOOR)
    Area = 1.9822137775 [SQUARE_METRE]
    Depth = 147.240624703 [MILLI METRE]
    Height = 2082.8 [MILLI METRE]
    Perimeter = 6069.0125 [MILLI METRE]
    Volume = 0.100108958048 [CUBIC_METRE]
    Width = 951.70625 [MILLI METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCDOOR)
    Area = 1.9822137775 [SQUARE_METRE]
    Depth = 160.337499857 [MILLI METRE]
    Height = 2082.8 [MILLI METRE]
    Perimeter = 6069.0125 [MILLI METRE]
    Volume = 0.100108958048 [CUBIC_METRE]
    Width = 951.70625 [MILLI METRE]
  BaseQuantities | quantities | on 5 objects (5 IFCBEAM)
    CrossSectionArea = 0.0093796048 [SQUARE_METRE]
    GrossSurfaceArea = 11.8724086148 [SQUARE_METRE]
    GrossVolume = 0.0669683342041 [CUBIC_METRE]
    Length = 7124.7 [MILLI METRE]
    NetSurfaceAreaExtrudedSides = 11.8536494052 [SQUARE_METRE]
    NetVolume = 0.0669683342041 [CUBIC_METRE]
    OuterSurfaceArea = 11.8536494052 [SQUARE_METRE]
    TotalSurfaceArea = 11.8724086148 [SQUARE_METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCWALL)
    GrossFootprintArea = 0.35999928 [SQUARE_METRE]
    GrossSideArea = 9.19740096 [SQUARE_METRE]
    GrossVolume = 1.4016839063 [CUBIC_METRE]
    Height = 3657.6 [MILLI METRE]
    Length = 2362.2 [MILLI METRE]
    NetFootprintArea = 0.35999928 [SQUARE_METRE]
    NetSideArea = 9.19740096 [SQUARE_METRE]
    NetVolume = 1.4016839063 [CUBIC_METRE]
    Width = 152.4 [MILLI METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCWALL)
    GrossFootprintArea = 0.28935426 [SQUARE_METRE]
    GrossSideArea = 6.94450224 [SQUARE_METRE]
    GrossVolume = 1.05834214138 [CUBIC_METRE]
    Height = 3657.6 [MILLI METRE]
    Length = 1898.65 [MILLI METRE]
    NetFootprintArea = 0.28935426 [SQUARE_METRE]
    NetSideArea = 6.94450224 [SQUARE_METRE]
    NetVolume = 1.05834214138 [CUBIC_METRE]
    Width = 152.4 [MILLI METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCWALL)
    GrossFootprintArea = 0.28935426 [SQUARE_METRE]
    GrossSideArea = 6.94450224 [SQUARE_METRE]
    GrossVolume = 1.05834214138 [CUBIC_METRE]
    Height = 3657.6 [MILLI METRE]
    Length = 1898.65 [MILLI METRE]
    NetFootprintArea = 0.28935426 [SQUARE_METRE]
    NetSideArea = 3.30741274 [SQUARE_METRE]
    NetVolume = 0.504049701576 [CUBIC_METRE]
    Width = 152.4 [MILLI METRE]
  BaseQuantities: 136 more contents on 174 objects not shown
  Pset_ConcreteElementGeneral | properties | on 700 objects (534 IFCBEAM, 73 IFCCOLUMN, 61 IFCWALL, 14 IFCCOVERING)
    ConstructionType = "Undefined" (IFCLABEL)
    FireRating = "Unrated" (IFCLABEL)
  Pset_ConcreteElementGeneral | properties | on 237 objects (237 IFCBUILDINGELEMENTPROXY)
    FireRating = "" (IFCLABEL)
  Pset_ConcreteElementGeneral | properties | on 30 objects (30 IFCPILE)
    ConstructionType = "Undefined" (IFCLABEL)
  Pset_ConcreteElementGeneral | properties | on 6 objects (6 IFCSTAIRFLIGHT)
    FireRating = "Unrated" (IFCLABEL)
  AC_Pset_RenovationAndPhasing | properties | on 2290 objects (1761 IFCBUILDINGELEMENTPROXY, 118 IFCFLOWTERMINAL, 73 IFCCOLUMN, 61 IFCFURNISHINGELEMENT)
    Renovation Status = "New" (IFCLABEL)
  AC_Pset_RenovationAndPhasing | properties | on 587 objects (476 IFCBEAM, 96 IFCBUILDINGELEMENTPROXY, 15 IFCFURNISHINGELEMENT)
    Renovation Status = "Existing" (IFCLABEL)
  ArchiCADQuantities | quantities | on 82 objects (82 IFCBUILDINGELEMENTPROXY)
    Elevation to Project Zero = 3200.4 [MILLI METRE]
    Elevation to Reference Level 1 = 10820.4 [MILLI METRE]
    Elevation to Reference Level 2 = -4419.6 [MILLI METRE]
    Elevation to Sea Level = 33680.4 [MILLI METRE]
    Elevation to Story = 3200.4 [MILLI METRE]
    Frame Depth = 152.4 [MILLI METRE]
    Frame Length = 406.4 [MILLI METRE]
    Home Offset = 3200.4 [MILLI METRE]
    Net Volume = 0.003146316288 [CUBIC_METRE]
    Surface Area = 0.00774192 [SQUARE_METRE]
    Width = 50.8 [MILLI METRE]
  ArchiCADQuantities | quantities | on 81 objects (81 IFCBUILDINGELEMENTPROXY)
    Elevation to Project Zero = 152.4 [MILLI METRE]
    Elevation to Reference Level 1 = 7772.4 [MILLI METRE]
    Elevation to Reference Level 2 = -7467.6 [MILLI METRE]
    Elevation to Sea Level = 30632.4 [MILLI METRE]
    Elevation to Story = 152.4 [MILLI METRE]
    Frame Depth = 152.4 [MILLI METRE]
    Frame Length = 2936.875 [MILLI METRE]
    Home Offset = 152.4 [MILLI METRE]
    Net Volume = 0.0227370513 [CUBIC_METRE]
    Surface Area = 0.00774192 [SQUARE_METRE]
    Width = 50.8 [MILLI METRE]
  ArchiCADQuantities | quantities | on 73 objects (73 IFCBUILDINGELEMENTPROXY)
    Elevation to Project Zero = 3200.4 [MILLI METRE]
    Elevation to Reference Level 1 = 10820.4 [MILLI METRE]
    Elevation to Reference Level 2 = -4419.6 [MILLI METRE]
    Elevation to Sea Level = 33680.4 [MILLI METRE]
    Elevation to Story = 3200.4 [MILLI METRE]
    Gross Surface Area = 0.39483792 [SQUARE_METRE]
    Height = 381. [MILLI METRE]
    Home Offset = 3200.4 [MILLI METRE]
    Net Volume = 0.027994008528 [CUBIC_METRE]
    Nominal Height = 381. [MILLI METRE]
    Nominal Surface Area = 0.3290316 [SQUARE_METRE]
    Nominal Width = 863.6 [MILLI METRE]
    Perimeter = 2489.2 [MILLI METRE]
    Surface Area = 0.3290316 [SQUARE_METRE]
    Thickness = 25.4 [MILLI METRE]
    Width = 863.6 [MILLI METRE]
  ArchiCADQuantities | quantities | on 73 objects (73 IFCBUILDINGELEMENTPROXY)
    Elevation to Project Zero = 152.4 [MILLI METRE]
    Elevation to Reference Level 1 = 7772.4 [MILLI METRE]
    Elevation to Reference Level 2 = -7467.6 [MILLI METRE]
    Elevation to Sea Level = 30632.4 [MILLI METRE]
    Elevation to Story = 152.4 [MILLI METRE]
    Frame Depth = 152.4 [MILLI METRE]
    Frame Length = 914.4 [MILLI METRE]
    Home Offset = 152.4 [MILLI METRE]
    Net Volume = 0.01548577548 [CUBIC_METRE]
    Surface Area = 0.01693545 [SQUARE_METRE]
    Width = 111.125 [MILLI METRE]
  ArchiCADQuantities | quantities | on 73 objects (73 IFCBUILDINGELEMENTPROXY)
    Elevation to Project Zero = 3657.6 [MILLI METRE]
    Elevation to Reference Level 1 = 11277.6 [MILLI METRE]
    Elevation to Reference Level 2 = -3962.4 [MILLI METRE]
    Elevation to Sea Level = 34137.6 [MILLI METRE]
    Elevation to Story = 3657.6 [MILLI METRE]
    Frame Depth = 152.4 [MILLI METRE]
    Frame Length = 914.4 [MILLI METRE]
    Home Offset = 3657.6 [MILLI METRE]
    Net Volume = 0.007079211648 [CUBIC_METRE]
    Surface Area = 0.00774192 [SQUARE_METRE]
    Width = 50.8 [MILLI METRE]
  ArchiCADQuantities | quantities | on 73 objects (73 IFCBUILDINGELEMENTPROXY)
    Elevation to Project Zero = 3200.4 [MILLI METRE]
    Elevation to Reference Level 1 = 10820.4 [MILLI METRE]
    Elevation to Reference Level 2 = -4419.6 [MILLI METRE]
    Elevation to Sea Level = 33680.4 [MILLI METRE]
    Elevation to Story = 3200.4 [MILLI METRE]
    Frame Depth = 152.4 [MILLI METRE]
    Frame Length = 863.6 [MILLI METRE]
    Home Offset = 3200.4 [MILLI METRE]
    Net Volume = 0.006685922112 [CUBIC_METRE]
    Surface Area = 0.00774192 [SQUARE_METRE]
    Width = 50.8 [MILLI METRE]
  ArchiCADQuantities | quantities | on 67 objects (67 IFCBUILDINGELEMENTPROXY)
    Elevation to Project Zero = 152.4 [MILLI METRE]
    Elevation to Reference Level 1 = 7772.4 [MILLI METRE]
    Elevation to Reference Level 2 = -7467.6 [MILLI METRE]
    Elevation to Sea Level = 30632.4 [MILLI METRE]
    Elevation to Story = 152.4 [MILLI METRE]
    Gross Surface Area = 2.70870426 [SQUARE_METRE]
    Height = 2911.475 [MILLI METRE]
    Home Offset = 152.4 [MILLI METRE]
    Net Volume = 0.063864485174 [CUBIC_METRE]
    Nominal Height = 2911.475 [MILLI METRE]
    Nominal Surface Area = 2.51434981 [SQUARE_METRE]
    Nominal Width = 863.6 [MILLI METRE]
    Perimeter = 7550.15 [MILLI METRE]
    Surface Area = 2.51434981 [SQUARE_METRE]
    Thickness = 25.4 [MILLI METRE]
    Width = 863.6 [MILLI METRE]
  ArchiCADQuantities | quantities | on 59 objects (59 IFCBUILDINGELEMENTPROXY)
    Elevation to Project Zero = 6858. [MILLI METRE]
    Elevation to Reference Level 1 = 14478. [MILLI METRE]
    Elevation to Reference Level 2 = -762. [MILLI METRE]
    Elevation to Sea Level = 37338. [MILLI METRE]
    Elevation to Story = 3200.4 [MILLI METRE]
    Frame Depth = 152.4 [MILLI METRE]
    Frame Length = 406.4 [MILLI METRE]
    Home Offset = 3200.4 [MILLI METRE]
    Net Volume = 0.003146316288 [CUBIC_METRE]
    Surface Area = 0.00774192 [SQUARE_METRE]
    Width = 50.8 [MILLI METRE]
  ArchiCADQuantities: 865 more contents on 2296 objects not shown
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    FireRating = "Unrated" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    FireRating = "Unrated" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_SlabCommon | properties | on 3 objects (3 IFCSLAB)
    AcousticRating = "" (IFCLABEL)
    FireRating = "Unrated" (IFCLABEL)
  Pset_FireRatingProperties | properties | on 706 objects (534 IFCBEAM, 73 IFCCOLUMN, 61 IFCWALL, 14 IFCCOVERING)
    FireResistanceRating = "Unrated" (IFCLABEL)
  Pset_FireRatingProperties | properties | on 266 objects (237 IFCBUILDINGELEMENTPROXY, 24 IFCDOOR, 5 IFCWINDOW)
    FireResistanceRating = "" (IFCLABEL)
  Pset_BeamCommon | properties | on 476 objects (476 IFCBEAM)
    FireRating = "Unrated" (IFCLABEL)
  Pset_BeamCommon | properties | on 50 objects (50 IFCBEAM)
    FireRating = "Unrated" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "W18X50 7 1/2" x 18"" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 8 objects (8 IFCBEAM)
    FireRating = "Unrated" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_ColumnCommon | properties | on 73 objects (73 IFCCOLUMN)
    FireRating = "Unrated" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HP10X57 10 1/4" x 10"" (IFCIDENTIFIER)
  Pset_RailingCommon | properties | on 3 objects (3 IFCRAILING)
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_RailingCommon | properties | on 3 objects (3 IFCRAILING)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 26 objects (26 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    FireRating = "Unrated" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 24 objects (24 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    FireRating = "Unrated" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 11 objects (11 IFCWALL)
    AcousticRating = "" (IFCLABEL)
    FireRating = "Unrated" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_DoorWindowGlazingType | properties | on 25 objects (20 IFCDOOR, 5 IFCWINDOW)
    IsLaminated = FALSE (IFCBOOLEAN)
    IsTempered = FALSE (IFCBOOLEAN)
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.41210609453 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    SecurityRating = "Undefined" (IFCLABEL)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.412003145 (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    SecurityRating = "Undefined" (IFCLABEL)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0. (IFCPOSITIVERATIOMEASURE)
    IsExternal = TRUE (IFCBOOLEAN)
    SecurityRating = "Undefined" (IFCLABEL)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_ManufacturerOccurrence | properties | on 246 objects (237 IFCBUILDINGELEMENTPROXY, 5 IFCDOOR, 4 IFCWINDOW)
    SerialNumber = "Off" (IFCIDENTIFIER)
  Pset_ManufacturerOccurrence | properties | on 213 objects (118 IFCFLOWTERMINAL, 74 IFCFURNISHINGELEMENT, 19 IFCDOOR, 1 IFCTRANSPORTELEMENT)
    SerialNumber = "" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 459 objects (237 IFCBUILDINGELEMENTPROXY, 118 IFCFLOWTERMINAL, 74 IFCFURNISHINGELEMENT, 24 IFCDOOR)
    Manufacturer = "" (IFCLABEL)
    ProductionYear = "" (IFCLABEL)
  AC_Equantity_Storefront_Window_21 | quantities | on 3 objects (3 IFCWINDOW)
    AC Left Opening Oversize = 0. [MILLI METRE]
    AC Lower Opening Oversize = -0. [MILLI METRE]
    AC Right Opening Oversize = 0. [MILLI METRE]
    AC Upper Opening Oversize = 0. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Bottom Rail Width = 150. [MILLI METRE]
    Bottom Vert. Div. Width (0=No) = 300. [MILLI METRE]
    Butt Glazed Joint = 10. [MILLI METRE]
    Closer Thickness = 100. [MILLI METRE]
    Closer Width = 38. [MILLI METRE]
    Custom Thickness = 15. [MILLI METRE]
    Distance of Skin from Closer = 0. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame W. on Left Side = 50.8 [MILLI METRE]
    Frame W. on Right Side = 50.8 [MILLI METRE]
    Frame Width = 50.8 [MILLI METRE]
    Frame Width Lower = 150. [MILLI METRE]
    Frame Width Upper = 50.8 [MILLI METRE]
    Glass Setback = 19.05 [MILLI METRE]
    Glass Thickness = 12.7 [MILLI METRE]
    Head Jamb Depth = 60. [MILLI METRE]
    Height = 2848.16800625 [MILLI METRE]
    Horizontal Div. Width (0=No) = 304.8 [MILLI METRE]
    Horizontal Mullion Thickness = 50.8 [MILLI METRE]
    Horizontal Mullion Width = 38.1 [MILLI METRE]
    Inner Head Depth (gs_reveal_double_innerTop) = 60. [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 60. [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 60. [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 60. [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 60. [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 60. [MILLI METRE]
    Inner Sill Depth (gs_reveal_double_innerBottom) = 60. [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 60. [MILLI METRE]
    Jamb Depth = 60. [MILLI METRE]
    Jamb Depth Side 2 = 60. [MILLI METRE]
    Left Opening Oversize = 0. [MILLI METRE]
    Lower Opening Oversize = 0. [MILLI METRE]
    Middle Rail Elevation = 0. [MILLI METRE]
    Middle Rail Width = 150. [MILLI METRE]
    Middle Vert. Div. Width (0=No) = 304.8 [MILLI METRE]
    New Wall Fill Width Left = 150. [MILLI METRE]
    New Wall Fill Width Right = 150. [MILLI METRE]
    Outer Jamb Depth = 80. [MILLI METRE]
    Plaster Thickness Limit = 40. [MILLI METRE]
    Profile Height = 65. [MILLI METRE]
    Profile Thickness = 110. [MILLI METRE]
    Profile Width = 75. [MILLI METRE]
    Reveal Depth (AC_wido_sill) = 0. [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 0. [MILLI METRE]
    Reveal Height = 2848.16800625 [MILLI METRE]
    Reveal Width = 635. [MILLI METRE]
    Reveal to Wall Core = 0. [MILLI METRE]
    Right Opening Oversize = 0. [MILLI METRE]
    Sash Frame Thickness = 50.00625 [MILLI METRE]
    Sash Frame Width = 50. [MILLI METRE]
    Side Panel Width 1 = 0. [MILLI METRE]
    Side Panel Width 2 = 0. [MILLI METRE]
    Sill Height to Current Story = 263.524839793 [MILLI METRE]
    Sill Jamb Depth = 60. [MILLI METRE]
    Skin Overhang to Frame Depth = 0. [MILLI METRE]
    Strip Thickness = 25. [MILLI METRE]
    Tolerance = 0. [MILLI METRE]
    Tolerance Left = 0. [MILLI METRE]
    Tolerance Lower = 0. [MILLI METRE]
    Tolerance Right = 0. [MILLI METRE]
    Tolerance Upper = 0. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Top Vert. Div. Width (0=No) = 300. [MILLI METRE]
    Transom Height (middlePanelHeight) = 0. [MILLI METRE]
    Transom Height (transomHeight) = 0. [MILLI METRE]
    Unit Height = 2848.16800625 [MILLI METRE]
    Unit Width = 635. [MILLI METRE]
    Upper Opening Oversize = 0. [MILLI METRE]
    Vertical Mullion Thickness = 50.8 [MILLI METRE]
    Vertical Mullion Width = 38.1 [MILLI METRE]
    Wallhole Height = 2848.16800625 [MILLI METRE]
    Wallhole Width = 635. [MILLI METRE]
    Width = 635. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  AC_Equantity_Storefront_Window_21 | quantities | on 1 object (1 IFCWINDOW)
    AC Left Opening Oversize = 0. [MILLI METRE]
    AC Lower Opening Oversize = -0. [MILLI METRE]
    AC Right Opening Oversize = 0. [MILLI METRE]
    AC Upper Opening Oversize = 0. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Bottom Rail Width = 150. [MILLI METRE]
    Bottom Vert. Div. Width (0=No) = 300. [MILLI METRE]
    Butt Glazed Joint = 10. [MILLI METRE]
    Closer Thickness = 100. [MILLI METRE]
    Closer Width = 38. [MILLI METRE]
    Custom Thickness = 15. [MILLI METRE]
    Distance of Skin from Closer = 0. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame W. on Left Side = 50.8 [MILLI METRE]
    Frame W. on Right Side = 50.8 [MILLI METRE]
    Frame Width = 50.8 [MILLI METRE]
    Frame Width Lower = 150. [MILLI METRE]
    Frame Width Upper = 50.8 [MILLI METRE]
    Glass Setback = 19.05 [MILLI METRE]
    Glass Thickness = 12.7 [MILLI METRE]
    Head Jamb Depth = 60. [MILLI METRE]
    Height = 2847.975 [MILLI METRE]
    Horizontal Div. Width (0=No) = 304.8 [MILLI METRE]
    Horizontal Mullion Thickness = 50.8 [MILLI METRE]
    Horizontal Mullion Width = 38.1 [MILLI METRE]
    Inner Head Depth (gs_reveal_double_innerTop) = 60. [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 60. [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 60. [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 60. [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 60. [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 60. [MILLI METRE]
    Inner Sill Depth (gs_reveal_double_innerBottom) = 60. [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 60. [MILLI METRE]
    Jamb Depth = 60. [MILLI METRE]
    Jamb Depth Side 2 = 60. [MILLI METRE]
    Left Opening Oversize = 0. [MILLI METRE]
    Lower Opening Oversize = 0. [MILLI METRE]
    Middle Rail Elevation = 0. [MILLI METRE]
    Middle Rail Width = 150. [MILLI METRE]
    Middle Vert. Div. Width (0=No) = 304.8 [MILLI METRE]
    New Wall Fill Width Left = 150. [MILLI METRE]
    New Wall Fill Width Right = 150. [MILLI METRE]
    Outer Jamb Depth = 80. [MILLI METRE]
    Plaster Thickness Limit = 40. [MILLI METRE]
    Profile Height = 65. [MILLI METRE]
    Profile Thickness = 110. [MILLI METRE]
    Profile Width = 75. [MILLI METRE]
    Reveal Depth (AC_wido_sill) = 0. [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 0. [MILLI METRE]
    Reveal Height = 2847.975 [MILLI METRE]
    Reveal Width = 635. [MILLI METRE]
    Reveal to Wall Core = 0. [MILLI METRE]
    Right Opening Oversize = 0. [MILLI METRE]
    Sash Frame Thickness = 50.00625 [MILLI METRE]
    Sash Frame Width = 50. [MILLI METRE]
    Side Panel Width 1 = 0. [MILLI METRE]
    Side Panel Width 2 = 0. [MILLI METRE]
    Sill Height to Current Story = 263.525 [MILLI METRE]
    Sill Jamb Depth = 60. [MILLI METRE]
    Skin Overhang to Frame Depth = 0. [MILLI METRE]
    Strip Thickness = 25. [MILLI METRE]
    Tolerance = 0. [MILLI METRE]
    Tolerance Left = 0. [MILLI METRE]
    Tolerance Lower = 0. [MILLI METRE]
    Tolerance Right = 0. [MILLI METRE]
    Tolerance Upper = 0. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Top Vert. Div. Width (0=No) = 300. [MILLI METRE]
    Transom Height (middlePanelHeight) = 0. [MILLI METRE]
    Transom Height (transomHeight) = 0. [MILLI METRE]
    Unit Height = 2847.975 [MILLI METRE]
    Unit Width = 635. [MILLI METRE]
    Upper Opening Oversize = 0. [MILLI METRE]
    Vertical Mullion Thickness = 50.8 [MILLI METRE]
    Vertical Mullion Width = 38.1 [MILLI METRE]
    Wallhole Height = 2847.975 [MILLI METRE]
    Wallhole Width = 635. [MILLI METRE]
    Width = 635. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  Pset_DoorCommon | properties | on 15 objects (15 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0. (IFCPOSITIVERATIOMEASURE)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    SecurityRating = "Undefined" (IFCLABEL)
    SelfClosing = FALSE (IFCBOOLEAN)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 4 objects (4 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0. (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 3 objects (3 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.81677056 (IFCPOSITIVERATIOMEASURE)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    SecurityRating = "Undefined" (IFCLABEL)
    SelfClosing = FALSE (IFCBOOLEAN)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0. (IFCPOSITIVERATIOMEASURE)
    HandicapAccessible = TRUE (IFCBOOLEAN)
    SecurityRating = "Undefined" (IFCLABEL)
    SelfClosing = TRUE (IFCBOOLEAN)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0. (IFCPOSITIVERATIOMEASURE)
    HandicapAccessible = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    SecurityRating = "Undefined" (IFCLABEL)
    SelfClosing = FALSE (IFCBOOLEAN)
    SmokeStop = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  AC_Equantity_Storefront_Double_Door_21 | quantities | on 2 objects (2 IFCDOOR)
    AC Left Opening Oversize = 57.15 [MILLI METRE]
    AC Lower Opening Oversize = -0. [MILLI METRE]
    AC Right Opening Oversize = 57.15 [MILLI METRE]
    AC Upper Opening Oversize = 57.15 [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Bottom Rail Width = 152.4 [MILLI METRE]
    Bottom Vertical Div. Width (0-No) = 304.8 [MILLI METRE]
    Butt Glazed Joint = 10. [MILLI METRE]
    Closer Thickness = 100. [MILLI METRE]
    Closer Width = 38. [MILLI METRE]
    Custom Thickness = 15. [MILLI METRE]
    Distance of Skin from Closer = 0. [MILLI METRE]
    Door Stop Thickness = 50.8 [MILLI METRE]
    Door Stop Width = 12.7 [MILLI METRE]
    Egress Height = 2019.3 [MILLI METRE]
    Egress Width = 1498.6 [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Width = 50.8 [MILLI METRE]
    Glass Setback = 19.05 [MILLI METRE]
    Glass Thickness = 12.7 [MILLI METRE]
    Handle Distance from Leaf Edge Left = 35. [MILLI METRE]
    Handle Distance from Leaf Edge Right = 35. [MILLI METRE]
    Handle Height Left = 863.6 [MILLI METRE]
    Handle Height Right = 863.6 [MILLI METRE]
    Head Jamb Depth = 50.8 [MILLI METRE]
    Height = 2032. [MILLI METRE]
    Horizontal Division Width (0-No) = 304.8 [MILLI METRE]
    Horizontal Mullion Thickness = 50.8 [MILLI METRE]
    Horizontal Mullion Width = 38.1 [MILLI METRE]
    Inner Head Depth (gs_reveal_double_innerTop) = 101.6 [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 101.6 [MILLI METRE]
    Inner Sill Depth (gs_reveal_double_innerBottom) = 101.6 [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 101.6 [MILLI METRE]
    Jamb Depth = 50.8 [MILLI METRE]
    Jamb Depth Side 2 = 50.8 [MILLI METRE]
    Kick Board Height 2 = 100. [MILLI METRE]
    Kick Board Height = 100. [MILLI METRE]
    Leaf Frame Width = 101.6 [MILLI METRE]
    Leaf Frame Width Left = 50.8 [MILLI METRE]
    Leaf Frame Width Lower = 152.4 [MILLI METRE]
    Leaf Frame Width Right = 50.8 [MILLI METRE]
    Leaf Frame Width Upper = 50.8 [MILLI METRE]
    Leaf Height = 2032. [MILLI METRE]
    Leaf Thickness = 44.45 [MILLI METRE]
    Leaf Width = 1524. [MILLI METRE]
    Left Opening Oversize = 0. [MILLI METRE]
    Lower Opening Oversize = 0. [MILLI METRE]
    Middle Rail Elevation = 863.6 [MILLI METRE]
    Middle Rail Width = 152.4 [MILLI METRE]
    Middle Vertical Division Width (0-No) = 300. [MILLI METRE]
    New Wall Fill Width Left = 150. [MILLI METRE]
    New Wall Fill Width Right = 150. [MILLI METRE]
    Opening Side Depth = 1524. [MILLI METRE]
    Opening Side Width 1 = 0. [MILLI METRE]
    Opening Side Width 2 = 0. [MILLI METRE]
    Opposite Side Depth = 1219.2 [MILLI METRE]
    Opposite Side Width 1 = 0. [MILLI METRE]
    Opposite Side Width 2 = 0. [MILLI METRE]
    Outer Jamb Depth = 80. [MILLI METRE]
    Plaster Thickness Limit = 50.8 [MILLI METRE]
    Profile Height = 65. [MILLI METRE]
    Profile Thickness = 110. [MILLI METRE]
    Profile Width = 150. [MILLI METRE]
    Real Frame Thickness = 101.6 [MILLI METRE]
    Reveal Depth (AC_wido_sill) = 0. [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 0. [MILLI METRE]
    Reveal Height = 2089.15 [MILLI METRE]
    Reveal Width = 1638.3 [MILLI METRE]
    Reveal to Wall Core = 0. [MILLI METRE]
    Right Opening Oversize = 0. [MILLI METRE]
    Sidelight Width 1 = 0. [MILLI METRE]
    Sidelight Width 2 = 0. [MILLI METRE]
    Sill Height to Current Story = 212.725055714 [MILLI METRE]
    Sill Jamb Depth = 60. [MILLI METRE]
    Skin Overhang to Frame Depth = 0. [MILLI METRE]
    Strip Thickness = 25. [MILLI METRE]
    Tolerance Left = 6.35 [MILLI METRE]
    Tolerance Lower = 0. [MILLI METRE]
    Tolerance Right = 6.35 [MILLI METRE]
    Tolerance Upper = 6.35 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Height (gs_transom_height) = 0. [MILLI METRE]
    Transom Height (middlePanelHeight) = 0. [MILLI METRE]
    Transom Vertical Division Width (0-No) = 304.8 [MILLI METRE]
    Unit Height = 2082.8 [MILLI METRE]
    Unit Width = 1625.6 [MILLI METRE]
    Upper Opening Oversize = 0. [MILLI METRE]
    Vertical Mullion Thickness = 50.8 [MILLI METRE]
    Vertical Mullion Width = 38.1 [MILLI METRE]
    Wallhole Height = 2089.15 [MILLI METRE]
    Wallhole Width = 1638.3 [MILLI METRE]
    Width = 1524. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  AC_Equantity_Storefront_Double_Door_21 | quantities | on 1 object (1 IFCDOOR)
    AC Left Opening Oversize = 57.15 [MILLI METRE]
    AC Lower Opening Oversize = -0. [MILLI METRE]
    AC Right Opening Oversize = 57.15 [MILLI METRE]
    AC Upper Opening Oversize = 57.15 [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Bottom Rail Width = 152.4 [MILLI METRE]
    Bottom Vertical Div. Width (0-No) = 304.8 [MILLI METRE]
    Butt Glazed Joint = 10. [MILLI METRE]
    Closer Thickness = 100. [MILLI METRE]
    Closer Width = 38. [MILLI METRE]
    Custom Thickness = 15. [MILLI METRE]
    Distance of Skin from Closer = 0. [MILLI METRE]
    Door Stop Thickness = 50.8 [MILLI METRE]
    Door Stop Width = 12.7 [MILLI METRE]
    Egress Height = 2019.3 [MILLI METRE]
    Egress Width = 1498.6 [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Width = 50.8 [MILLI METRE]
    Glass Setback = 19.05 [MILLI METRE]
    Glass Thickness = 12.7 [MILLI METRE]
    Handle Distance from Leaf Edge Left = 35. [MILLI METRE]
    Handle Distance from Leaf Edge Right = 35. [MILLI METRE]
    Handle Height Left = 863.6 [MILLI METRE]
    Handle Height Right = 863.6 [MILLI METRE]
    Head Jamb Depth = 50.8 [MILLI METRE]
    Height = 2032. [MILLI METRE]
    Horizontal Division Width (0-No) = 304.8 [MILLI METRE]
    Horizontal Mullion Thickness = 50.8 [MILLI METRE]
    Horizontal Mullion Width = 38.1 [MILLI METRE]
    Inner Head Depth (gs_reveal_double_innerTop) = 101.6 [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 101.6 [MILLI METRE]
    Inner Sill Depth (gs_reveal_double_innerBottom) = 101.6 [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 101.6 [MILLI METRE]
    Jamb Depth = 50.8 [MILLI METRE]
    Jamb Depth Side 2 = 50.8 [MILLI METRE]
    Kick Board Height 2 = 100. [MILLI METRE]
    Kick Board Height = 100. [MILLI METRE]
    Leaf Frame Width = 101.6 [MILLI METRE]
    Leaf Frame Width Left = 50.8 [MILLI METRE]
    Leaf Frame Width Lower = 152.4 [MILLI METRE]
    Leaf Frame Width Right = 50.8 [MILLI METRE]
    Leaf Frame Width Upper = 50.8 [MILLI METRE]
    Leaf Height = 2032. [MILLI METRE]
    Leaf Thickness = 44.45 [MILLI METRE]
    Leaf Width = 1524. [MILLI METRE]
    Left Opening Oversize = 0. [MILLI METRE]
    Lower Opening Oversize = 0. [MILLI METRE]
    Middle Rail Elevation = 863.6 [MILLI METRE]
    Middle Rail Width = 152.4 [MILLI METRE]
    Middle Vertical Division Width (0-No) = 300. [MILLI METRE]
    New Wall Fill Width Left = 150. [MILLI METRE]
    New Wall Fill Width Right = 150. [MILLI METRE]
    Opening Side Depth = 1524. [MILLI METRE]
    Opening Side Width 1 = 0. [MILLI METRE]
    Opening Side Width 2 = 0. [MILLI METRE]
    Opposite Side Depth = 1219.2 [MILLI METRE]
    Opposite Side Width 1 = 0. [MILLI METRE]
    Opposite Side Width 2 = 0. [MILLI METRE]
    Outer Jamb Depth = 80. [MILLI METRE]
    Plaster Thickness Limit = 50.8 [MILLI METRE]
    Profile Height = 65. [MILLI METRE]
    Profile Thickness = 110. [MILLI METRE]
    Profile Width = 150. [MILLI METRE]
    Real Frame Thickness = 101.6 [MILLI METRE]
    Reveal Depth (AC_wido_sill) = 0. [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 0. [MILLI METRE]
    Reveal Height = 2089.15 [MILLI METRE]
    Reveal Width = 1638.3 [MILLI METRE]
    Reveal to Wall Core = 0. [MILLI METRE]
    Right Opening Oversize = 0. [MILLI METRE]
    Sidelight Width 1 = 0. [MILLI METRE]
    Sidelight Width 2 = 0. [MILLI METRE]
    Sill Height to Current Story = 263.525 [MILLI METRE]
    Sill Jamb Depth = 60. [MILLI METRE]
    Skin Overhang to Frame Depth = 0. [MILLI METRE]
    Strip Thickness = 25. [MILLI METRE]
    Tolerance Left = 6.35 [MILLI METRE]
    Tolerance Lower = 0. [MILLI METRE]
    Tolerance Right = 6.35 [MILLI METRE]
    Tolerance Upper = 6.35 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Height (gs_transom_height) = 0. [MILLI METRE]
    Transom Height (middlePanelHeight) = 0. [MILLI METRE]
    Transom Vertical Division Width (0-No) = 304.8 [MILLI METRE]
    Unit Height = 2082.8 [MILLI METRE]
    Unit Width = 1625.6 [MILLI METRE]
    Upper Opening Oversize = 0. [MILLI METRE]
    Vertical Mullion Thickness = 50.8 [MILLI METRE]
    Vertical Mullion Width = 38.1 [MILLI METRE]
    Wallhole Height = 2089.15 [MILLI METRE]
    Wallhole Width = 1638.3 [MILLI METRE]
    Width = 1524. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
  Pset_CurtainWallCommon | properties | on 4 objects (4 IFCCURTAINWALL)
    AcousticRating = "" (IFCLABEL)
    FireRating = "Unrated" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
  Pset_PrecastConcreteElementGeneral | properties | on 237 objects (237 IFCBUILDINGELEMENTPROXY)
    SerialNumber = "Off" (IFCIDENTIFIER)
  AC_Equantity_CW_Panel_21 | quantities | on 204 objects (204 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Coating Thickness = 6. [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 381. [MILLI METRE]
    Nominal Height = 381. [MILLI METRE]
    Nominal Width = 863.6 [MILLI METRE]
    Panel Thickness = 80. [MILLI METRE]
    Thickness = 80. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 863.6 [MILLI METRE]
  AC_Equantity_CW_Panel_21 | quantities | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Coating Thickness = 6. [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 381. [MILLI METRE]
    Nominal Height = 381. [MILLI METRE]
    Nominal Width = 599.078975516 [MILLI METRE]
    Panel Thickness = 80. [MILLI METRE]
    Thickness = 80. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 599.078975516 [MILLI METRE]
  AC_Equantity_CW_Panel_21 | quantities | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Coating Thickness = 6. [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 381. [MILLI METRE]
    Nominal Height = 381. [MILLI METRE]
    Nominal Width = 427.311475516 [MILLI METRE]
    Panel Thickness = 80. [MILLI METRE]
    Thickness = 80. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 427.311475516 [MILLI METRE]
  AC_Equantity_CW_Panel_21 | quantities | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Coating Thickness = 6. [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 381. [MILLI METRE]
    Nominal Height = 381. [MILLI METRE]
    Nominal Width = 412.432594613 [MILLI METRE]
    Panel Thickness = 80. [MILLI METRE]
    Thickness = 80. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 412.432594613 [MILLI METRE]
  AC_Equantity_CW_Panel_21 | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Coating Thickness = 6. [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 381. [MILLI METRE]
    Nominal Height = 381. [MILLI METRE]
    Nominal Width = 144.418975516 [MILLI METRE]
    Panel Thickness = 80. [MILLI METRE]
    Thickness = 80. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 144.418975516 [MILLI METRE]
  AC_Equantity_CW_Panel_21 | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Coating Thickness = 6. [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 381. [MILLI METRE]
    Nominal Height = 381. [MILLI METRE]
    Nominal Width = 144.472392945 [MILLI METRE]
    Panel Thickness = 80. [MILLI METRE]
    Thickness = 80. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 144.472392945 [MILLI METRE]
  AC_Equantity_CW_Panel_21 | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Coating Thickness = 6. [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 381. [MILLI METRE]
    Nominal Height = 381. [MILLI METRE]
    Nominal Width = 144.447202907 [MILLI METRE]
    Panel Thickness = 80. [MILLI METRE]
    Thickness = 80. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 144.447202907 [MILLI METRE]
  AC_Equantity_CW_Panel_21 | quantities | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Coating Thickness = 6. [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 381. [MILLI METRE]
    Nominal Height = 381. [MILLI METRE]
    Nominal Width = 426.070592574 [MILLI METRE]
    Panel Thickness = 80. [MILLI METRE]
    Thickness = 80. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 426.070592574 [MILLI METRE]
  AC_Equantity_CW_Panel_21: 5 more contents on 5 objects not shown
  AC_Equantity_CW_Double_Door_21 | quantities | on 2 objects (2 IFCDOOR)
    Adapter Thickness = 40. [MILLI METRE]
    Adapter Width = 25. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Frame Recess Thickness = 50. [MILLI METRE]
    Frame Recess Width = 25. [MILLI METRE]
    Frame Thickness = 55. [MILLI METRE]
    Frame Width = 45. [MILLI METRE]
    Glass Offset = 10. [MILLI METRE]
    Glass Thickness = 16. [MILLI METRE]
    Glass from Bottom = 1000. [MILLI METRE]
    Glass from Left = 300. [MILLI METRE]
    Glass from Right = 300. [MILLI METRE]
    Glass from Top = 300. [MILLI METRE]
    Grill Thickness = 20. [MILLI METRE]
    Grill Width Horizontal 1 = 10. [MILLI METRE]
    Grill Width Horizontal 2 = 10. [MILLI METRE]
    Grill Width Vertical 1 = 10. [MILLI METRE]
    Grill Width Vertical 2 = 10. [MILLI METRE]
    Handle Height = 1000. [MILLI METRE]
    Handle Position = 50. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 2911.475 [MILLI METRE]
    Leaf Frame Thickness = 55. [MILLI METRE]
    Leaf Frame Width = 120. [MILLI METRE]
    Nominal Height = 2911.475 [MILLI METRE]
    Nominal Width = 1778. [MILLI METRE]
    Panel Offset = 0. [MILLI METRE]
    Thickness = 55. [MILLI METRE]
    Threshold Height = 25. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 1778. [MILLI METRE]
  AC_Equantity_CW_Double_Door_21 | quantities | on 1 object (1 IFCDOOR)
    Adapter Thickness = 40. [MILLI METRE]
    Adapter Width = 25. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Frame Recess Thickness = 50. [MILLI METRE]
    Frame Recess Width = 25. [MILLI METRE]
    Frame Thickness = 55. [MILLI METRE]
    Frame Width = 45. [MILLI METRE]
    Glass Offset = 10. [MILLI METRE]
    Glass Thickness = 16. [MILLI METRE]
    Glass from Bottom = 1000. [MILLI METRE]
    Glass from Left = 300. [MILLI METRE]
    Glass from Right = 300. [MILLI METRE]
    Glass from Top = 300. [MILLI METRE]
    Grill Thickness = 20. [MILLI METRE]
    Grill Width Horizontal 1 = 10. [MILLI METRE]
    Grill Width Horizontal 2 = 10. [MILLI METRE]
    Grill Width Vertical 1 = 10. [MILLI METRE]
    Grill Width Vertical 2 = 10. [MILLI METRE]
    Handle Height = 1000. [MILLI METRE]
    Handle Position = 50. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 2971.8 [MILLI METRE]
    Leaf Frame Thickness = 55. [MILLI METRE]
    Leaf Frame Width = 120. [MILLI METRE]
    Nominal Height = 2971.8 [MILLI METRE]
    Nominal Width = 1325.61680738 [MILLI METRE]
    Panel Offset = 0. [MILLI METRE]
    Thickness = 55. [MILLI METRE]
    Threshold Height = 25. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 1325.61680738 [MILLI METRE]
  AC_Equantity_CW_Double_Door_21 | quantities | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Adapter Thickness = 40. [MILLI METRE]
    Adapter Width = 25. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Frame Recess Thickness = 50. [MILLI METRE]
    Frame Recess Width = 25. [MILLI METRE]
    Frame Thickness = 55. [MILLI METRE]
    Frame Width = 45. [MILLI METRE]
    Glass Offset = 10. [MILLI METRE]
    Glass Thickness = 16. [MILLI METRE]
    Glass from Bottom = 1000. [MILLI METRE]
    Glass from Left = 300. [MILLI METRE]
    Glass from Right = 300. [MILLI METRE]
    Glass from Top = 300. [MILLI METRE]
    Grill Thickness = 20. [MILLI METRE]
    Grill Width Horizontal 1 = 10. [MILLI METRE]
    Grill Width Horizontal 2 = 10. [MILLI METRE]
    Grill Width Vertical 1 = 10. [MILLI METRE]
    Grill Width Vertical 2 = 10. [MILLI METRE]
    Handle Height = 1000. [MILLI METRE]
    Handle Position = 50. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 2971.8 [MILLI METRE]
    Leaf Frame Thickness = 55. [MILLI METRE]
    Leaf Frame Width = 120. [MILLI METRE]
    Nominal Height = 2971.8 [MILLI METRE]
    Nominal Width = 1778. [MILLI METRE]
    Panel Offset = 0. [MILLI METRE]
    Thickness = 55. [MILLI METRE]
    Threshold Height = 25. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 1778. [MILLI METRE]
  AC_Equantity_CW_Double_Door_21 | quantities | on 1 object (1 IFCDOOR)
    Adapter Thickness = 40. [MILLI METRE]
    Adapter Width = 25. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Frame Recess Thickness = 50. [MILLI METRE]
    Frame Recess Width = 25. [MILLI METRE]
    Frame Thickness = 55. [MILLI METRE]
    Frame Width = 45. [MILLI METRE]
    Glass Offset = 10. [MILLI METRE]
    Glass Thickness = 16. [MILLI METRE]
    Glass from Bottom = 1000. [MILLI METRE]
    Glass from Left = 300. [MILLI METRE]
    Glass from Right = 300. [MILLI METRE]
    Glass from Top = 300. [MILLI METRE]
    Grill Thickness = 20. [MILLI METRE]
    Grill Width Horizontal 1 = 10. [MILLI METRE]
    Grill Width Horizontal 2 = 10. [MILLI METRE]
    Grill Width Vertical 1 = 10. [MILLI METRE]
    Grill Width Vertical 2 = 10. [MILLI METRE]
    Handle Height = 1000. [MILLI METRE]
    Handle Position = 50. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 2971.8 [MILLI METRE]
    Leaf Frame Thickness = 55. [MILLI METRE]
    Leaf Frame Width = 120. [MILLI METRE]
    Nominal Height = 2971.8 [MILLI METRE]
    Nominal Width = 1513.47897552 [MILLI METRE]
    Panel Offset = 0. [MILLI METRE]
    Thickness = 55. [MILLI METRE]
    Threshold Height = 25. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 1513.47897552 [MILLI METRE]
  IfcDoorPanelProperties | properties | on 1 object (1 IFCDOOR)
    Panel Operation = "REVOLVING" (IFCLABEL)
  AC_Equantity_CW_Door_Revolving_21 | quantities | on 1 object (1 IFCDOOR)
    Bottom Level = 1000. [MILLI METRE]
    Clamp Width = 25.4 [MILLI METRE]
    Dimension 1 = 1000. [MILLI METRE]
    Dimension 2 = 1000. [MILLI METRE]
    Frame Thickness = 55. [MILLI METRE]
    Frame Width = 45. [MILLI METRE]
    Glazing Thickness = 16. [MILLI METRE]
    Height (ZZYZX) = 1000. [MILLI METRE]
    Height (ac_height) = 2911.475 [MILLI METRE]
    Leaf Thickness = 55. [MILLI METRE]
    Leaf Width = 120. [MILLI METRE]
    Nominal Height = 2911.475 [MILLI METRE]
    Nominal Width = 1778. [MILLI METRE]
    Panel Offset = 0. [MILLI METRE]
    Thickness = 55. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width = 1778. [MILLI METRE]
  Pset_CoveringCommon | properties | on 5 objects (5 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    FireRating = "Unrated" (IFCLABEL)
    Material = "Demo Tiles Flooring" (IFCLABEL)
  Pset_CoveringCommon | properties | on 4 objects (4 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    FireRating = "Unrated" (IFCLABEL)
    Material = "Demo Carpet Floor" (IFCLABEL)
  Pset_CoveringCommon | properties | on 3 objects (3 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    FireRating = "Unrated" (IFCLABEL)
    Material = "Demo Terrace Flooring copy" (IFCLABEL)
  Pset_CoveringCommon | properties | on 2 objects (2 IFCCOVERING)
    AcousticRating = "" (IFCLABEL)
    FireRating = "Unrated" (IFCLABEL)
    Material = "Demo 1st Floor Flooring" (IFCLABEL)
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "Unrated" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 19. (IFCCOUNTMEASURE)
    NumberOfTreads = 19. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 189.330263158 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "Unrated" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 19. (IFCCOUNTMEASURE)
    NumberOfTreads = 19. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 192.505260226 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  Pset_StairCommon | properties | on 1 object (1 IFCSTAIR)
    FireRating = "Unrated" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    NumberOfRiser = 19. (IFCCOUNTMEASURE)
    NumberOfTreads = 19. (IFCCOUNTMEASURE)
    RequiredHeadroom = 2000. (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
    RiserHeight = 192.505263158 (IFCPOSITIVELENGTHMEASURE) [MILLI METRE]
  AC_Equantity_Elevator_21 | quantities | on 1 object (1 IFCTRANSPORTELEMENT)
    Bottom Level = 0. [MILLI METRE]
    Car Depth = 1738. [MILLI METRE]
    Car Height = 2286. [MILLI METRE]
    Car Inner Depth = 1797.42278451 [MILLI METRE]
    Car Inner Width = 1486.4432539 [MILLI METRE]
    Car Width = 2235.2 [MILLI METRE]
    Clear Opening Height = 2082.8 [MILLI METRE]
    Clear Opening Width = 914.4 [MILLI METRE]
    Depth of Counter Weight = 20. [MILLI METRE]
    Door Axis from Center = 0. [MILLI METRE]
    Elevation of Edited Story = 7315.2 [MILLI METRE]
    Elevator Shaft Depth = 2362.2 [MILLI METRE]
    Elevator Shaft Inner Depth = 2342.2 [MILLI METRE]
    Elevator Shaft Inner Width = 1726.25 [MILLI METRE]
    Elevator Shaft Thickness = 10. [MILLI METRE]
    Elevator Shaft Width = 1746.25 [MILLI METRE]
    Elevator Wall Thickness = 150. [MILLI METRE]
    Height = 14630.4 [MILLI METRE]
    Height of Edited Story = 3657.6 [MILLI METRE]
    Maximum Height of Structural Floor = 1828.8 [MILLI METRE]
    Overrun Height = 304.8 [MILLI METRE]
    Pit Depth = 990.6 [MILLI METRE]
    Pit Slab Thickness = 609.6 [MILLI METRE]
    Second Door Axis from Center = 0. [MILLI METRE]
    Split-Level Story Distance to Normal Story = 1524. [MILLI METRE]
    Top Level = 14630.4 [MILLI METRE]
    Top Slab Thickness = 101.6 [MILLI METRE]
    Wall Overhang = 120. [MILLI METRE]
    Width of Counter Weight = 914.4 [MILLI METRE]
  Pset_SpaceCommon | properties | on 15 objects (15 IFCSPACE)
    Category = "Toilette" (IFCLABEL)
    Reference = "Undefined" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 7 objects (7 IFCSPACE)
    Category = "Unconditioned Space" (IFCLABEL)
    Reference = "Undefined" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 6 objects (6 IFCSPACE)
    Category = "General" (IFCLABEL)
    Reference = "Undefined" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 3 objects (3 IFCSPACE)
    Category = "Office" (IFCLABEL)
    Reference = "Undefined" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 2 objects (2 IFCSPACE)
    Category = "Kitchen" (IFCLABEL)
    Reference = "Undefined" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Entry" (IFCLABEL)
    Reference = "Undefined" (IFCIDENTIFIER)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    Category = "Café" (IFCLABEL)
    Reference = "Undefined" (IFCIDENTIFIER)
  Pset_SpaceThermalDesign | properties | on 35 objects (35 IFCSPACE)
    VentilationAirFlowrate = 5. (IFCVOLUMETRICFLOWRATEMEASURE)
  Pset_SpaceThermalRequirements | properties | on 35 objects (35 IFCSPACE)
    SpaceTemperatureMax = 68. (IFCTHERMODYNAMICTEMPERATUREMEASURE) [DEGREE_CELSIUS]
  AC_Equantity_Zone_Stamp_02_21 | quantities | on 2 objects (2 IFCSPACE)
    Apartment ID Position (X) = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:50 = 0. [MILLI METRE]
    Apartment ID Position (Y) = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:50 = 0. [MILLI METRE]
    Circle Temp Radius = 150. [MILLI METRE]
    Combined Width of Doors = 0. [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_0) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_100) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_200) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_50) = 200. [MILLI METRE]
    Floor Level = 203.2 [MILLI METRE]
    Height = 3454.4 [MILLI METRE]
    Length of Perimeter Walls = 4410.4996151 [MILLI METRE]
    Net Perimeter = 5194.50437929 [MILLI METRE]
    Perimeter = 5194.50437929 [MILLI METRE]
    Perimeter of Holes = 0. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_0) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_100) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_200) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_50) = 1500. [MILLI METRE]
    Pointer Offset X = 0. [MILLI METRE]
    Pointer Offset X in 1:100 = 0. [MILLI METRE]
    Pointer Offset X in 1:200 = 0. [MILLI METRE]
    Pointer Offset X in 1:50 = 0. [MILLI METRE]
    Pointer Offset Y = 0. [MILLI METRE]
    Pointer Offset Y in 1:100 = 0. [MILLI METRE]
    Pointer Offset Y in 1:200 = 0. [MILLI METRE]
    Pointer Offset Y in 1:50 = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
    X Distance = 0. [MILLI METRE]
    X Distance in 1:100 = 0. [MILLI METRE]
    X Distance in 1:200 = 0. [MILLI METRE]
    X Distance in 1:50 = 0. [MILLI METRE]
    Y Distance = 0. [MILLI METRE]
    Y Distance in 1:100 = 0. [MILLI METRE]
    Y Distance in 1:200 = 0. [MILLI METRE]
    Y Distance in 1:50 = 0. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_0) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_100) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_200) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_50) = 250. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_0) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_100) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_200) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_50) = 200. [MILLI METRE]
  AC_Equantity_Zone_Stamp_02_21 | quantities | on 2 objects (2 IFCSPACE)
    Apartment ID Position (X) = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:50 = 0. [MILLI METRE]
    Apartment ID Position (Y) = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:50 = 0. [MILLI METRE]
    Circle Temp Radius = 150. [MILLI METRE]
    Combined Width of Doors = 1746.25 [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_0) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_100) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_200) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_50) = 200. [MILLI METRE]
    Floor Level = 263.524839793 [MILLI METRE]
    Height = 3657.6 [MILLI METRE]
    Length of Perimeter Walls = 7912.1 [MILLI METRE]
    Net Perimeter = 7912.1 [MILLI METRE]
    Perimeter = 7912.1 [MILLI METRE]
    Perimeter of Holes = 0. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_0) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_100) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_200) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_50) = 1500. [MILLI METRE]
    Pointer Offset X = 0. [MILLI METRE]
    Pointer Offset X in 1:100 = 0. [MILLI METRE]
    Pointer Offset X in 1:200 = 0. [MILLI METRE]
    Pointer Offset X in 1:50 = 0. [MILLI METRE]
    Pointer Offset Y = 0. [MILLI METRE]
    Pointer Offset Y in 1:100 = 0. [MILLI METRE]
    Pointer Offset Y in 1:200 = 0. [MILLI METRE]
    Pointer Offset Y in 1:50 = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
    X Distance = 0. [MILLI METRE]
    X Distance in 1:100 = 0. [MILLI METRE]
    X Distance in 1:200 = 0. [MILLI METRE]
    X Distance in 1:50 = 0. [MILLI METRE]
    Y Distance = 0. [MILLI METRE]
    Y Distance in 1:100 = 0. [MILLI METRE]
    Y Distance in 1:200 = 0. [MILLI METRE]
    Y Distance in 1:50 = 0. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_0) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_100) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_200) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_50) = 250. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_0) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_100) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_200) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_50) = 200. [MILLI METRE]
  AC_Equantity_Zone_Stamp_02_21 | quantities | on 1 object (1 IFCSPACE)
    Apartment ID Position (X) = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:50 = 0. [MILLI METRE]
    Apartment ID Position (Y) = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:50 = 0. [MILLI METRE]
    Circle Temp Radius = 150. [MILLI METRE]
    Combined Width of Doors = 1746.25 [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_0) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_100) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_200) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_50) = 200. [MILLI METRE]
    Floor Level = -711.199944286 [MILLI METRE]
    Height = 4632.32478408 [MILLI METRE]
    Length of Perimeter Walls = 7912.1 [MILLI METRE]
    Net Perimeter = 7912.1 [MILLI METRE]
    Perimeter = 7912.1 [MILLI METRE]
    Perimeter of Holes = 0. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_0) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_100) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_200) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_50) = 1500. [MILLI METRE]
    Pointer Offset X = 0. [MILLI METRE]
    Pointer Offset X in 1:100 = 0. [MILLI METRE]
    Pointer Offset X in 1:200 = 0. [MILLI METRE]
    Pointer Offset X in 1:50 = 0. [MILLI METRE]
    Pointer Offset Y = 0. [MILLI METRE]
    Pointer Offset Y in 1:100 = 0. [MILLI METRE]
    Pointer Offset Y in 1:200 = 0. [MILLI METRE]
    Pointer Offset Y in 1:50 = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
    X Distance = 0. [MILLI METRE]
    X Distance in 1:100 = 0. [MILLI METRE]
    X Distance in 1:200 = 0. [MILLI METRE]
    X Distance in 1:50 = 0. [MILLI METRE]
    Y Distance = 0. [MILLI METRE]
    Y Distance in 1:100 = 0. [MILLI METRE]
    Y Distance in 1:200 = 0. [MILLI METRE]
    Y Distance in 1:50 = 0. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_0) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_100) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_200) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_50) = 250. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_0) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_100) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_200) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_50) = 200. [MILLI METRE]
  AC_Equantity_Zone_Stamp_02_21 | quantities | on 1 object (1 IFCSPACE)
    Apartment ID Position (X) = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:50 = 0. [MILLI METRE]
    Apartment ID Position (Y) = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:50 = 0. [MILLI METRE]
    Circle Temp Radius = 150. [MILLI METRE]
    Combined Width of Doors = 6798.95037397 [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_0) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_100) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_200) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_50) = 200. [MILLI METRE]
    Floor Level = 263.525 [MILLI METRE]
    Height = 3394.075 [MILLI METRE]
    Length of Perimeter Walls = 5756.275 [MILLI METRE]
    Net Perimeter = 34505.0203487 [MILLI METRE]
    Perimeter = 34505.0203487 [MILLI METRE]
    Perimeter of Holes = 1515.62050257 [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_0) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_100) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_200) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_50) = 1500. [MILLI METRE]
    Pointer Offset X = 0. [MILLI METRE]
    Pointer Offset X in 1:100 = 0. [MILLI METRE]
    Pointer Offset X in 1:200 = 0. [MILLI METRE]
    Pointer Offset X in 1:50 = 0. [MILLI METRE]
    Pointer Offset Y = 0. [MILLI METRE]
    Pointer Offset Y in 1:100 = 0. [MILLI METRE]
    Pointer Offset Y in 1:200 = 0. [MILLI METRE]
    Pointer Offset Y in 1:50 = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
    X Distance = 0. [MILLI METRE]
    X Distance in 1:100 = 0. [MILLI METRE]
    X Distance in 1:200 = 0. [MILLI METRE]
    X Distance in 1:50 = 0. [MILLI METRE]
    Y Distance = 0. [MILLI METRE]
    Y Distance in 1:100 = 0. [MILLI METRE]
    Y Distance in 1:200 = 0. [MILLI METRE]
    Y Distance in 1:50 = 0. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_0) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_100) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_200) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_50) = 250. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_0) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_100) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_200) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_50) = 200. [MILLI METRE]
  AC_Equantity_Zone_Stamp_02_21 | quantities | on 1 object (1 IFCSPACE)
    Apartment ID Position (X) = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:50 = 0. [MILLI METRE]
    Apartment ID Position (Y) = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:50 = 0. [MILLI METRE]
    Circle Temp Radius = 150. [MILLI METRE]
    Combined Width of Doors = 0. [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_0) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_100) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_200) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_50) = 200. [MILLI METRE]
    Floor Level = 152.399942444 [MILLI METRE]
    Height = 3454.40005756 [MILLI METRE]
    Length of Perimeter Walls = 4410.4996151 [MILLI METRE]
    Net Perimeter = 5194.50437929 [MILLI METRE]
    Perimeter = 5194.50437929 [MILLI METRE]
    Perimeter of Holes = 0. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_0) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_100) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_200) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_50) = 1500. [MILLI METRE]
    Pointer Offset X = 0. [MILLI METRE]
    Pointer Offset X in 1:100 = 0. [MILLI METRE]
    Pointer Offset X in 1:200 = 0. [MILLI METRE]
    Pointer Offset X in 1:50 = 0. [MILLI METRE]
    Pointer Offset Y = 0. [MILLI METRE]
    Pointer Offset Y in 1:100 = 0. [MILLI METRE]
    Pointer Offset Y in 1:200 = 0. [MILLI METRE]
    Pointer Offset Y in 1:50 = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
    X Distance = 0. [MILLI METRE]
    X Distance in 1:100 = 0. [MILLI METRE]
    X Distance in 1:200 = 0. [MILLI METRE]
    X Distance in 1:50 = 0. [MILLI METRE]
    Y Distance = 0. [MILLI METRE]
    Y Distance in 1:100 = 0. [MILLI METRE]
    Y Distance in 1:200 = 0. [MILLI METRE]
    Y Distance in 1:50 = 0. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_0) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_100) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_200) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_50) = 250. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_0) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_100) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_200) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_50) = 200. [MILLI METRE]
  AC_Equantity_Zone_Stamp_02_21 | quantities | on 1 object (1 IFCSPACE)
    Apartment ID Position (X) = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:50 = 0. [MILLI METRE]
    Apartment ID Position (Y) = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:50 = 0. [MILLI METRE]
    Circle Temp Radius = 150. [MILLI METRE]
    Combined Width of Doors = 3524.2739904 [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_0) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_100) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_200) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_50) = 200. [MILLI METRE]
    Floor Level = 263.525 [MILLI METRE]
    Height = 3394.075 [MILLI METRE]
    Length of Perimeter Walls = 0. [MILLI METRE]
    Net Perimeter = 45107.8559212 [MILLI METRE]
    Perimeter = 45107.8559212 [MILLI METRE]
    Perimeter of Holes = 3031.24065175 [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_0) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_100) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_200) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_50) = 1500. [MILLI METRE]
    Pointer Offset X = 0. [MILLI METRE]
    Pointer Offset X in 1:100 = 0. [MILLI METRE]
    Pointer Offset X in 1:200 = 0. [MILLI METRE]
    Pointer Offset X in 1:50 = 0. [MILLI METRE]
    Pointer Offset Y = 0. [MILLI METRE]
    Pointer Offset Y in 1:100 = 0. [MILLI METRE]
    Pointer Offset Y in 1:200 = 0. [MILLI METRE]
    Pointer Offset Y in 1:50 = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
    X Distance = 0. [MILLI METRE]
    X Distance in 1:100 = 0. [MILLI METRE]
    X Distance in 1:200 = 0. [MILLI METRE]
    X Distance in 1:50 = 0. [MILLI METRE]
    Y Distance = 0. [MILLI METRE]
    Y Distance in 1:100 = 0. [MILLI METRE]
    Y Distance in 1:200 = 0. [MILLI METRE]
    Y Distance in 1:50 = 0. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_0) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_100) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_200) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_50) = 250. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_0) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_100) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_200) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_50) = 200. [MILLI METRE]
  AC_Equantity_Zone_Stamp_02_21 | quantities | on 1 object (1 IFCSPACE)
    Apartment ID Position (X) = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:50 = 0. [MILLI METRE]
    Apartment ID Position (Y) = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:50 = 0. [MILLI METRE]
    Circle Temp Radius = 150. [MILLI METRE]
    Combined Width of Doors = 3270.25 [MILLI METRE]
    Combined Width of Windows = 635. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_0) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_100) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_200) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_50) = 200. [MILLI METRE]
    Floor Level = 263.525 [MILLI METRE]
    Height = 3394.075 [MILLI METRE]
    Length of Perimeter Walls = 31166.5937631 [MILLI METRE]
    Net Perimeter = 28105.1000193 [MILLI METRE]
    Perimeter = 28105.1000193 [MILLI METRE]
    Perimeter of Holes = 9131.29994947 [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_0) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_100) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_200) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_50) = 1500. [MILLI METRE]
    Pointer Offset X = 0. [MILLI METRE]
    Pointer Offset X in 1:100 = 0. [MILLI METRE]
    Pointer Offset X in 1:200 = 0. [MILLI METRE]
    Pointer Offset X in 1:50 = 0. [MILLI METRE]
    Pointer Offset Y = 0. [MILLI METRE]
    Pointer Offset Y in 1:100 = 0. [MILLI METRE]
    Pointer Offset Y in 1:200 = 0. [MILLI METRE]
    Pointer Offset Y in 1:50 = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
    X Distance = 0. [MILLI METRE]
    X Distance in 1:100 = 0. [MILLI METRE]
    X Distance in 1:200 = 0. [MILLI METRE]
    X Distance in 1:50 = 0. [MILLI METRE]
    Y Distance = 0. [MILLI METRE]
    Y Distance in 1:100 = 0. [MILLI METRE]
    Y Distance in 1:200 = 0. [MILLI METRE]
    Y Distance in 1:50 = 0. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_0) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_100) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_200) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_50) = 250. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_0) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_100) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_200) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_50) = 200. [MILLI METRE]
  AC_Equantity_Zone_Stamp_02_21 | quantities | on 1 object (1 IFCSPACE)
    Apartment ID Position (X) = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (X) in 1:50 = 0. [MILLI METRE]
    Apartment ID Position (Y) = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:100 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:200 = 0. [MILLI METRE]
    Apartment ID Position (Y) in 1:50 = 0. [MILLI METRE]
    Circle Temp Radius = 150. [MILLI METRE]
    Combined Width of Doors = 0. [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_0) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_100) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_200) = 200. [MILLI METRE]
    Data Font Size (model) (fontDataSizeModel_50) = 200. [MILLI METRE]
    Floor Level = 263.525 [MILLI METRE]
    Height = 3394.075 [MILLI METRE]
    Length of Perimeter Walls = 9213.04293134 [MILLI METRE]
    Net Perimeter = 20811.0969215 [MILLI METRE]
    Perimeter = 20811.0969215 [MILLI METRE]
    Perimeter of Holes = 0. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_0) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_100) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_200) = 1500. [MILLI METRE]
    Pointer Horizontal Distance (pointerHorDist_50) = 1500. [MILLI METRE]
    Pointer Offset X = 0. [MILLI METRE]
    Pointer Offset X in 1:100 = 0. [MILLI METRE]
    Pointer Offset X in 1:200 = 0. [MILLI METRE]
    Pointer Offset X in 1:50 = 0. [MILLI METRE]
    Pointer Offset Y = 0. [MILLI METRE]
    Pointer Offset Y in 1:100 = 0. [MILLI METRE]
    Pointer Offset Y in 1:200 = 0. [MILLI METRE]
    Pointer Offset Y in 1:50 = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
    X Distance = 0. [MILLI METRE]
    X Distance in 1:100 = 0. [MILLI METRE]
    X Distance in 1:200 = 0. [MILLI METRE]
    X Distance in 1:50 = 0. [MILLI METRE]
    Y Distance = 0. [MILLI METRE]
    Y Distance in 1:100 = 0. [MILLI METRE]
    Y Distance in 1:200 = 0. [MILLI METRE]
    Y Distance in 1:50 = 0. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_0) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_100) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_200) = 250. [MILLI METRE]
    Zone Name Font Size (model) (fontTitleSizeModel_50) = 250. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_0) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_100) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_200) = 200. [MILLI METRE]
    Zone Number Font Size (model) (fontTitle2SizeModel_50) = 200. [MILLI METRE]
  AC_Equantity_Zone_Stamp_02_21: 5 more contents on 5 objects not shown
  AC_Equantity_Mirror_21 | quantities | on 2 objects (2 IFCFLOWTERMINAL)
    Bottom Level = 1000. [MILLI METRE]
    Bottom Width = 25.4 [MILLI METRE]
    Frame Thickness = 25.4 [MILLI METRE]
    Frame Width (0-None) = 0. [MILLI METRE]
    Height = 812.8 [MILLI METRE]
    Shelf Height = 12.7 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    X Dimension = 1625.6 [MILLI METRE]
    Y Dimension = 10. [MILLI METRE]
  AC_Equantity_Mirror_21 | quantities | on 1 object (1 IFCFLOWTERMINAL)
    Bottom Level = 1000. [MILLI METRE]
    Bottom Width = 25.4 [MILLI METRE]
    Frame Thickness = 25.4 [MILLI METRE]
    Frame Width (0-None) = 0. [MILLI METRE]
    Height = 812.8 [MILLI METRE]
    Shelf Height = 12.7 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    X Dimension = 1623.24889387 [MILLI METRE]
    Y Dimension = 10. [MILLI METRE]
  AC_Equantity_D1_Commercial_21 | quantities | on 4 objects (4 IFCDOOR)
    3D Closed Height = 0. [MILLI METRE]
    3D Closed Length = 0. [MILLI METRE]
    3D Opening Height = 1500. [MILLI METRE]
    3D Opening Length 1 = 560. [MILLI METRE]
    3D Opening Length 2 = 140. [MILLI METRE]
    3D Opening Length = 1500. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Box Axis Height from Header = 0. [MILLI METRE]
    Box Depth (gs_shutLam_boxWidth) = 150. [MILLI METRE]
    Box Depth (gs_shutRoll_boxWidth) = 150. [MILLI METRE]
    Box Height (gs_shutLam2_boxHeight) = 60. [MILLI METRE]
    Box Height (gs_shutLam_boxHeight) = 200. [MILLI METRE]
    Box Height (gs_shutRoll_boxHeight) = 200. [MILLI METRE]
    Box Left Offset = 0. [MILLI METRE]
    Box Right Offset = 0. [MILLI METRE]
    Box Width = 60. [MILLI METRE]
    Brick Thickness (gs_brick_sill_br_thk) = 65. [MILLI METRE]
    Brick Thickness (gs_masonry_arch_brick_thk) = 66.675 [MILLI METRE]
    Closer Thickness = 100. [MILLI METRE]
    Closer Width = 38. [MILLI METRE]
    Closing Depth = 0. [MILLI METRE]
    Cover Width = 0. [MILLI METRE]
    Custom Thickness = 15. [MILLI METRE]
    Dead Bolt Height = 1066.8 [MILLI METRE]
    Depth of Rails = 72.5 [MILLI METRE]
    Distance between Arch and Door = 0. [MILLI METRE]
    Distance from Header (gs_shutLam2_distFromHead) = 60. [MILLI METRE]
    Distance from Header (gs_shutLam_distFromHead) = 0. [MILLI METRE]
    Distance from Header (gs_shutRoll_distFromHead) = 0. [MILLI METRE]
    Distance from Wall (gs_shutLam_distFromWall) = 0. [MILLI METRE]
    Distance from Wall (gs_shutRoll_distFromWall) = 0. [MILLI METRE]
    Distance from Window = 60. [MILLI METRE]
    Distance of Skin from Closer = 0. [MILLI METRE]
    Door Panel Overlap Width = 50.8 [MILLI METRE]
    Door Stop Projection = 44.45 [MILLI METRE]
    Door Stop Thickness = 38.1 [MILLI METRE]
    Door Stop Width = 12.7 [MILLI METRE]
    Egress Height = 2019.3 [MILLI METRE]
    Egress Width = 824.70625 [MILLI METRE]
    Ext. Threshold Overhang Inside = 50.8 [MILLI METRE]
    Ext. Threshold Overhang Outside = 50.8 [MILLI METRE]
    Extra Frame Thickness = 30. [MILLI METRE]
    Extra Frame Width = 40. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Thickness Inside = 101.6 [MILLI METRE]
    Frame Width = 50.8 [MILLI METRE]
    Frame Width Bottom = 50. [MILLI METRE]
    Frame Width Left = 50.8 [MILLI METRE]
    Frame Width Right = 50.8 [MILLI METRE]
    Frame Width Upper = 50.8 [MILLI METRE]
    Glass Thickness = 12.7 [MILLI METRE]
    Grid Thickness = 19.05 [MILLI METRE]
    Grid Width = 12.7 [MILLI METRE]
    Handle Height = 914.4 [MILLI METRE]
    Handle Position = 50.8 [MILLI METRE]
    Hanging Stick Length = 20. [MILLI METRE]
    Hanging Stick Radius = 5. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_left_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_right_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_left_out) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_right_out) = 0. [MILLI METRE]
    Head Jamb Depth = 31.75 [MILLI METRE]
    Head Width Inside = 63.5 [MILLI METRE]
    Head Width Outside = 63.5 [MILLI METRE]
    Hole Radius = 10. [MILLI METRE]
    Horizontal Boards Approximate Width = 115. [MILLI METRE]
    Horizontal Boards Thickness = 25. [MILLI METRE]
    Horizontal Frame Divider Width = 50. [MILLI METRE]
    Inner Head Depth (gs_reveal_double_innerTop) = 101.6 [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 101.6 [MILLI METRE]
    Inner Offset = 20. [MILLI METRE]
    Inner Panel Width = 120. [MILLI METRE]
    Inner Sill Depth (gs_reveal_double_innerBottom) = 101.6 [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 101.6 [MILLI METRE]
    Jamb Depth = 31.75 [MILLI METRE]
    Jamb Depth Side 2 = 31.75 [MILLI METRE]
    Jamb Extension Width = 12.7 [MILLI METRE]
    Jamb Extension Width Outside = 0. [MILLI METRE]
    Keystone Oversize = 0. [MILLI METRE]
    Keystone Projection = 10. [MILLI METRE]
    Keystone Width = 100. [MILLI METRE]
    Leaf Frame Width Internal = 25.4 [MILLI METRE]
    Leaf Frame Width Left = 101.6 [MILLI METRE]
    Leaf Frame Width Lower = 101.6 [MILLI METRE]
    Leaf Frame Width Right = 101.6 [MILLI METRE]
    Leaf Frame Width Side = 101.6 [MILLI METRE]
    Leaf Frame Width Upper = 101.6 [MILLI METRE]
    Leaf Height = 2032. [MILLI METRE]
    Leaf Thickness = 44.45 [MILLI METRE]
    Leaf Width = 850.10625 [MILLI METRE]
    Left Opening Oversize = 0. [MILLI METRE]
    Left Panel Width = 283.36875 [MILLI METRE]
    Louver Thickness = 10. [MILLI METRE]
    Louver Width = 40. [MILLI METRE]
    Lower Opening Oversize = 0. [MILLI METRE]
    Main Door Panel Width = 457.2 [MILLI METRE]
    Masonry Arch Depth = 101.6 [MILLI METRE]
    Masonry Arch Height = 203.2 [MILLI METRE]
    Masonry Arch Overhang Left = 0. [MILLI METRE]
    Masonry Arch Overhang Right = 0. [MILLI METRE]
    Masonry Arch Projection = 0. [MILLI METRE]
    Masonry Arch Rise = 50.8 [MILLI METRE]
    Middle Frame Width = 101.6 [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 15. [MILLI METRE]
    Mortar Thickness (gs_masonry_arch_mort_thk) = 9.525 [MILLI METRE]
    Offset Inside = 0. [MILLI METRE]
    Offset Outside = -63.5 [MILLI METRE]
    Offset from Edge if not Center = 152.4 [MILLI METRE]
    Opening Side Depth = 1524. [MILLI METRE]
    Opening Side Width 1 = 0. [MILLI METRE]
    Opening Side Width 2 = 457.2 [MILLI METRE]
    Opening Width in 2D = 0. [MILLI METRE]
    Opening Width in 3D = 0. [MILLI METRE]
    Opposite Side Width 2 = 304.8 [MILLI METRE]
    Outer Jamb Depth = 80. [MILLI METRE]
    Outside Overhang = 0. [MILLI METRE]
    Overhang 1 Left = 22.225 [MILLI METRE]
    Overhang 1 Right = 22.225 [MILLI METRE]
    Overhang 1 Upper = 22.225 [MILLI METRE]
    Panel Distance = 6. [MILLI METRE]
    Panel Fill Thickness = 10. [MILLI METRE]
    Panel Frame Width = 50.8 [MILLI METRE]
    Panel Height = 1500. [MILLI METRE]
    Panel Thickness = 50.8 [MILLI METRE]
    Panel Width = 0. [MILLI METRE]
    Plaster Thickness Limit = 38.1 [MILLI METRE]
    Profile Width = 150. [MILLI METRE]
    Rail Height = 914.4 [MILLI METRE]
    Rail Width = 38.1 [MILLI METRE]
    Rear Hole Depth = 0. [MILLI METRE]
    Rebate Width = 12.7 [MILLI METRE]
    Reveal Depth (AC_wido_sill) = 0. [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 0. [MILLI METRE]
    Reveal Height = 2082.8 [MILLI METRE]
    Reveal Width = 951.70625 [MILLI METRE]
    Reveal to Wall Core = 0. [MILLI METRE]
    Right Opening Oversize = 0. [MILLI METRE]
    Right Panel Width = 283.36875 [MILLI METRE]
    Segment Width (gs_shutLam2_segmentWidth) = 60. [MILLI METRE]
    Segment Width (gs_shutLam_segmentWidth) = 60. [MILLI METRE]
    Side Width Inside = 63.5 [MILLI METRE]
    Side Width Outside = 63.5 [MILLI METRE]
    Sidelight Frame Thickness = 38.1 [MILLI METRE]
    Sidelight Frame Width = 50.8 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left) = 355.6 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_half) = 150. [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_orig) = 300. [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right) = 355.6 [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_half) = 150. [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_orig) = 300. [MILLI METRE]
    Sill Height to Current Story = 203.200010131 [MILLI METRE]
    Sill Jamb Depth = 60. [MILLI METRE]
    Sill Nosing = 31.75 [MILLI METRE]
    Sill Overhang Left = 0. [MILLI METRE]
    Sill Overhang Right = 0. [MILLI METRE]
    Sill Slip-in Depth = 25.4 [MILLI METRE]
    Sill Thickness = 100. [MILLI METRE]
    Sill Top Height = 10. [MILLI METRE]
    Sill Top Width = 10. [MILLI METRE]
    Skin Overhang to Frame Depth = 0. [MILLI METRE]
    Slat Width = 50. [MILLI METRE]
    Strip Thickness = 25. [MILLI METRE]
    Thickness Inside = 31.75 [MILLI METRE]
    Thickness Outside = 31.75 [MILLI METRE]
    Threshold External Thickness = 5.80737765736 [MILLI METRE]
    Threshold Nosing Inside = 25.4 [MILLI METRE]
    Threshold Nosing Outside = 25.4 [MILLI METRE]
    Threshold Thickness = 12.7 [MILLI METRE]
    Threshold Width = 10. [MILLI METRE]
    Tolerance Left = 0. [MILLI METRE]
    Tolerance Lower = 0. [MILLI METRE]
    Tolerance Right = 0. [MILLI METRE]
    Tolerance Upper = 0. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Frame Thickness = 38.1 [MILLI METRE]
    Transom Frame Width = 50.8 [MILLI METRE]
    Transom Height = 355.6 [MILLI METRE]
    Unit Height = 2082.8 [MILLI METRE]
    Unit Width = 951.70625 [MILLI METRE]
    Upper Opening Oversize = 0. [MILLI METRE]
    Vertical Board Width = 100. [MILLI METRE]
    Vertical Boards Approximate Width = 80. [MILLI METRE]
    Vertical Boards Thickness = 25. [MILLI METRE]
    Vertical Frame Divider Width = 50. [MILLI METRE]
    Vertical Grid Height = 914.4 [MILLI METRE]
    Wallhole Height = 2082.8 [MILLI METRE]
    Wallhole Width = 951.70625 [MILLI METRE]
    Width Side (gs_tw_left_in) = 63.5 [MILLI METRE]
    Width Side (gs_tw_left_out) = 63.5 [MILLI METRE]
    Width of Sill = 0. [MILLI METRE]
    Window Height = 304.8 [MILLI METRE]
    Window Sill Height = 1524. [MILLI METRE]
    Window Width = 304.8 [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
    Z Frame Thickness = 25. [MILLI METRE]
    Z Frame Width = 50. [MILLI METRE]
  AC_Equantity_D1_Commercial_21 | quantities | on 3 objects (3 IFCDOOR)
    3D Closed Height = 0. [MILLI METRE]
    3D Closed Length = 0. [MILLI METRE]
    3D Opening Height = 1500. [MILLI METRE]
    3D Opening Length 1 = 560. [MILLI METRE]
    3D Opening Length 2 = 140. [MILLI METRE]
    3D Opening Length = 1500. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Box Axis Height from Header = 0. [MILLI METRE]
    Box Depth (gs_shutLam_boxWidth) = 150. [MILLI METRE]
    Box Depth (gs_shutRoll_boxWidth) = 150. [MILLI METRE]
    Box Height (gs_shutLam2_boxHeight) = 60. [MILLI METRE]
    Box Height (gs_shutLam_boxHeight) = 200. [MILLI METRE]
    Box Height (gs_shutRoll_boxHeight) = 200. [MILLI METRE]
    Box Left Offset = 0. [MILLI METRE]
    Box Right Offset = 0. [MILLI METRE]
    Box Width = 60. [MILLI METRE]
    Brick Thickness (gs_brick_sill_br_thk) = 65. [MILLI METRE]
    Brick Thickness (gs_masonry_arch_brick_thk) = 66.675 [MILLI METRE]
    Closer Thickness = 100. [MILLI METRE]
    Closer Width = 38. [MILLI METRE]
    Closing Depth = 0. [MILLI METRE]
    Cover Width = 0. [MILLI METRE]
    Custom Thickness = 15. [MILLI METRE]
    Dead Bolt Height = 1066.8 [MILLI METRE]
    Depth of Rails = 72.5 [MILLI METRE]
    Distance between Arch and Door = 0. [MILLI METRE]
    Distance from Header (gs_shutLam2_distFromHead) = 60. [MILLI METRE]
    Distance from Header (gs_shutLam_distFromHead) = 0. [MILLI METRE]
    Distance from Header (gs_shutRoll_distFromHead) = 0. [MILLI METRE]
    Distance from Wall (gs_shutLam_distFromWall) = 0. [MILLI METRE]
    Distance from Wall (gs_shutRoll_distFromWall) = 0. [MILLI METRE]
    Distance from Window = 60. [MILLI METRE]
    Distance of Skin from Closer = 0. [MILLI METRE]
    Door Panel Overlap Width = 50.8 [MILLI METRE]
    Door Stop Projection = 44.45 [MILLI METRE]
    Door Stop Thickness = 38.1 [MILLI METRE]
    Door Stop Width = 12.7 [MILLI METRE]
    Egress Height = 2019.3 [MILLI METRE]
    Egress Width = 824.70625 [MILLI METRE]
    Ext. Threshold Overhang Inside = 50.8 [MILLI METRE]
    Ext. Threshold Overhang Outside = 50.8 [MILLI METRE]
    Extra Frame Thickness = 30. [MILLI METRE]
    Extra Frame Width = 40. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Thickness Inside = 101.6 [MILLI METRE]
    Frame Width = 50.8 [MILLI METRE]
    Frame Width Bottom = 50. [MILLI METRE]
    Frame Width Left = 50.8 [MILLI METRE]
    Frame Width Right = 50.8 [MILLI METRE]
    Frame Width Upper = 50.8 [MILLI METRE]
    Glass Thickness = 12.7 [MILLI METRE]
    Grid Thickness = 19.05 [MILLI METRE]
    Grid Width = 12.7 [MILLI METRE]
    Handle Height = 914.4 [MILLI METRE]
    Handle Position = 50.8 [MILLI METRE]
    Hanging Stick Length = 20. [MILLI METRE]
    Hanging Stick Radius = 5. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_left_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_right_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_left_out) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_right_out) = 0. [MILLI METRE]
    Head Jamb Depth = 31.75 [MILLI METRE]
    Head Width Inside = 63.5 [MILLI METRE]
    Head Width Outside = 63.5 [MILLI METRE]
    Hole Radius = 10. [MILLI METRE]
    Horizontal Boards Approximate Width = 115. [MILLI METRE]
    Horizontal Boards Thickness = 25. [MILLI METRE]
    Horizontal Frame Divider Width = 50. [MILLI METRE]
    Inner Head Depth (gs_reveal_double_innerTop) = 101.6 [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 101.6 [MILLI METRE]
    Inner Offset = 20. [MILLI METRE]
    Inner Panel Width = 120. [MILLI METRE]
    Inner Sill Depth (gs_reveal_double_innerBottom) = 101.6 [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 101.6 [MILLI METRE]
    Jamb Depth = 31.75 [MILLI METRE]
    Jamb Depth Side 2 = 31.75 [MILLI METRE]
    Jamb Extension Width = 12.7 [MILLI METRE]
    Jamb Extension Width Outside = 0. [MILLI METRE]
    Keystone Oversize = 0. [MILLI METRE]
    Keystone Projection = 10. [MILLI METRE]
    Keystone Width = 100. [MILLI METRE]
    Leaf Frame Width Internal = 25.4 [MILLI METRE]
    Leaf Frame Width Left = 101.6 [MILLI METRE]
    Leaf Frame Width Lower = 101.6 [MILLI METRE]
    Leaf Frame Width Right = 101.6 [MILLI METRE]
    Leaf Frame Width Side = 101.6 [MILLI METRE]
    Leaf Frame Width Upper = 101.6 [MILLI METRE]
    Leaf Height = 2032. [MILLI METRE]
    Leaf Thickness = 44.45 [MILLI METRE]
    Leaf Width = 850.10625 [MILLI METRE]
    Left Opening Oversize = 0. [MILLI METRE]
    Left Panel Width = 266.7 [MILLI METRE]
    Louver Thickness = 10. [MILLI METRE]
    Louver Width = 40. [MILLI METRE]
    Lower Opening Oversize = 0. [MILLI METRE]
    Main Door Panel Width = 457.2 [MILLI METRE]
    Masonry Arch Depth = 101.6 [MILLI METRE]
    Masonry Arch Height = 203.2 [MILLI METRE]
    Masonry Arch Overhang Left = 0. [MILLI METRE]
    Masonry Arch Overhang Right = 0. [MILLI METRE]
    Masonry Arch Projection = 0. [MILLI METRE]
    Masonry Arch Rise = 50.8 [MILLI METRE]
    Middle Frame Width = 101.6 [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 15. [MILLI METRE]
    Mortar Thickness (gs_masonry_arch_mort_thk) = 9.525 [MILLI METRE]
    Offset Inside = 0. [MILLI METRE]
    Offset Outside = -63.5 [MILLI METRE]
    Offset from Edge if not Center = 152.4 [MILLI METRE]
    Opening Side Depth = 1524. [MILLI METRE]
    Opening Side Width 1 = 0. [MILLI METRE]
    Opening Side Width 2 = 457.2 [MILLI METRE]
    Opening Width in 2D = 0. [MILLI METRE]
    Opening Width in 3D = 0. [MILLI METRE]
    Opposite Side Width 2 = 304.8 [MILLI METRE]
    Outer Jamb Depth = 80. [MILLI METRE]
    Outside Overhang = 0. [MILLI METRE]
    Overhang 1 Left = 22.225 [MILLI METRE]
    Overhang 1 Right = 22.225 [MILLI METRE]
    Overhang 1 Upper = 22.225 [MILLI METRE]
    Panel Distance = 6. [MILLI METRE]
    Panel Fill Thickness = 10. [MILLI METRE]
    Panel Frame Width = 50.8 [MILLI METRE]
    Panel Height = 1500. [MILLI METRE]
    Panel Thickness = 50.8 [MILLI METRE]
    Panel Width = 0. [MILLI METRE]
    Plaster Thickness Limit = 38.1 [MILLI METRE]
    Profile Width = 150. [MILLI METRE]
    Rail Height = 914.4 [MILLI METRE]
    Rail Width = 38.1 [MILLI METRE]
    Rear Hole Depth = 0. [MILLI METRE]
    Rebate Width = 12.7 [MILLI METRE]
    Reveal Depth (AC_wido_sill) = 0. [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 0. [MILLI METRE]
    Reveal Height = 2082.8 [MILLI METRE]
    Reveal Width = 951.70625 [MILLI METRE]
    Reveal to Wall Core = 0. [MILLI METRE]
    Right Opening Oversize = 0. [MILLI METRE]
    Right Panel Width = 266.7 [MILLI METRE]
    Segment Width (gs_shutLam2_segmentWidth) = 60. [MILLI METRE]
    Segment Width (gs_shutLam_segmentWidth) = 60. [MILLI METRE]
    Side Width Inside = 63.5 [MILLI METRE]
    Side Width Outside = 63.5 [MILLI METRE]
    Sidelight Frame Thickness = 38.1 [MILLI METRE]
    Sidelight Frame Width = 50.8 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left) = 355.6 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_half) = 150. [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_orig) = 300. [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right) = 355.6 [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_half) = 150. [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_orig) = 300. [MILLI METRE]
    Sill Height to Current Story = 203.200009289 [MILLI METRE]
    Sill Jamb Depth = 60. [MILLI METRE]
    Sill Nosing = 31.75 [MILLI METRE]
    Sill Overhang Left = 0. [MILLI METRE]
    Sill Overhang Right = 0. [MILLI METRE]
    Sill Slip-in Depth = 25.4 [MILLI METRE]
    Sill Thickness = 100. [MILLI METRE]
    Sill Top Height = 10. [MILLI METRE]
    Sill Top Width = 10. [MILLI METRE]
    Skin Overhang to Frame Depth = 0. [MILLI METRE]
    Slat Width = 50. [MILLI METRE]
    Strip Thickness = 25. [MILLI METRE]
    Thickness Inside = 31.75 [MILLI METRE]
    Thickness Outside = 31.75 [MILLI METRE]
    Threshold External Thickness = 5.80737765736 [MILLI METRE]
    Threshold Nosing Inside = 25.4 [MILLI METRE]
    Threshold Nosing Outside = 25.4 [MILLI METRE]
    Threshold Thickness = 12.7 [MILLI METRE]
    Threshold Width = 10. [MILLI METRE]
    Tolerance Left = 0. [MILLI METRE]
    Tolerance Lower = 0. [MILLI METRE]
    Tolerance Right = 0. [MILLI METRE]
    Tolerance Upper = 0. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Frame Thickness = 38.1 [MILLI METRE]
    Transom Frame Width = 50.8 [MILLI METRE]
    Transom Height = 355.6 [MILLI METRE]
    Unit Height = 2082.8 [MILLI METRE]
    Unit Width = 951.70625 [MILLI METRE]
    Upper Opening Oversize = 0. [MILLI METRE]
    Vertical Board Width = 100. [MILLI METRE]
    Vertical Boards Approximate Width = 80. [MILLI METRE]
    Vertical Boards Thickness = 25. [MILLI METRE]
    Vertical Frame Divider Width = 50. [MILLI METRE]
    Vertical Grid Height = 914.4 [MILLI METRE]
    Wallhole Height = 2082.8 [MILLI METRE]
    Wallhole Width = 951.70625 [MILLI METRE]
    Width Side (gs_tw_left_in) = 63.5 [MILLI METRE]
    Width Side (gs_tw_left_out) = 63.5 [MILLI METRE]
    Width of Sill = 0. [MILLI METRE]
    Window Height = 304.8 [MILLI METRE]
    Window Sill Height = 1524. [MILLI METRE]
    Window Width = 304.8 [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
    Z Frame Thickness = 25. [MILLI METRE]
    Z Frame Width = 50. [MILLI METRE]
  AC_Equantity_D1_Commercial_21 | quantities | on 3 objects (3 IFCDOOR)
    3D Closed Height = 0. [MILLI METRE]
    3D Closed Length = 0. [MILLI METRE]
    3D Opening Height = 1500. [MILLI METRE]
    3D Opening Length 1 = 560. [MILLI METRE]
    3D Opening Length 2 = 140. [MILLI METRE]
    3D Opening Length = 1500. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Box Axis Height from Header = 0. [MILLI METRE]
    Box Depth (gs_shutLam_boxWidth) = 150. [MILLI METRE]
    Box Depth (gs_shutRoll_boxWidth) = 150. [MILLI METRE]
    Box Height (gs_shutLam2_boxHeight) = 60. [MILLI METRE]
    Box Height (gs_shutLam_boxHeight) = 200. [MILLI METRE]
    Box Height (gs_shutRoll_boxHeight) = 200. [MILLI METRE]
    Box Left Offset = 0. [MILLI METRE]
    Box Right Offset = 0. [MILLI METRE]
    Box Width = 60. [MILLI METRE]
    Brick Thickness (gs_brick_sill_br_thk) = 65. [MILLI METRE]
    Brick Thickness (gs_masonry_arch_brick_thk) = 66.675 [MILLI METRE]
    Closer Thickness = 100. [MILLI METRE]
    Closer Width = 38. [MILLI METRE]
    Closing Depth = 0. [MILLI METRE]
    Cover Width = 0. [MILLI METRE]
    Custom Thickness = 15. [MILLI METRE]
    Dead Bolt Height = 1066.8 [MILLI METRE]
    Depth of Rails = 72.5 [MILLI METRE]
    Distance between Arch and Door = 0. [MILLI METRE]
    Distance from Header (gs_shutLam2_distFromHead) = 60. [MILLI METRE]
    Distance from Header (gs_shutLam_distFromHead) = 0. [MILLI METRE]
    Distance from Header (gs_shutRoll_distFromHead) = 0. [MILLI METRE]
    Distance from Wall (gs_shutLam_distFromWall) = 0. [MILLI METRE]
    Distance from Wall (gs_shutRoll_distFromWall) = 0. [MILLI METRE]
    Distance from Window = 60. [MILLI METRE]
    Distance of Skin from Closer = 0. [MILLI METRE]
    Door Panel Overlap Width = 50.8 [MILLI METRE]
    Door Stop Projection = 44.45 [MILLI METRE]
    Door Stop Thickness = 38.1 [MILLI METRE]
    Door Stop Width = 12.7 [MILLI METRE]
    Egress Height = 2019.3 [MILLI METRE]
    Egress Width = 824.70625 [MILLI METRE]
    Ext. Threshold Overhang Inside = 50.8 [MILLI METRE]
    Ext. Threshold Overhang Outside = 50.8 [MILLI METRE]
    Extra Frame Thickness = 30. [MILLI METRE]
    Extra Frame Width = 40. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Thickness Inside = 101.6 [MILLI METRE]
    Frame Width = 50.8 [MILLI METRE]
    Frame Width Bottom = 50. [MILLI METRE]
    Frame Width Left = 50.8 [MILLI METRE]
    Frame Width Right = 50.8 [MILLI METRE]
    Frame Width Upper = 50.8 [MILLI METRE]
    Glass Thickness = 12.7 [MILLI METRE]
    Grid Thickness = 19.05 [MILLI METRE]
    Grid Width = 12.7 [MILLI METRE]
    Handle Height = 914.4 [MILLI METRE]
    Handle Position = 50.8 [MILLI METRE]
    Hanging Stick Length = 20. [MILLI METRE]
    Hanging Stick Radius = 5. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_left_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_right_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_left_out) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_right_out) = 0. [MILLI METRE]
    Head Jamb Depth = 31.75 [MILLI METRE]
    Head Width Inside = 63.5 [MILLI METRE]
    Head Width Outside = 63.5 [MILLI METRE]
    Hole Radius = 10. [MILLI METRE]
    Horizontal Boards Approximate Width = 115. [MILLI METRE]
    Horizontal Boards Thickness = 25. [MILLI METRE]
    Horizontal Frame Divider Width = 50. [MILLI METRE]
    Inner Head Depth (gs_reveal_double_innerTop) = 101.6 [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 101.6 [MILLI METRE]
    Inner Offset = 20. [MILLI METRE]
    Inner Panel Width = 120. [MILLI METRE]
    Inner Sill Depth (gs_reveal_double_innerBottom) = 101.6 [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 101.6 [MILLI METRE]
    Jamb Depth = 31.75 [MILLI METRE]
    Jamb Depth Side 2 = 31.75 [MILLI METRE]
    Jamb Extension Width = 12.7 [MILLI METRE]
    Jamb Extension Width Outside = 0. [MILLI METRE]
    Keystone Oversize = 0. [MILLI METRE]
    Keystone Projection = 10. [MILLI METRE]
    Keystone Width = 100. [MILLI METRE]
    Leaf Frame Width Internal = 25.4 [MILLI METRE]
    Leaf Frame Width Left = 101.6 [MILLI METRE]
    Leaf Frame Width Lower = 101.6 [MILLI METRE]
    Leaf Frame Width Right = 101.6 [MILLI METRE]
    Leaf Frame Width Side = 101.6 [MILLI METRE]
    Leaf Frame Width Upper = 101.6 [MILLI METRE]
    Leaf Height = 2032. [MILLI METRE]
    Leaf Thickness = 44.45 [MILLI METRE]
    Leaf Width = 850.10625 [MILLI METRE]
    Left Opening Oversize = 0. [MILLI METRE]
    Left Panel Width = 283.36875 [MILLI METRE]
    Louver Thickness = 10. [MILLI METRE]
    Louver Width = 40. [MILLI METRE]
    Lower Opening Oversize = 0. [MILLI METRE]
    Main Door Panel Width = 457.2 [MILLI METRE]
    Masonry Arch Depth = 101.6 [MILLI METRE]
    Masonry Arch Height = 203.2 [MILLI METRE]
    Masonry Arch Overhang Left = 0. [MILLI METRE]
    Masonry Arch Overhang Right = 0. [MILLI METRE]
    Masonry Arch Projection = 0. [MILLI METRE]
    Masonry Arch Rise = 50.8 [MILLI METRE]
    Middle Frame Width = 101.6 [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 15. [MILLI METRE]
    Mortar Thickness (gs_masonry_arch_mort_thk) = 9.525 [MILLI METRE]
    Offset Inside = 0. [MILLI METRE]
    Offset Outside = -63.5 [MILLI METRE]
    Offset from Edge if not Center = 152.4 [MILLI METRE]
    Opening Side Depth = 1524. [MILLI METRE]
    Opening Side Width 1 = 0. [MILLI METRE]
    Opening Side Width 2 = 457.2 [MILLI METRE]
    Opening Width in 2D = 0. [MILLI METRE]
    Opening Width in 3D = 0. [MILLI METRE]
    Opposite Side Width 2 = 304.8 [MILLI METRE]
    Outer Jamb Depth = 80. [MILLI METRE]
    Outside Overhang = 0. [MILLI METRE]
    Overhang 1 Left = 22.225 [MILLI METRE]
    Overhang 1 Right = 22.225 [MILLI METRE]
    Overhang 1 Upper = 22.225 [MILLI METRE]
    Panel Distance = 6. [MILLI METRE]
    Panel Fill Thickness = 10. [MILLI METRE]
    Panel Frame Width = 50.8 [MILLI METRE]
    Panel Height = 1500. [MILLI METRE]
    Panel Thickness = 50.8 [MILLI METRE]
    Panel Width = 0. [MILLI METRE]
    Plaster Thickness Limit = 38.1 [MILLI METRE]
    Profile Width = 150. [MILLI METRE]
    Rail Height = 914.4 [MILLI METRE]
    Rail Width = 38.1 [MILLI METRE]
    Rear Hole Depth = 0. [MILLI METRE]
    Rebate Width = 12.7 [MILLI METRE]
    Reveal Depth (AC_wido_sill) = 0. [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 0. [MILLI METRE]
    Reveal Height = 2082.8 [MILLI METRE]
    Reveal Width = 951.70625 [MILLI METRE]
    Reveal to Wall Core = 0. [MILLI METRE]
    Right Opening Oversize = 0. [MILLI METRE]
    Right Panel Width = 283.36875 [MILLI METRE]
    Segment Width (gs_shutLam2_segmentWidth) = 60. [MILLI METRE]
    Segment Width (gs_shutLam_segmentWidth) = 60. [MILLI METRE]
    Side Width Inside = 63.5 [MILLI METRE]
    Side Width Outside = 63.5 [MILLI METRE]
    Sidelight Frame Thickness = 38.1 [MILLI METRE]
    Sidelight Frame Width = 50.8 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left) = 355.6 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_half) = 150. [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_orig) = 300. [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right) = 355.6 [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_half) = 150. [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_orig) = 300. [MILLI METRE]
    Sill Height to Current Story = 203.200009289 [MILLI METRE]
    Sill Jamb Depth = 60. [MILLI METRE]
    Sill Nosing = 31.75 [MILLI METRE]
    Sill Overhang Left = 0. [MILLI METRE]
    Sill Overhang Right = 0. [MILLI METRE]
    Sill Slip-in Depth = 25.4 [MILLI METRE]
    Sill Thickness = 100. [MILLI METRE]
    Sill Top Height = 10. [MILLI METRE]
    Sill Top Width = 10. [MILLI METRE]
    Skin Overhang to Frame Depth = 0. [MILLI METRE]
    Slat Width = 50. [MILLI METRE]
    Strip Thickness = 25. [MILLI METRE]
    Thickness Inside = 31.75 [MILLI METRE]
    Thickness Outside = 31.75 [MILLI METRE]
    Threshold External Thickness = 5.80737765736 [MILLI METRE]
    Threshold Nosing Inside = 25.4 [MILLI METRE]
    Threshold Nosing Outside = 25.4 [MILLI METRE]
    Threshold Thickness = 12.7 [MILLI METRE]
    Threshold Width = 10. [MILLI METRE]
    Tolerance Left = 0. [MILLI METRE]
    Tolerance Lower = 0. [MILLI METRE]
    Tolerance Right = 0. [MILLI METRE]
    Tolerance Upper = 0. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Frame Thickness = 38.1 [MILLI METRE]
    Transom Frame Width = 50.8 [MILLI METRE]
    Transom Height = 355.6 [MILLI METRE]
    Unit Height = 2082.8 [MILLI METRE]
    Unit Width = 951.70625 [MILLI METRE]
    Upper Opening Oversize = 0. [MILLI METRE]
    Vertical Board Width = 100. [MILLI METRE]
    Vertical Boards Approximate Width = 80. [MILLI METRE]
    Vertical Boards Thickness = 25. [MILLI METRE]
    Vertical Frame Divider Width = 50. [MILLI METRE]
    Vertical Grid Height = 914.4 [MILLI METRE]
    Wallhole Height = 2082.8 [MILLI METRE]
    Wallhole Width = 951.70625 [MILLI METRE]
    Width Side (gs_tw_left_in) = 63.5 [MILLI METRE]
    Width Side (gs_tw_left_out) = 63.5 [MILLI METRE]
    Width of Sill = 0. [MILLI METRE]
    Window Height = 304.8 [MILLI METRE]
    Window Sill Height = 1524. [MILLI METRE]
    Window Width = 304.8 [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
    Z Frame Thickness = 25. [MILLI METRE]
    Z Frame Width = 50. [MILLI METRE]
  AC_Equantity_D1_Commercial_21 | quantities | on 2 objects (2 IFCDOOR)
    3D Closed Height = 0. [MILLI METRE]
    3D Closed Length = 0. [MILLI METRE]
    3D Opening Height = 1500. [MILLI METRE]
    3D Opening Length 1 = 560. [MILLI METRE]
    3D Opening Length 2 = 140. [MILLI METRE]
    3D Opening Length = 1500. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Box Axis Height from Header = 0. [MILLI METRE]
    Box Depth (gs_shutLam_boxWidth) = 150. [MILLI METRE]
    Box Depth (gs_shutRoll_boxWidth) = 150. [MILLI METRE]
    Box Height (gs_shutLam2_boxHeight) = 60. [MILLI METRE]
    Box Height (gs_shutLam_boxHeight) = 200. [MILLI METRE]
    Box Height (gs_shutRoll_boxHeight) = 200. [MILLI METRE]
    Box Left Offset = 0. [MILLI METRE]
    Box Right Offset = 0. [MILLI METRE]
    Box Width = 60. [MILLI METRE]
    Brick Thickness (gs_brick_sill_br_thk) = 65. [MILLI METRE]
    Brick Thickness (gs_masonry_arch_brick_thk) = 66.675 [MILLI METRE]
    Closer Thickness = 100. [MILLI METRE]
    Closer Width = 38. [MILLI METRE]
    Closing Depth = 0. [MILLI METRE]
    Cover Width = 0. [MILLI METRE]
    Custom Thickness = 15. [MILLI METRE]
    Dead Bolt Height = 1066.8 [MILLI METRE]
    Depth of Rails = 72.5 [MILLI METRE]
    Distance between Arch and Door = 0. [MILLI METRE]
    Distance from Header (gs_shutLam2_distFromHead) = 60. [MILLI METRE]
    Distance from Header (gs_shutLam_distFromHead) = 0. [MILLI METRE]
    Distance from Header (gs_shutRoll_distFromHead) = 0. [MILLI METRE]
    Distance from Wall (gs_shutLam_distFromWall) = 0. [MILLI METRE]
    Distance from Wall (gs_shutRoll_distFromWall) = 0. [MILLI METRE]
    Distance from Window = 60. [MILLI METRE]
    Distance of Skin from Closer = 0. [MILLI METRE]
    Door Panel Overlap Width = 50.8 [MILLI METRE]
    Door Stop Projection = 44.45 [MILLI METRE]
    Door Stop Thickness = 38.1 [MILLI METRE]
    Door Stop Width = 12.7 [MILLI METRE]
    Egress Height = 2019.3 [MILLI METRE]
    Egress Width = 824.70625 [MILLI METRE]
    Ext. Threshold Overhang Inside = 50.8 [MILLI METRE]
    Ext. Threshold Overhang Outside = 50.8 [MILLI METRE]
    Extra Frame Thickness = 30. [MILLI METRE]
    Extra Frame Width = 40. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Thickness Inside = 101.6 [MILLI METRE]
    Frame Width = 50.8 [MILLI METRE]
    Frame Width Bottom = 50. [MILLI METRE]
    Frame Width Left = 50.8 [MILLI METRE]
    Frame Width Right = 50.8 [MILLI METRE]
    Frame Width Upper = 50.8 [MILLI METRE]
    Glass Thickness = 12.7 [MILLI METRE]
    Grid Thickness = 19.05 [MILLI METRE]
    Grid Width = 12.7 [MILLI METRE]
    Handle Height = 914.4 [MILLI METRE]
    Handle Position = 50.8 [MILLI METRE]
    Hanging Stick Length = 20. [MILLI METRE]
    Hanging Stick Radius = 5. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_left_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_right_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_left_out) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_right_out) = 0. [MILLI METRE]
    Head Jamb Depth = 31.75 [MILLI METRE]
    Head Width Inside = 63.5 [MILLI METRE]
    Head Width Outside = 63.5 [MILLI METRE]
    Hole Radius = 10. [MILLI METRE]
    Horizontal Boards Approximate Width = 115. [MILLI METRE]
    Horizontal Boards Thickness = 25. [MILLI METRE]
    Horizontal Frame Divider Width = 50. [MILLI METRE]
    Inner Head Depth (gs_reveal_double_innerTop) = 101.6 [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 101.6 [MILLI METRE]
    Inner Offset = 20. [MILLI METRE]
    Inner Panel Width = 120. [MILLI METRE]
    Inner Sill Depth (gs_reveal_double_innerBottom) = 101.6 [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 101.6 [MILLI METRE]
    Jamb Depth = 31.75 [MILLI METRE]
    Jamb Depth Side 2 = 31.75 [MILLI METRE]
    Jamb Extension Width = 12.7 [MILLI METRE]
    Jamb Extension Width Outside = 0. [MILLI METRE]
    Keystone Oversize = 0. [MILLI METRE]
    Keystone Projection = 10. [MILLI METRE]
    Keystone Width = 100. [MILLI METRE]
    Leaf Frame Width Internal = 25.4 [MILLI METRE]
    Leaf Frame Width Left = 101.6 [MILLI METRE]
    Leaf Frame Width Lower = 101.6 [MILLI METRE]
    Leaf Frame Width Right = 101.6 [MILLI METRE]
    Leaf Frame Width Side = 101.6 [MILLI METRE]
    Leaf Frame Width Upper = 101.6 [MILLI METRE]
    Leaf Height = 2032. [MILLI METRE]
    Leaf Thickness = 44.45 [MILLI METRE]
    Leaf Width = 850.10625 [MILLI METRE]
    Left Opening Oversize = 0. [MILLI METRE]
    Left Panel Width = 283.36875 [MILLI METRE]
    Louver Thickness = 10. [MILLI METRE]
    Louver Width = 40. [MILLI METRE]
    Lower Opening Oversize = 0. [MILLI METRE]
    Main Door Panel Width = 457.2 [MILLI METRE]
    Masonry Arch Depth = 101.6 [MILLI METRE]
    Masonry Arch Height = 203.2 [MILLI METRE]
    Masonry Arch Overhang Left = 0. [MILLI METRE]
    Masonry Arch Overhang Right = 0. [MILLI METRE]
    Masonry Arch Projection = 0. [MILLI METRE]
    Masonry Arch Rise = 50.8 [MILLI METRE]
    Middle Frame Width = 101.6 [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 15. [MILLI METRE]
    Mortar Thickness (gs_masonry_arch_mort_thk) = 9.525 [MILLI METRE]
    Offset Inside = 0. [MILLI METRE]
    Offset Outside = -63.5 [MILLI METRE]
    Offset from Edge if not Center = 152.4 [MILLI METRE]
    Opening Side Depth = 1524. [MILLI METRE]
    Opening Side Width 1 = 0. [MILLI METRE]
    Opening Side Width 2 = 457.2 [MILLI METRE]
    Opening Width in 2D = 0. [MILLI METRE]
    Opening Width in 3D = 0. [MILLI METRE]
    Opposite Side Width 2 = 304.8 [MILLI METRE]
    Outer Jamb Depth = 80. [MILLI METRE]
    Outside Overhang = 0. [MILLI METRE]
    Overhang 1 Left = 22.225 [MILLI METRE]
    Overhang 1 Right = 22.225 [MILLI METRE]
    Overhang 1 Upper = 22.225 [MILLI METRE]
    Panel Distance = 6. [MILLI METRE]
    Panel Fill Thickness = 10. [MILLI METRE]
    Panel Frame Width = 50.8 [MILLI METRE]
    Panel Height = 1500. [MILLI METRE]
    Panel Thickness = 50.8 [MILLI METRE]
    Panel Width = 0. [MILLI METRE]
    Plaster Thickness Limit = 38.1 [MILLI METRE]
    Profile Width = 150. [MILLI METRE]
    Rail Height = 914.4 [MILLI METRE]
    Rail Width = 38.1 [MILLI METRE]
    Rear Hole Depth = 0. [MILLI METRE]
    Rebate Width = 12.7 [MILLI METRE]
    Reveal Depth (AC_wido_sill) = 0. [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 0. [MILLI METRE]
    Reveal Height = 2082.8 [MILLI METRE]
    Reveal Width = 951.70625 [MILLI METRE]
    Reveal to Wall Core = 0. [MILLI METRE]
    Right Opening Oversize = 0. [MILLI METRE]
    Right Panel Width = 283.36875 [MILLI METRE]
    Segment Width (gs_shutLam2_segmentWidth) = 60. [MILLI METRE]
    Segment Width (gs_shutLam_segmentWidth) = 60. [MILLI METRE]
    Side Width Inside = 63.5 [MILLI METRE]
    Side Width Outside = 63.5 [MILLI METRE]
    Sidelight Frame Thickness = 38.1 [MILLI METRE]
    Sidelight Frame Width = 50.8 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left) = 355.6 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_half) = 150. [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_orig) = 300. [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right) = 355.6 [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_half) = 150. [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_orig) = 300. [MILLI METRE]
    Sill Height to Current Story = 263.525 [MILLI METRE]
    Sill Jamb Depth = 60. [MILLI METRE]
    Sill Nosing = 31.75 [MILLI METRE]
    Sill Overhang Left = 0. [MILLI METRE]
    Sill Overhang Right = 0. [MILLI METRE]
    Sill Slip-in Depth = 25.4 [MILLI METRE]
    Sill Thickness = 100. [MILLI METRE]
    Sill Top Height = 10. [MILLI METRE]
    Sill Top Width = 10. [MILLI METRE]
    Skin Overhang to Frame Depth = 0. [MILLI METRE]
    Slat Width = 50. [MILLI METRE]
    Strip Thickness = 25. [MILLI METRE]
    Thickness Inside = 31.75 [MILLI METRE]
    Thickness Outside = 31.75 [MILLI METRE]
    Threshold External Thickness = 5.80737765736 [MILLI METRE]
    Threshold Nosing Inside = 25.4 [MILLI METRE]
    Threshold Nosing Outside = 25.4 [MILLI METRE]
    Threshold Thickness = 12.7 [MILLI METRE]
    Threshold Width = 10. [MILLI METRE]
    Tolerance Left = 0. [MILLI METRE]
    Tolerance Lower = 0. [MILLI METRE]
    Tolerance Right = 0. [MILLI METRE]
    Tolerance Upper = 0. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Frame Thickness = 38.1 [MILLI METRE]
    Transom Frame Width = 50.8 [MILLI METRE]
    Transom Height = 355.6 [MILLI METRE]
    Unit Height = 2082.8 [MILLI METRE]
    Unit Width = 951.70625 [MILLI METRE]
    Upper Opening Oversize = 0. [MILLI METRE]
    Vertical Board Width = 100. [MILLI METRE]
    Vertical Boards Approximate Width = 80. [MILLI METRE]
    Vertical Boards Thickness = 25. [MILLI METRE]
    Vertical Frame Divider Width = 50. [MILLI METRE]
    Vertical Grid Height = 914.4 [MILLI METRE]
    Wallhole Height = 2082.8 [MILLI METRE]
    Wallhole Width = 951.70625 [MILLI METRE]
    Width Side (gs_tw_left_in) = 63.5 [MILLI METRE]
    Width Side (gs_tw_left_out) = 63.5 [MILLI METRE]
    Width of Sill = 0. [MILLI METRE]
    Window Height = 304.8 [MILLI METRE]
    Window Sill Height = 1524. [MILLI METRE]
    Window Width = 304.8 [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
    Z Frame Thickness = 25. [MILLI METRE]
    Z Frame Width = 50. [MILLI METRE]
  AC_Equantity_D1_Commercial_21 | quantities | on 2 objects (2 IFCDOOR)
    3D Closed Height = 0. [MILLI METRE]
    3D Closed Length = 0. [MILLI METRE]
    3D Opening Height = 1500. [MILLI METRE]
    3D Opening Length 1 = 560. [MILLI METRE]
    3D Opening Length 2 = 140. [MILLI METRE]
    3D Opening Length = 1500. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Box Axis Height from Header = 0. [MILLI METRE]
    Box Depth (gs_shutLam_boxWidth) = 150. [MILLI METRE]
    Box Depth (gs_shutRoll_boxWidth) = 150. [MILLI METRE]
    Box Height (gs_shutLam2_boxHeight) = 60. [MILLI METRE]
    Box Height (gs_shutLam_boxHeight) = 200. [MILLI METRE]
    Box Height (gs_shutRoll_boxHeight) = 200. [MILLI METRE]
    Box Left Offset = 0. [MILLI METRE]
    Box Right Offset = 0. [MILLI METRE]
    Box Width = 60. [MILLI METRE]
    Brick Thickness (gs_brick_sill_br_thk) = 65. [MILLI METRE]
    Brick Thickness (gs_masonry_arch_brick_thk) = 66.675 [MILLI METRE]
    Closer Thickness = 100. [MILLI METRE]
    Closer Width = 38. [MILLI METRE]
    Closing Depth = 0. [MILLI METRE]
    Cover Width = 0. [MILLI METRE]
    Custom Thickness = 15. [MILLI METRE]
    Dead Bolt Height = 1066.8 [MILLI METRE]
    Depth of Rails = 72.5 [MILLI METRE]
    Distance between Arch and Door = 0. [MILLI METRE]
    Distance from Header (gs_shutLam2_distFromHead) = 60. [MILLI METRE]
    Distance from Header (gs_shutLam_distFromHead) = 0. [MILLI METRE]
    Distance from Header (gs_shutRoll_distFromHead) = 0. [MILLI METRE]
    Distance from Wall (gs_shutLam_distFromWall) = 0. [MILLI METRE]
    Distance from Wall (gs_shutRoll_distFromWall) = 0. [MILLI METRE]
    Distance from Window = 60. [MILLI METRE]
    Distance of Skin from Closer = 0. [MILLI METRE]
    Door Panel Overlap Width = 50.8 [MILLI METRE]
    Door Stop Projection = 44.45 [MILLI METRE]
    Door Stop Thickness = 38.1 [MILLI METRE]
    Door Stop Width = 12.7 [MILLI METRE]
    Egress Height = 2019.3 [MILLI METRE]
    Egress Width = 990.190429156 [MILLI METRE]
    Ext. Threshold Overhang Inside = 50.8 [MILLI METRE]
    Ext. Threshold Overhang Outside = 50.8 [MILLI METRE]
    Extra Frame Thickness = 30. [MILLI METRE]
    Extra Frame Width = 40. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Thickness Inside = 101.6 [MILLI METRE]
    Frame Width = 50.8 [MILLI METRE]
    Frame Width Bottom = 50. [MILLI METRE]
    Frame Width Left = 50.8 [MILLI METRE]
    Frame Width Right = 50.8 [MILLI METRE]
    Frame Width Upper = 50.8 [MILLI METRE]
    Glass Thickness = 12.7 [MILLI METRE]
    Grid Thickness = 19.05 [MILLI METRE]
    Grid Width = 12.7 [MILLI METRE]
    Handle Height = 914.4 [MILLI METRE]
    Handle Position = 50.8 [MILLI METRE]
    Hanging Stick Length = 20. [MILLI METRE]
    Hanging Stick Radius = 5. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_left_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_right_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_left_out) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_right_out) = 0. [MILLI METRE]
    Head Jamb Depth = 31.75 [MILLI METRE]
    Head Width Inside = 63.5 [MILLI METRE]
    Head Width Outside = 63.5 [MILLI METRE]
    Hole Radius = 10. [MILLI METRE]
    Horizontal Boards Approximate Width = 115. [MILLI METRE]
    Horizontal Boards Thickness = 25. [MILLI METRE]
    Horizontal Frame Divider Width = 50. [MILLI METRE]
    Inner Head Depth (gs_reveal_double_innerTop) = 101.6 [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 101.6 [MILLI METRE]
    Inner Offset = 20. [MILLI METRE]
    Inner Panel Width = 120. [MILLI METRE]
    Inner Sill Depth (gs_reveal_double_innerBottom) = 101.6 [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 101.6 [MILLI METRE]
    Jamb Depth = 31.75 [MILLI METRE]
    Jamb Depth Side 2 = 31.75 [MILLI METRE]
    Jamb Extension Width = 12.7 [MILLI METRE]
    Jamb Extension Width Outside = 0. [MILLI METRE]
    Keystone Oversize = 0. [MILLI METRE]
    Keystone Projection = 10. [MILLI METRE]
    Keystone Width = 100. [MILLI METRE]
    Leaf Frame Width Internal = 25.4 [MILLI METRE]
    Leaf Frame Width Left = 101.6 [MILLI METRE]
    Leaf Frame Width Lower = 101.6 [MILLI METRE]
    Leaf Frame Width Right = 101.6 [MILLI METRE]
    Leaf Frame Width Side = 101.6 [MILLI METRE]
    Leaf Frame Width Upper = 101.6 [MILLI METRE]
    Leaf Height = 2032. [MILLI METRE]
    Leaf Thickness = 44.45 [MILLI METRE]
    Leaf Width = 1015.59042916 [MILLI METRE]
    Left Opening Oversize = 0. [MILLI METRE]
    Left Panel Width = 283.36875 [MILLI METRE]
    Louver Thickness = 10. [MILLI METRE]
    Louver Width = 40. [MILLI METRE]
    Lower Opening Oversize = 0. [MILLI METRE]
    Main Door Panel Width = 457.2 [MILLI METRE]
    Masonry Arch Depth = 101.6 [MILLI METRE]
    Masonry Arch Height = 203.2 [MILLI METRE]
    Masonry Arch Overhang Left = 0. [MILLI METRE]
    Masonry Arch Overhang Right = 0. [MILLI METRE]
    Masonry Arch Projection = 0. [MILLI METRE]
    Masonry Arch Rise = 50.8 [MILLI METRE]
    Middle Frame Width = 101.6 [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 15. [MILLI METRE]
    Mortar Thickness (gs_masonry_arch_mort_thk) = 9.525 [MILLI METRE]
    Offset Inside = 0. [MILLI METRE]
    Offset Outside = -63.5 [MILLI METRE]
    Offset from Edge if not Center = 152.4 [MILLI METRE]
    Opening Side Depth = 1524. [MILLI METRE]
    Opening Side Width 1 = 0. [MILLI METRE]
    Opening Side Width 2 = 457.2 [MILLI METRE]
    Opening Width in 2D = 0. [MILLI METRE]
    Opening Width in 3D = 0. [MILLI METRE]
    Opposite Side Width 2 = 304.8 [MILLI METRE]
    Outer Jamb Depth = 80. [MILLI METRE]
    Outside Overhang = 0. [MILLI METRE]
    Overhang 1 Left = 22.225 [MILLI METRE]
    Overhang 1 Right = 22.225 [MILLI METRE]
    Overhang 1 Upper = 22.225 [MILLI METRE]
    Panel Distance = 6. [MILLI METRE]
    Panel Fill Thickness = 10. [MILLI METRE]
    Panel Frame Width = 50.8 [MILLI METRE]
    Panel Height = 1500. [MILLI METRE]
    Panel Thickness = 50.8 [MILLI METRE]
    Panel Width = 0. [MILLI METRE]
    Plaster Thickness Limit = 38.1 [MILLI METRE]
    Profile Width = 150. [MILLI METRE]
    Rail Height = 914.4 [MILLI METRE]
    Rail Width = 38.1 [MILLI METRE]
    Rear Hole Depth = 0. [MILLI METRE]
    Rebate Width = 12.7 [MILLI METRE]
    Reveal Depth (AC_wido_sill) = 0. [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 0. [MILLI METRE]
    Reveal Height = 2082.8 [MILLI METRE]
    Reveal Width = 1117.19042916 [MILLI METRE]
    Reveal to Wall Core = 0. [MILLI METRE]
    Right Opening Oversize = 0. [MILLI METRE]
    Right Panel Width = 283.36875 [MILLI METRE]
    Segment Width (gs_shutLam2_segmentWidth) = 60. [MILLI METRE]
    Segment Width (gs_shutLam_segmentWidth) = 60. [MILLI METRE]
    Side Width Inside = 63.5 [MILLI METRE]
    Side Width Outside = 63.5 [MILLI METRE]
    Sidelight Frame Thickness = 38.1 [MILLI METRE]
    Sidelight Frame Width = 50.8 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left) = 355.6 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_half) = 150. [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_orig) = 300. [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right) = 355.6 [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_half) = 150. [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_orig) = 300. [MILLI METRE]
    Sill Height to Current Story = 203.200010131 [MILLI METRE]
    Sill Jamb Depth = 60. [MILLI METRE]
    Sill Nosing = 31.75 [MILLI METRE]
    Sill Overhang Left = 0. [MILLI METRE]
    Sill Overhang Right = 0. [MILLI METRE]
    Sill Slip-in Depth = 25.4 [MILLI METRE]
    Sill Thickness = 100. [MILLI METRE]
    Sill Top Height = 10. [MILLI METRE]
    Sill Top Width = 10. [MILLI METRE]
    Skin Overhang to Frame Depth = 0. [MILLI METRE]
    Slat Width = 50. [MILLI METRE]
    Strip Thickness = 25. [MILLI METRE]
    Thickness Inside = 31.75 [MILLI METRE]
    Thickness Outside = 31.75 [MILLI METRE]
    Threshold External Thickness = 5.80737765736 [MILLI METRE]
    Threshold Nosing Inside = 25.4 [MILLI METRE]
    Threshold Nosing Outside = 25.4 [MILLI METRE]
    Threshold Thickness = 12.7 [MILLI METRE]
    Threshold Width = 10. [MILLI METRE]
    Tolerance Left = 0. [MILLI METRE]
    Tolerance Lower = 0. [MILLI METRE]
    Tolerance Right = 0. [MILLI METRE]
    Tolerance Upper = 0. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Frame Thickness = 38.1 [MILLI METRE]
    Transom Frame Width = 50.8 [MILLI METRE]
    Transom Height = 355.6 [MILLI METRE]
    Unit Height = 2082.8 [MILLI METRE]
    Unit Width = 1117.19042916 [MILLI METRE]
    Upper Opening Oversize = 0. [MILLI METRE]
    Vertical Board Width = 100. [MILLI METRE]
    Vertical Boards Approximate Width = 80. [MILLI METRE]
    Vertical Boards Thickness = 25. [MILLI METRE]
    Vertical Frame Divider Width = 50. [MILLI METRE]
    Vertical Grid Height = 914.4 [MILLI METRE]
    Wallhole Height = 2082.8 [MILLI METRE]
    Wallhole Width = 1117.19042916 [MILLI METRE]
    Width Side (gs_tw_left_in) = 63.5 [MILLI METRE]
    Width Side (gs_tw_left_out) = 63.5 [MILLI METRE]
    Width of Sill = 0. [MILLI METRE]
    Window Height = 304.8 [MILLI METRE]
    Window Sill Height = 1524. [MILLI METRE]
    Window Width = 304.8 [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
    Z Frame Thickness = 25. [MILLI METRE]
    Z Frame Width = 50. [MILLI METRE]
  AC_Equantity_D1_Commercial_21 | quantities | on 1 object (1 IFCDOOR)
    3D Closed Height = 0. [MILLI METRE]
    3D Closed Length = 0. [MILLI METRE]
    3D Opening Height = 1500. [MILLI METRE]
    3D Opening Length 1 = 560. [MILLI METRE]
    3D Opening Length 2 = 140. [MILLI METRE]
    3D Opening Length = 1500. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Box Axis Height from Header = 0. [MILLI METRE]
    Box Depth (gs_shutLam_boxWidth) = 150. [MILLI METRE]
    Box Depth (gs_shutRoll_boxWidth) = 150. [MILLI METRE]
    Box Height (gs_shutLam2_boxHeight) = 60. [MILLI METRE]
    Box Height (gs_shutLam_boxHeight) = 200. [MILLI METRE]
    Box Height (gs_shutRoll_boxHeight) = 200. [MILLI METRE]
    Box Left Offset = 0. [MILLI METRE]
    Box Right Offset = 0. [MILLI METRE]
    Box Width = 60. [MILLI METRE]
    Brick Thickness (gs_brick_sill_br_thk) = 65. [MILLI METRE]
    Brick Thickness (gs_masonry_arch_brick_thk) = 66.675 [MILLI METRE]
    Closer Thickness = 100. [MILLI METRE]
    Closer Width = 38. [MILLI METRE]
    Closing Depth = 0. [MILLI METRE]
    Cover Width = 0. [MILLI METRE]
    Custom Thickness = 15. [MILLI METRE]
    Dead Bolt Height = 1066.8 [MILLI METRE]
    Depth of Rails = 72.5 [MILLI METRE]
    Distance between Arch and Door = 0. [MILLI METRE]
    Distance from Header (gs_shutLam2_distFromHead) = 60. [MILLI METRE]
    Distance from Header (gs_shutLam_distFromHead) = 0. [MILLI METRE]
    Distance from Header (gs_shutRoll_distFromHead) = 0. [MILLI METRE]
    Distance from Wall (gs_shutLam_distFromWall) = 0. [MILLI METRE]
    Distance from Wall (gs_shutRoll_distFromWall) = 0. [MILLI METRE]
    Distance from Window = 60. [MILLI METRE]
    Distance of Skin from Closer = 0. [MILLI METRE]
    Door Panel Overlap Width = 50.8 [MILLI METRE]
    Door Stop Projection = 44.45 [MILLI METRE]
    Door Stop Thickness = 38.1 [MILLI METRE]
    Door Stop Width = 12.7 [MILLI METRE]
    Egress Height = 2019.3 [MILLI METRE]
    Egress Width = 990.190429156 [MILLI METRE]
    Ext. Threshold Overhang Inside = 50.8 [MILLI METRE]
    Ext. Threshold Overhang Outside = 50.8 [MILLI METRE]
    Extra Frame Thickness = 30. [MILLI METRE]
    Extra Frame Width = 40. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Thickness Inside = 101.6 [MILLI METRE]
    Frame Width = 50.8 [MILLI METRE]
    Frame Width Bottom = 50. [MILLI METRE]
    Frame Width Left = 50.8 [MILLI METRE]
    Frame Width Right = 50.8 [MILLI METRE]
    Frame Width Upper = 50.8 [MILLI METRE]
    Glass Thickness = 12.7 [MILLI METRE]
    Grid Thickness = 19.05 [MILLI METRE]
    Grid Width = 12.7 [MILLI METRE]
    Handle Height = 914.4 [MILLI METRE]
    Handle Position = 50.8 [MILLI METRE]
    Hanging Stick Length = 20. [MILLI METRE]
    Hanging Stick Radius = 5. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_left_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_right_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_left_out) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_right_out) = 0. [MILLI METRE]
    Head Jamb Depth = 31.75 [MILLI METRE]
    Head Width Inside = 63.5 [MILLI METRE]
    Head Width Outside = 63.5 [MILLI METRE]
    Hole Radius = 10. [MILLI METRE]
    Horizontal Boards Approximate Width = 115. [MILLI METRE]
    Horizontal Boards Thickness = 25. [MILLI METRE]
    Horizontal Frame Divider Width = 50. [MILLI METRE]
    Inner Head Depth (gs_reveal_double_innerTop) = 101.6 [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 101.6 [MILLI METRE]
    Inner Offset = 20. [MILLI METRE]
    Inner Panel Width = 120. [MILLI METRE]
    Inner Sill Depth (gs_reveal_double_innerBottom) = 101.6 [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 101.6 [MILLI METRE]
    Jamb Depth = 31.75 [MILLI METRE]
    Jamb Depth Side 2 = 31.75 [MILLI METRE]
    Jamb Extension Width = 12.7 [MILLI METRE]
    Jamb Extension Width Outside = 0. [MILLI METRE]
    Keystone Oversize = 0. [MILLI METRE]
    Keystone Projection = 10. [MILLI METRE]
    Keystone Width = 100. [MILLI METRE]
    Leaf Frame Width Internal = 25.4 [MILLI METRE]
    Leaf Frame Width Left = 101.6 [MILLI METRE]
    Leaf Frame Width Lower = 101.6 [MILLI METRE]
    Leaf Frame Width Right = 101.6 [MILLI METRE]
    Leaf Frame Width Side = 101.6 [MILLI METRE]
    Leaf Frame Width Upper = 101.6 [MILLI METRE]
    Leaf Height = 2032. [MILLI METRE]
    Leaf Thickness = 44.45 [MILLI METRE]
    Leaf Width = 1015.59042916 [MILLI METRE]
    Left Opening Oversize = 0. [MILLI METRE]
    Left Panel Width = 283.36875 [MILLI METRE]
    Louver Thickness = 10. [MILLI METRE]
    Louver Width = 40. [MILLI METRE]
    Lower Opening Oversize = 0. [MILLI METRE]
    Main Door Panel Width = 457.2 [MILLI METRE]
    Masonry Arch Depth = 101.6 [MILLI METRE]
    Masonry Arch Height = 203.2 [MILLI METRE]
    Masonry Arch Overhang Left = 0. [MILLI METRE]
    Masonry Arch Overhang Right = 0. [MILLI METRE]
    Masonry Arch Projection = 0. [MILLI METRE]
    Masonry Arch Rise = 50.8 [MILLI METRE]
    Middle Frame Width = 101.6 [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 15. [MILLI METRE]
    Mortar Thickness (gs_masonry_arch_mort_thk) = 9.525 [MILLI METRE]
    Offset Inside = 0. [MILLI METRE]
    Offset Outside = -63.5 [MILLI METRE]
    Offset from Edge if not Center = 152.4 [MILLI METRE]
    Opening Side Depth = 1524. [MILLI METRE]
    Opening Side Width 1 = 0. [MILLI METRE]
    Opening Side Width 2 = 457.2 [MILLI METRE]
    Opening Width in 2D = 0. [MILLI METRE]
    Opening Width in 3D = 0. [MILLI METRE]
    Opposite Side Width 2 = 304.8 [MILLI METRE]
    Outer Jamb Depth = 80. [MILLI METRE]
    Outside Overhang = 0. [MILLI METRE]
    Overhang 1 Left = 22.225 [MILLI METRE]
    Overhang 1 Right = 22.225 [MILLI METRE]
    Overhang 1 Upper = 22.225 [MILLI METRE]
    Panel Distance = 6. [MILLI METRE]
    Panel Fill Thickness = 10. [MILLI METRE]
    Panel Frame Width = 50.8 [MILLI METRE]
    Panel Height = 1500. [MILLI METRE]
    Panel Thickness = 50.8 [MILLI METRE]
    Panel Width = 0. [MILLI METRE]
    Plaster Thickness Limit = 38.1 [MILLI METRE]
    Profile Width = 150. [MILLI METRE]
    Rail Height = 914.4 [MILLI METRE]
    Rail Width = 38.1 [MILLI METRE]
    Rear Hole Depth = 0. [MILLI METRE]
    Rebate Width = 12.7 [MILLI METRE]
    Reveal Depth (AC_wido_sill) = 0. [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 0. [MILLI METRE]
    Reveal Height = 2082.8 [MILLI METRE]
    Reveal Width = 1117.19042916 [MILLI METRE]
    Reveal to Wall Core = 0. [MILLI METRE]
    Right Opening Oversize = 0. [MILLI METRE]
    Right Panel Width = 283.36875 [MILLI METRE]
    Segment Width (gs_shutLam2_segmentWidth) = 60. [MILLI METRE]
    Segment Width (gs_shutLam_segmentWidth) = 60. [MILLI METRE]
    Side Width Inside = 63.5 [MILLI METRE]
    Side Width Outside = 63.5 [MILLI METRE]
    Sidelight Frame Thickness = 38.1 [MILLI METRE]
    Sidelight Frame Width = 50.8 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left) = 355.6 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_half) = 150. [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_orig) = 300. [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right) = 355.6 [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_half) = 150. [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_orig) = 300. [MILLI METRE]
    Sill Height to Current Story = 263.525 [MILLI METRE]
    Sill Jamb Depth = 60. [MILLI METRE]
    Sill Nosing = 31.75 [MILLI METRE]
    Sill Overhang Left = 0. [MILLI METRE]
    Sill Overhang Right = 0. [MILLI METRE]
    Sill Slip-in Depth = 25.4 [MILLI METRE]
    Sill Thickness = 100. [MILLI METRE]
    Sill Top Height = 10. [MILLI METRE]
    Sill Top Width = 10. [MILLI METRE]
    Skin Overhang to Frame Depth = 0. [MILLI METRE]
    Slat Width = 50. [MILLI METRE]
    Strip Thickness = 25. [MILLI METRE]
    Thickness Inside = 31.75 [MILLI METRE]
    Thickness Outside = 31.75 [MILLI METRE]
    Threshold External Thickness = 5.80737765736 [MILLI METRE]
    Threshold Nosing Inside = 25.4 [MILLI METRE]
    Threshold Nosing Outside = 25.4 [MILLI METRE]
    Threshold Thickness = 12.7 [MILLI METRE]
    Threshold Width = 10. [MILLI METRE]
    Tolerance Left = 0. [MILLI METRE]
    Tolerance Lower = 0. [MILLI METRE]
    Tolerance Right = 0. [MILLI METRE]
    Tolerance Upper = 0. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Frame Thickness = 38.1 [MILLI METRE]
    Transom Frame Width = 50.8 [MILLI METRE]
    Transom Height = 355.6 [MILLI METRE]
    Unit Height = 2082.8 [MILLI METRE]
    Unit Width = 1117.19042916 [MILLI METRE]
    Upper Opening Oversize = 0. [MILLI METRE]
    Vertical Board Width = 100. [MILLI METRE]
    Vertical Boards Approximate Width = 80. [MILLI METRE]
    Vertical Boards Thickness = 25. [MILLI METRE]
    Vertical Frame Divider Width = 50. [MILLI METRE]
    Vertical Grid Height = 914.4 [MILLI METRE]
    Wallhole Height = 2082.8 [MILLI METRE]
    Wallhole Width = 1117.19042916 [MILLI METRE]
    Width Side (gs_tw_left_in) = 63.5 [MILLI METRE]
    Width Side (gs_tw_left_out) = 63.5 [MILLI METRE]
    Width of Sill = 0. [MILLI METRE]
    Window Height = 304.8 [MILLI METRE]
    Window Sill Height = 1524. [MILLI METRE]
    Window Width = 304.8 [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
    Z Frame Thickness = 25. [MILLI METRE]
    Z Frame Width = 50. [MILLI METRE]
  AC_Equantity_Commercial_Bath_Stall_21 | quantities | on 3 objects (3 IFCFLOWTERMINAL)
    Bottom Height = 203.2 [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Depth = 1676.4 [MILLI METRE]
    Divider Depth = 304.8 [MILLI METRE]
    Divider Elevation = 711.2 [MILLI METRE]
    Divider Height = 609.6 [MILLI METRE]
    Divider Width = 127. [MILLI METRE]
    Division Bottom Height = 0. [MILLI METRE]
    Division Height = 1828.8 [MILLI METRE]
    Division Thickness = 19.05 [MILLI METRE]
    Division Top Height = 2133.6 [MILLI METRE]
    Division Width on Hinge Side = 101.6 [MILLI METRE]
    Division Width on Lock Side = 101.6 [MILLI METRE]
    Door Bottom = 203.2 [MILLI METRE]
    Door Depth (ms_openingSDepth) = 1524. [MILLI METRE]
    Door Depth (ms_openingSDepth_in) = 1219.2 [MILLI METRE]
    Door Height = 1828.8 [MILLI METRE]
    Door Pull Height = 914.4 [MILLI METRE]
    Door Pull Position = 38.1 [MILLI METRE]
    Door Thickness = 19.05 [MILLI METRE]
    Door Width = 711.2 [MILLI METRE]
    Door on Side 1 (ms_openingSWidth1) = 0. [MILLI METRE]
    Door on Side 1 (ms_openingSWidth1_in) = 101.6 [MILLI METRE]
    Door on Side 2 (ms_openingSWidth2) = 406.4 [MILLI METRE]
    Door on Side 2 (ms_openingSWidth2_in) = 254. [MILLI METRE]
    Element Height = 19.05 [MILLI METRE]
    Element Width = 925.512763099 [MILLI METRE]
    End Division 1 Length = 1676.4 [MILLI METRE]
    End Division 2 Length = 1676.4 [MILLI METRE]
    Fixture in Front = 800. [MILLI METRE]
    Fixture on Side 1 = 300. [MILLI METRE]
    Fixture on Side 2 = 300. [MILLI METRE]
    Height = 2133.6 [MILLI METRE]
    Latch Height = 1066.8 [MILLI METRE]
    Latch Position = 38.1 [MILLI METRE]
    Left Overhang = 0. [MILLI METRE]
    Right Overhang = 0. [MILLI METRE]
    Screen End Length = 120. [MILLI METRE]
    Screen Length = 600. [MILLI METRE]
    Stall Depth = 1676.4 [MILLI METRE]
    Thickness = 19.05 [MILLI METRE]
    Top Division Height = 250. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Urinal Top Height = 762. [MILLI METRE]
    Urinal Width = 406.4 [MILLI METRE]
    Width = 1851.0255262 [MILLI METRE]
  AC_Equantity_Commercial_Bath_Stall_21 | quantities | on 3 objects (3 IFCFLOWTERMINAL)
    Bottom Height = 203.2 [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Depth = 1676.4 [MILLI METRE]
    Divider Depth = 304.8 [MILLI METRE]
    Divider Elevation = 711.2 [MILLI METRE]
    Divider Height = 609.6 [MILLI METRE]
    Divider Width = 127. [MILLI METRE]
    Division Bottom Height = 0. [MILLI METRE]
    Division Height = 1828.8 [MILLI METRE]
    Division Thickness = 19.05 [MILLI METRE]
    Division Top Height = 2133.6 [MILLI METRE]
    Division Width on Hinge Side = 101.6 [MILLI METRE]
    Division Width on Lock Side = 101.6 [MILLI METRE]
    Door Bottom = 203.2 [MILLI METRE]
    Door Depth (ms_openingSDepth) = 1524. [MILLI METRE]
    Door Depth (ms_openingSDepth_in) = 1219.2 [MILLI METRE]
    Door Height = 1828.8 [MILLI METRE]
    Door Pull Height = 914.4 [MILLI METRE]
    Door Pull Position = 38.1 [MILLI METRE]
    Door Thickness = 19.05 [MILLI METRE]
    Door Width = 711.2 [MILLI METRE]
    Door on Side 1 (ms_openingSWidth1) = 0. [MILLI METRE]
    Door on Side 1 (ms_openingSWidth1_in) = 101.6 [MILLI METRE]
    Door on Side 2 (ms_openingSWidth2) = 406.4 [MILLI METRE]
    Door on Side 2 (ms_openingSWidth2_in) = 254. [MILLI METRE]
    Element Height = 19.05 [MILLI METRE]
    Element Width = 914.4 [MILLI METRE]
    End Division 1 Length = 1676.4 [MILLI METRE]
    End Division 2 Length = 1676.4 [MILLI METRE]
    Fixture in Front = 609.6 [MILLI METRE]
    Fixture on Side 1 = 0. [MILLI METRE]
    Fixture on Side 2 = 0. [MILLI METRE]
    Height = 2133.6 [MILLI METRE]
    Latch Height = 1066.8 [MILLI METRE]
    Latch Position = 38.1 [MILLI METRE]
    Left Overhang = 0. [MILLI METRE]
    Right Overhang = 0. [MILLI METRE]
    Screen End Length = 120. [MILLI METRE]
    Screen Length = 600. [MILLI METRE]
    Stall Depth = 1676.4 [MILLI METRE]
    Thickness = 19.05 [MILLI METRE]
    Top Division Height = 250. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Urinal Top Height = 762. [MILLI METRE]
    Urinal Width = 406.4 [MILLI METRE]
    Width = 914.4 [MILLI METRE]
  AC_Equantity_Toilet_ADA_21 | quantities | on 3 objects (3 IFCFLOWTERMINAL)
    Axis Distance from Wall = 815. [MILLI METRE]
    Axis from Seat = 180. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Bowl Depth = 609.6 [MILLI METRE]
    Bowl Height = 430. [MILLI METRE]
    Bowl Width = 355.6 [MILLI METRE]
    Carrier Depth = 120. [MILLI METRE]
    Carrier Height = 1200. [MILLI METRE]
    Carrier Width = 500. [MILLI METRE]
    Cistern Depth = 203.2 [MILLI METRE]
    Cistern Elevation = 1200. [MILLI METRE]
    Cistern Height = 304.8 [MILLI METRE]
    Cistern Width = 457.2 [MILLI METRE]
    Connection Length (ConLength_1) = 20. [MILLI METRE]
    Connection Length (ConLength_2) = 20. [MILLI METRE]
    Connection Position X (ConPosX_1) = 0. [MILLI METRE]
    Connection Position X (ConPosX_2) = 0. [MILLI METRE]
    Connection Position Y (ConPosY_1) = -25.4 [MILLI METRE]
    Connection Position Y (ConPosY_2) = -157.661428571 [MILLI METRE]
    Connection Position Z (ConPosZ_1) = 684. [MILLI METRE]
    Connection Position Z (ConPosZ_2) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_1) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_2) = 0. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_1) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_2) = 120.65 [MILLI METRE]
    Connector Width (ConConnectorWidth2_1) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_2) = 6.35 [MILLI METRE]
    Dimension 1 = 355.6 [MILLI METRE]
    Dimension 2 = 609.6 [MILLI METRE]
    Distance from Floor = 381. [MILLI METRE]
    Distance from Wall = 25.4 [MILLI METRE]
    Grab Bar Diameter = 25.4 [MILLI METRE]
    Grab Bars Distance from Floor = 914.4 [MILLI METRE]
    Grip Diameter = 38.1 [MILLI METRE]
    Height = 430. [MILLI METRE]
    Minimal Space in Front = 1016. [MILLI METRE]
    Minimal Space on Side 1 = 917.2 [MILLI METRE]
    Minimal Space on Side 2 = 252.2 [MILLI METRE]
    Nominal Depth (ConNominalDepth_1) = 30. [MILLI METRE]
    Nominal Depth (ConNominalDepth_2) = 110. [MILLI METRE]
    Outer Depth (ConDepth_1) = 31.75 [MILLI METRE]
    Outer Depth (ConDepth_2) = 114.3 [MILLI METRE]
    Outer Diameter (ConWidth_1) = 31.75 [MILLI METRE]
    Outer Diameter (ConWidth_2) = 114.3 [MILLI METRE]
    Pipe Diameter = 30. [MILLI METRE]
    Rear Grab Bar Length 1 = 610. [MILLI METRE]
    Rear Grab Bar Length 2 = 305. [MILLI METRE]
    Seat Height = 430. [MILLI METRE]
    Side Grab Bar Distance from Wall = 304.8 [MILLI METRE]
    Side Grab Bar Length = 1065. [MILLI METRE]
    Toilet Axis Distance from Wall = 430. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Vertical Grab Bar Distance = 1016. [MILLI METRE]
    Vertical Grab Bar Distance from Floor = 1016. [MILLI METRE]
    Vertical Grab Bar Length = 457.2 [MILLI METRE]
    Wall Thickness (ConWallThickness_1) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_2) = 3.175 [MILLI METRE]
    Water Connection Height = 755. [MILLI METRE]
  AC_Equantity_Basin_21 | quantities | on 3 objects (3 IFCFLOWTERMINAL)
    Basin Depth = 584.2 [MILLI METRE]
    Basin Width = 685.8 [MILLI METRE]
    Bottom Level = 711.2 [MILLI METRE]
    Connection Length (ConLength_1) = 20. [MILLI METRE]
    Connection Length (ConLength_2) = 20. [MILLI METRE]
    Connection Length (ConLength_3) = 20. [MILLI METRE]
    Connection Position X (ConPosX_1) = -88.9 [MILLI METRE]
    Connection Position X (ConPosX_2) = 88.9 [MILLI METRE]
    Connection Position X (ConPosX_3) = 0. [MILLI METRE]
    Connection Position Y (ConPosY_1) = 0. [MILLI METRE]
    Connection Position Y (ConPosY_2) = 0. [MILLI METRE]
    Connection Position Y (ConPosY_3) = -246.94134 [MILLI METRE]
    Connection Position Z (ConPosZ_1) = -38.1 [MILLI METRE]
    Connection Position Z (ConPosZ_2) = -38.1 [MILLI METRE]
    Connection Position Z (ConPosZ_3) = 68.58 [MILLI METRE]
    Connector Depth (ConConnectorDepth_1) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_2) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_3) = 0. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_1) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_2) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_3) = 38.1 [MILLI METRE]
    Connector Width (ConConnectorWidth2_1) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_2) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_3) = 6.35 [MILLI METRE]
    Height = 203.2 [MILLI METRE]
    Minimal Space in Front = 1092.2 [MILLI METRE]
    Minimal Space on Side 1 = 165.1 [MILLI METRE]
    Minimal Space on Side 2 = 228.6 [MILLI METRE]
    Nominal Depth (ConNominalDepth_1) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_2) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_3) = 40. [MILLI METRE]
    Outer Depth (ConDepth_1) = 31.75 [MILLI METRE]
    Outer Depth (ConDepth_2) = 31.75 [MILLI METRE]
    Outer Depth (ConDepth_3) = 38.1 [MILLI METRE]
    Outer Diameter (ConWidth_1) = 31.75 [MILLI METRE]
    Outer Diameter (ConWidth_2) = 31.75 [MILLI METRE]
    Outer Diameter (ConWidth_3) = 38.1 [MILLI METRE]
    Tap Height = 990.63 [MILLI METRE]
    Tap X Position = 0. [MILLI METRE]
    Tap Y Position = 0. [MILLI METRE]
    Tap Z Position = 0. [MILLI METRE]
    Top Height = 914.4 [MILLI METRE]
    Top Level = 914.4 [MILLI METRE]
    Wall Thickness (ConWallThickness_1) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_2) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_3) = 3.175 [MILLI METRE]
  AC_Equantity_Urinal_21 | quantities | on 3 objects (3 IFCFLOWTERMINAL)
    Basin Front Height = 558.8 [MILLI METRE]
    Basin Front Height From Bottom = 347.2445 [MILLI METRE]
    Bottom Level = 248.98604 [MILLI METRE]
    Connection Length (ConLength_1) = 40. [MILLI METRE]
    Connection Length (ConLength_2) = 20. [MILLI METRE]
    Connection Position X (ConPosX_1) = 0. [MILLI METRE]
    Connection Position X (ConPosX_2) = 0. [MILLI METRE]
    Connection Position Y (ConPosY_1) = -15.875 [MILLI METRE]
    Connection Position Y (ConPosY_2) = -166.624 [MILLI METRE]
    Connection Position Z (ConPosZ_1) = 0. [MILLI METRE]
    Connection Position Z (ConPosZ_2) = -736.6 [MILLI METRE]
    Connector Depth (ConConnectorDepth_1) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_2) = 0. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_1) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_2) = 38.1 [MILLI METRE]
    Connector Width (ConConnectorWidth2_1) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_2) = 6.35 [MILLI METRE]
    Depth = 406.4 [MILLI METRE]
    Half A = 165. [MILLI METRE]
    Height = 736.6 [MILLI METRE]
    Minimal Space in Front = 685.8 [MILLI METRE]
    Minimal Space on Side 1 = 203.2 [MILLI METRE]
    Minimal Space on Side 2 = 203.2 [MILLI METRE]
    Nominal Depth (ConNominalDepth_1) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_2) = 40. [MILLI METRE]
    Outer Depth (ConDepth_1) = 31.75 [MILLI METRE]
    Outer Depth (ConDepth_2) = 38.1 [MILLI METRE]
    Outer Diameter (ConWidth_1) = 31.75 [MILLI METRE]
    Outer Diameter (ConWidth_2) = 38.1 [MILLI METRE]
    Top Level = 558.8 [MILLI METRE]
    Wall Thickness (ConWallThickness_1) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_2) = 3.175 [MILLI METRE]
    Width = 406.4 [MILLI METRE]
  AC_Equantity_Multi-Basin_Counter_21 | quantities | on 3 objects (3 IFCFLOWTERMINAL)
    Back and Side Splash Height = 101.6 [MILLI METRE]
    Basin Depth = 304.8 [MILLI METRE]
    Basin Distance from Center = 0. [MILLI METRE]
    Basin Spacing = 355.653372447 [MILLI METRE]
    Basin Width = 457.2 [MILLI METRE]
    Basin Y Distance from Counter Center = 0. [MILLI METRE]
    Bottom Level = 825.5 [MILLI METRE]
    Connection Length (ConLength_1) = 20. [MILLI METRE]
    Connection Length (ConLength_10) = 20. [MILLI METRE]
    Connection Length (ConLength_11) = 20. [MILLI METRE]
    Connection Length (ConLength_12) = 20. [MILLI METRE]
    Connection Length (ConLength_13) = 20. [MILLI METRE]
    Connection Length (ConLength_14) = 20. [MILLI METRE]
    Connection Length (ConLength_15) = 20. [MILLI METRE]
    Connection Length (ConLength_16) = 20. [MILLI METRE]
    Connection Length (ConLength_17) = 20. [MILLI METRE]
    Connection Length (ConLength_2) = 20. [MILLI METRE]
    Connection Length (ConLength_3) = 20. [MILLI METRE]
    Connection Length (ConLength_4) = 20. [MILLI METRE]
    Connection Length (ConLength_5) = 20. [MILLI METRE]
    Connection Length (ConLength_6) = 20. [MILLI METRE]
    Connection Length (ConLength_7) = 20. [MILLI METRE]
    Connection Length (ConLength_8) = 20. [MILLI METRE]
    Connection Length (ConLength_9) = 20. [MILLI METRE]
    Connection Position X (ConPosX_1) = -100. [MILLI METRE]
    Connection Position X (ConPosX_10) = 1280. [MILLI METRE]
    Connection Position X (ConPosX_11) = 1480. [MILLI METRE]
    Connection Position X (ConPosX_12) = 1380. [MILLI METRE]
    Connection Position X (ConPosX_13) = 1970. [MILLI METRE]
    Connection Position X (ConPosX_14) = 2170. [MILLI METRE]
    Connection Position X (ConPosX_15) = 2070. [MILLI METRE]
    Connection Position X (ConPosX_16) = 2660. [MILLI METRE]
    Connection Position X (ConPosX_2) = 100. [MILLI METRE]
    Connection Position X (ConPosX_3) = 0. [MILLI METRE]
    Connection Position X (ConPosX_4) = -100. [MILLI METRE]
    Connection Position X (ConPosX_5) = 100. [MILLI METRE]
    Connection Position X (ConPosX_6) = 0. [MILLI METRE]
    Connection Position X (ConPosX_7) = -100. [MILLI METRE]
    Connection Position X (ConPosX_8) = 100. [MILLI METRE]
    Connection Position X (ConPosX_9) = 0. [MILLI METRE]
    Connection Position Y (ConPosY_1) = -15.875 [MILLI METRE]
    Connection Position Y (ConPosY_10) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_11) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_12) = -158.90845 [MILLI METRE]
    Connection Position Y (ConPosY_13) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_14) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_15) = -158.90845 [MILLI METRE]
    Connection Position Y (ConPosY_16) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_2) = -15.875 [MILLI METRE]
    Connection Position Y (ConPosY_3) = -169.864532 [MILLI METRE]
    Connection Position Y (ConPosY_4) = -15.875 [MILLI METRE]
    Connection Position Y (ConPosY_5) = -15.875 [MILLI METRE]
    Connection Position Y (ConPosY_6) = -169.864532 [MILLI METRE]
    Connection Position Y (ConPosY_7) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_8) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_9) = -158.90845 [MILLI METRE]
    Connection Position Z (ConPosZ_1) = -38.1 [MILLI METRE]
    Connection Position Z (ConPosZ_10) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_11) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_12) = -167. [MILLI METRE]
    Connection Position Z (ConPosZ_13) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_14) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_15) = -167. [MILLI METRE]
    Connection Position Z (ConPosZ_16) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_2) = -38.1 [MILLI METRE]
    Connection Position Z (ConPosZ_3) = -180.1 [MILLI METRE]
    Connection Position Z (ConPosZ_4) = -38.1 [MILLI METRE]
    Connection Position Z (ConPosZ_5) = -38.1 [MILLI METRE]
    Connection Position Z (ConPosZ_6) = -180.1 [MILLI METRE]
    Connection Position Z (ConPosZ_7) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_8) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_9) = -167. [MILLI METRE]
    Connector Depth (ConConnectorDepth_1) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_10) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_11) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_12) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_13) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_14) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_15) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_16) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_2) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_3) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_4) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_5) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_6) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_7) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_8) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_9) = 0. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_1) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_10) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_11) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_12) = 42. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_13) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_14) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_15) = 42. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_16) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_2) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_3) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_4) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_5) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_6) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_7) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_8) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_9) = 42. [MILLI METRE]
    Connector Width (ConConnectorWidth2_1) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_10) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_11) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_12) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_13) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_14) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_15) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_16) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_2) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_3) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_4) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_5) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_6) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_7) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_8) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_9) = 5. [MILLI METRE]
    Counter Top Height = 863.6 [MILLI METRE]
    Countertop Depth = 508. [MILLI METRE]
    Countertop Half Width = 812.853372447 [MILLI METRE]
    Countertop Thickness = 38.1 [MILLI METRE]
    Countertop Width = 1625.70674489 [MILLI METRE]
    Distance of End Basin from End Left = 177.826686224 [MILLI METRE]
    Distance of End Basin from End Right = 177.826686224 [MILLI METRE]
    Front Face Panel Height = 152.4 [MILLI METRE]
    Front Face Panel Overhang = 63.5 [MILLI METRE]
    Height = 38.1 [MILLI METRE]
    Nominal Depth (ConNominalDepth_1) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_10) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_11) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_12) = 40. [MILLI METRE]
    Nominal Depth (ConNominalDepth_13) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_14) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_15) = 40. [MILLI METRE]
    Nominal Depth (ConNominalDepth_16) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_17) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_2) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_3) = 40. [MILLI METRE]
    Nominal Depth (ConNominalDepth_4) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_5) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_6) = 40. [MILLI METRE]
    Nominal Depth (ConNominalDepth_7) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_8) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_9) = 40. [MILLI METRE]
    Outer Depth (ConDepth_1) = 31.75 [MILLI METRE]
    Outer Depth (ConDepth_10) = 27. [MILLI METRE]
    Outer Depth (ConDepth_11) = 27. [MILLI METRE]
    Outer Depth (ConDepth_12) = 42. [MILLI METRE]
    Outer Depth (ConDepth_13) = 27. [MILLI METRE]
    Outer Depth (ConDepth_14) = 27. [MILLI METRE]
    Outer Depth (ConDepth_15) = 42. [MILLI METRE]
    Outer Depth (ConDepth_16) = 27. [MILLI METRE]
    Outer Depth (ConDepth_17) = 27. [MILLI METRE]
    Outer Depth (ConDepth_2) = 31.75 [MILLI METRE]
    Outer Depth (ConDepth_3) = 38.1 [MILLI METRE]
    Outer Depth (ConDepth_4) = 31.75 [MILLI METRE]
    Outer Depth (ConDepth_5) = 31.75 [MILLI METRE]
    Outer Depth (ConDepth_6) = 38.1 [MILLI METRE]
    Outer Depth (ConDepth_7) = 27. [MILLI METRE]
    Outer Depth (ConDepth_8) = 27. [MILLI METRE]
    Outer Depth (ConDepth_9) = 42. [MILLI METRE]
    Outer Diameter (ConWidth_1) = 31.75 [MILLI METRE]
    Outer Diameter (ConWidth_10) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_11) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_12) = 42. [MILLI METRE]
    Outer Diameter (ConWidth_13) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_14) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_15) = 42. [MILLI METRE]
    Outer Diameter (ConWidth_16) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_17) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_2) = 31.75 [MILLI METRE]
    Outer Diameter (ConWidth_3) = 38.1 [MILLI METRE]
    Outer Diameter (ConWidth_4) = 31.75 [MILLI METRE]
    Outer Diameter (ConWidth_5) = 31.75 [MILLI METRE]
    Outer Diameter (ConWidth_6) = 38.1 [MILLI METRE]
    Outer Diameter (ConWidth_7) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_8) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_9) = 42. [MILLI METRE]
    Tap Height = 1200. [MILLI METRE]
    Top Level = 863.6 [MILLI METRE]
    Wall Thickness (ConWallThickness_1) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_10) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_11) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_12) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_13) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_14) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_15) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_16) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_17) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_2) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_3) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_4) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_5) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_6) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_7) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_8) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_9) = 1. [MILLI METRE]
  AC_Equantity_Multi-Basin_Counter_21 | quantities | on 3 objects (3 IFCFLOWTERMINAL)
    Back and Side Splash Height = 101.6 [MILLI METRE]
    Basin Depth = 304.8 [MILLI METRE]
    Basin Distance from Center = 0. [MILLI METRE]
    Basin Spacing = 355.6 [MILLI METRE]
    Basin Width = 457.2 [MILLI METRE]
    Basin Y Distance from Counter Center = 0. [MILLI METRE]
    Bottom Level = 825.5 [MILLI METRE]
    Connection Length (ConLength_1) = 20. [MILLI METRE]
    Connection Length (ConLength_10) = 20. [MILLI METRE]
    Connection Length (ConLength_11) = 20. [MILLI METRE]
    Connection Length (ConLength_12) = 20. [MILLI METRE]
    Connection Length (ConLength_13) = 20. [MILLI METRE]
    Connection Length (ConLength_14) = 20. [MILLI METRE]
    Connection Length (ConLength_15) = 20. [MILLI METRE]
    Connection Length (ConLength_16) = 20. [MILLI METRE]
    Connection Length (ConLength_17) = 20. [MILLI METRE]
    Connection Length (ConLength_2) = 20. [MILLI METRE]
    Connection Length (ConLength_3) = 20. [MILLI METRE]
    Connection Length (ConLength_4) = 20. [MILLI METRE]
    Connection Length (ConLength_5) = 20. [MILLI METRE]
    Connection Length (ConLength_6) = 20. [MILLI METRE]
    Connection Length (ConLength_7) = 20. [MILLI METRE]
    Connection Length (ConLength_8) = 20. [MILLI METRE]
    Connection Length (ConLength_9) = 20. [MILLI METRE]
    Connection Position X (ConPosX_1) = -100. [MILLI METRE]
    Connection Position X (ConPosX_10) = 1280. [MILLI METRE]
    Connection Position X (ConPosX_11) = 1480. [MILLI METRE]
    Connection Position X (ConPosX_12) = 1380. [MILLI METRE]
    Connection Position X (ConPosX_13) = 1970. [MILLI METRE]
    Connection Position X (ConPosX_14) = 2170. [MILLI METRE]
    Connection Position X (ConPosX_15) = 2070. [MILLI METRE]
    Connection Position X (ConPosX_16) = 2660. [MILLI METRE]
    Connection Position X (ConPosX_2) = 100. [MILLI METRE]
    Connection Position X (ConPosX_3) = 0. [MILLI METRE]
    Connection Position X (ConPosX_4) = -100. [MILLI METRE]
    Connection Position X (ConPosX_5) = 100. [MILLI METRE]
    Connection Position X (ConPosX_6) = 0. [MILLI METRE]
    Connection Position X (ConPosX_7) = -100. [MILLI METRE]
    Connection Position X (ConPosX_8) = 100. [MILLI METRE]
    Connection Position X (ConPosX_9) = 0. [MILLI METRE]
    Connection Position Y (ConPosY_1) = -15.875 [MILLI METRE]
    Connection Position Y (ConPosY_10) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_11) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_12) = -158.90845 [MILLI METRE]
    Connection Position Y (ConPosY_13) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_14) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_15) = -158.90845 [MILLI METRE]
    Connection Position Y (ConPosY_16) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_2) = -15.875 [MILLI METRE]
    Connection Position Y (ConPosY_3) = -169.864532 [MILLI METRE]
    Connection Position Y (ConPosY_4) = -15.875 [MILLI METRE]
    Connection Position Y (ConPosY_5) = -15.875 [MILLI METRE]
    Connection Position Y (ConPosY_6) = -169.864532 [MILLI METRE]
    Connection Position Y (ConPosY_7) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_8) = -13.5 [MILLI METRE]
    Connection Position Y (ConPosY_9) = -158.90845 [MILLI METRE]
    Connection Position Z (ConPosZ_1) = -38.1 [MILLI METRE]
    Connection Position Z (ConPosZ_10) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_11) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_12) = -167. [MILLI METRE]
    Connection Position Z (ConPosZ_13) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_14) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_15) = -167. [MILLI METRE]
    Connection Position Z (ConPosZ_16) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_2) = -38.1 [MILLI METRE]
    Connection Position Z (ConPosZ_3) = -180.1 [MILLI METRE]
    Connection Position Z (ConPosZ_4) = -38.1 [MILLI METRE]
    Connection Position Z (ConPosZ_5) = -38.1 [MILLI METRE]
    Connection Position Z (ConPosZ_6) = -180.1 [MILLI METRE]
    Connection Position Z (ConPosZ_7) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_8) = -25. [MILLI METRE]
    Connection Position Z (ConPosZ_9) = -167. [MILLI METRE]
    Connector Depth (ConConnectorDepth_1) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_10) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_11) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_12) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_13) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_14) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_15) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_16) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_2) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_3) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_4) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_5) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_6) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_7) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_8) = 0. [MILLI METRE]
    Connector Depth (ConConnectorDepth_9) = 0. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_1) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_10) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_11) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_12) = 42. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_13) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_14) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_15) = 42. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_16) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_2) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_3) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_4) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_5) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_6) = 38.1 [MILLI METRE]
    Connector Diameter (ConConnectorWidth_7) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_8) = 40. [MILLI METRE]
    Connector Diameter (ConConnectorWidth_9) = 42. [MILLI METRE]
    Connector Width (ConConnectorWidth2_1) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_10) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_11) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_12) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_13) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_14) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_15) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_16) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_2) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_3) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_4) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_5) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_6) = 6.35 [MILLI METRE]
    Connector Width (ConConnectorWidth2_7) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_8) = 5. [MILLI METRE]
    Connector Width (ConConnectorWidth2_9) = 5. [MILLI METRE]
    Counter Top Height = 863.6 [MILLI METRE]
    Countertop Depth = 508. [MILLI METRE]
    Countertop Half Width = 812.8 [MILLI METRE]
    Countertop Thickness = 38.1 [MILLI METRE]
    Countertop Width = 1625.6 [MILLI METRE]
    Distance of End Basin from End Left = 177.8 [MILLI METRE]
    Distance of End Basin from End Right = 177.8 [MILLI METRE]
    Front Face Panel Height = 152.4 [MILLI METRE]
    Front Face Panel Overhang = 63.5 [MILLI METRE]
    Height = 38.1 [MILLI METRE]
    Nominal Depth (ConNominalDepth_1) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_10) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_11) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_12) = 40. [MILLI METRE]
    Nominal Depth (ConNominalDepth_13) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_14) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_15) = 40. [MILLI METRE]
    Nominal Depth (ConNominalDepth_16) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_17) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_2) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_3) = 40. [MILLI METRE]
    Nominal Depth (ConNominalDepth_4) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_5) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_6) = 40. [MILLI METRE]
    Nominal Depth (ConNominalDepth_7) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_8) = 25. [MILLI METRE]
    Nominal Depth (ConNominalDepth_9) = 40. [MILLI METRE]
    Outer Depth (ConDepth_1) = 31.75 [MILLI METRE]
    Outer Depth (ConDepth_10) = 27. [MILLI METRE]
    Outer Depth (ConDepth_11) = 27. [MILLI METRE]
    Outer Depth (ConDepth_12) = 42. [MILLI METRE]
    Outer Depth (ConDepth_13) = 27. [MILLI METRE]
    Outer Depth (ConDepth_14) = 27. [MILLI METRE]
    Outer Depth (ConDepth_15) = 42. [MILLI METRE]
    Outer Depth (ConDepth_16) = 27. [MILLI METRE]
    Outer Depth (ConDepth_17) = 27. [MILLI METRE]
    Outer Depth (ConDepth_2) = 31.75 [MILLI METRE]
    Outer Depth (ConDepth_3) = 38.1 [MILLI METRE]
    Outer Depth (ConDepth_4) = 31.75 [MILLI METRE]
    Outer Depth (ConDepth_5) = 31.75 [MILLI METRE]
    Outer Depth (ConDepth_6) = 38.1 [MILLI METRE]
    Outer Depth (ConDepth_7) = 27. [MILLI METRE]
    Outer Depth (ConDepth_8) = 27. [MILLI METRE]
    Outer Depth (ConDepth_9) = 42. [MILLI METRE]
    Outer Diameter (ConWidth_1) = 31.75 [MILLI METRE]
    Outer Diameter (ConWidth_10) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_11) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_12) = 42. [MILLI METRE]
    Outer Diameter (ConWidth_13) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_14) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_15) = 42. [MILLI METRE]
    Outer Diameter (ConWidth_16) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_17) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_2) = 31.75 [MILLI METRE]
    Outer Diameter (ConWidth_3) = 38.1 [MILLI METRE]
    Outer Diameter (ConWidth_4) = 31.75 [MILLI METRE]
    Outer Diameter (ConWidth_5) = 31.75 [MILLI METRE]
    Outer Diameter (ConWidth_6) = 38.1 [MILLI METRE]
    Outer Diameter (ConWidth_7) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_8) = 27. [MILLI METRE]
    Outer Diameter (ConWidth_9) = 42. [MILLI METRE]
    Tap Height = 1200. [MILLI METRE]
    Top Level = 863.6 [MILLI METRE]
    Wall Thickness (ConWallThickness_1) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_10) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_11) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_12) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_13) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_14) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_15) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_16) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_17) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_2) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_3) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_4) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_5) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_6) = 3.175 [MILLI METRE]
    Wall Thickness (ConWallThickness_7) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_8) = 1. [MILLI METRE]
    Wall Thickness (ConWallThickness_9) = 1. [MILLI METRE]
  AC_Equantity_Sofa_Layout_21 | quantities | on 1 object (1 IFCFURNISHINGELEMENT)
    Arm Height = 600. [MILLI METRE]
    Armchair Depth = 762. [MILLI METRE]
    Armchair Width = 762. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Dimension 1 = 1981.2 [MILLI METRE]
    Dimension 2 = 2692.4 [MILLI METRE]
    Dist. behind Armchair = 200. [MILLI METRE]
    Distance between Seats = 203.2 [MILLI METRE]
    Height = 800. [MILLI METRE]
    Leg Height = 101.6 [MILLI METRE]
    Leg Width = 38.1 [MILLI METRE]
    Minimal Space Depth = 1981.2 [MILLI METRE]
    Minimal Space Width = 2892.4 [MILLI METRE]
    Shelf Position = 250. [MILLI METRE]
    Shelf Thickness = 20. [MILLI METRE]
    Sitting Height = 450. [MILLI METRE]
    Sofa Depth = 914.4 [MILLI METRE]
    Sofa Width on the Bottom = 1600. [MILLI METRE]
    Sofa Width on the Top = 1981.2 [MILLI METRE]
    Table Depth = 609.6 [MILLI METRE]
    Table Width = 1219.2 [MILLI METRE]
    Tabletop Height = 457.2 [MILLI METRE]
    Tabletop Overhang X = 40. [MILLI METRE]
    Tabletop Overhang Y = 40. [MILLI METRE]
    Tabletop Thickness = 38.1 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Equantity_Sofa_Layout_21 | quantities | on 1 object (1 IFCFURNISHINGELEMENT)
    Arm Height = 600. [MILLI METRE]
    Armchair Depth = 762. [MILLI METRE]
    Armchair Width = 762. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Dimension 1 = 3911.6 [MILLI METRE]
    Dimension 2 = 2844.8 [MILLI METRE]
    Dist. behind Armchair = 200. [MILLI METRE]
    Distance between Seats = 203.2 [MILLI METRE]
    Height = 800. [MILLI METRE]
    Leg Height = 101.6 [MILLI METRE]
    Leg Width = 38.1 [MILLI METRE]
    Minimal Space Depth = 4311.6 [MILLI METRE]
    Minimal Space Width = 3044.8 [MILLI METRE]
    Shelf Position = 250. [MILLI METRE]
    Shelf Thickness = 20. [MILLI METRE]
    Sitting Height = 450. [MILLI METRE]
    Sofa Depth = 914.4 [MILLI METRE]
    Sofa Width on the Bottom = 1600. [MILLI METRE]
    Sofa Width on the Top = 1981.2 [MILLI METRE]
    Table Depth = 609.6 [MILLI METRE]
    Table Width = 1219.2 [MILLI METRE]
    Tabletop Height = 457.2 [MILLI METRE]
    Tabletop Overhang X = 40. [MILLI METRE]
    Tabletop Overhang Y = 40. [MILLI METRE]
    Tabletop Thickness = 38.1 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Equantity_Pendant_Lamp_21 | quantities | on 44 objects (44 IFCFLOWTERMINAL)
    Bottom Diameter = 790.512292605 [MILLI METRE]
    Bottom Dimension = 395.256146303 [MILLI METRE]
    Bottom Level = -1524. [MILLI METRE]
    Bottom Width = 400. [MILLI METRE]
    Diameter (D2) = 250. [MILLI METRE]
    Diameter (diameter) = 500. [MILLI METRE]
    Height = 1524. [MILLI METRE]
    Light Distance = 1600. [MILLI METRE]
    Rod Thickness = 20. [MILLI METRE]
    Shade Height = 72. [MILLI METRE]
    Shade Thickness = 1. [MILLI METRE]
    Symbol Depth = 450. [MILLI METRE]
    Symbol Size = 300. [MILLI METRE]
    Symbol Width = 700. [MILLI METRE]
    Text (txt_pos_x) = 200. [MILLI METRE]
    Text (txt_pos_y) = -100. [MILLI METRE]
    Top Diameter = 400. [MILLI METRE]
    Top Dimension = 200. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Top Width = 200. [MILLI METRE]
    Width (A) = 56. [MILLI METRE]
    Width (A2) = 395.256146303 [MILLI METRE]
    Width (B) = 56. [MILLI METRE]
    Width (width) = 790.512292605 [MILLI METRE]
  AC_Equantity_Pendant_Lamp_21 | quantities | on 41 objects (41 IFCFLOWTERMINAL)
    Bottom Diameter = 790.512292605 [MILLI METRE]
    Bottom Dimension = 395.256146303 [MILLI METRE]
    Bottom Level = -1524. [MILLI METRE]
    Bottom Width = 400. [MILLI METRE]
    Diameter (D2) = 250. [MILLI METRE]
    Diameter (diameter) = 500. [MILLI METRE]
    Height = 1524. [MILLI METRE]
    Light Distance = 1600. [MILLI METRE]
    Rod Thickness = 20. [MILLI METRE]
    Shade Height = 300. [MILLI METRE]
    Shade Thickness = 1. [MILLI METRE]
    Symbol Depth = 450. [MILLI METRE]
    Symbol Size = 300. [MILLI METRE]
    Symbol Width = 700. [MILLI METRE]
    Text (txt_pos_x) = 200. [MILLI METRE]
    Text (txt_pos_y) = -100. [MILLI METRE]
    Top Diameter = 400. [MILLI METRE]
    Top Dimension = 200. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Top Width = 200. [MILLI METRE]
    Width (A) = 790.512292605 [MILLI METRE]
    Width (A2) = 395.256146303 [MILLI METRE]
    Width (B) = 790.512292605 [MILLI METRE]
    Width (width) = 790.512292605 [MILLI METRE]
  AC_Equantity_Pendant_Lamp_21 | quantities | on 1 object (1 IFCFLOWTERMINAL)
    Bottom Diameter = 790.512292605 [MILLI METRE]
    Bottom Dimension = 395.256146303 [MILLI METRE]
    Bottom Level = -1585.43342619 [MILLI METRE]
    Bottom Width = 400. [MILLI METRE]
    Diameter (D2) = 250. [MILLI METRE]
    Diameter (diameter) = 500. [MILLI METRE]
    Height = 1585.43342619 [MILLI METRE]
    Light Distance = 1600. [MILLI METRE]
    Rod Thickness = 20. [MILLI METRE]
    Shade Height = 300. [MILLI METRE]
    Shade Thickness = 1. [MILLI METRE]
    Symbol Depth = 450. [MILLI METRE]
    Symbol Size = 300. [MILLI METRE]
    Symbol Width = 700. [MILLI METRE]
    Text (txt_pos_x) = 200. [MILLI METRE]
    Text (txt_pos_y) = -100. [MILLI METRE]
    Top Diameter = 400. [MILLI METRE]
    Top Dimension = 200. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Top Width = 200. [MILLI METRE]
    Width (A) = 790.512292605 [MILLI METRE]
    Width (A2) = 395.256146303 [MILLI METRE]
    Width (B) = 790.512292605 [MILLI METRE]
    Width (width) = 790.512292605 [MILLI METRE]
  AC_Equantity_Dining_Table_Rectangle_21 | quantities | on 9 objects (9 IFCFURNISHINGELEMENT)
    Additional Side Space for Wheelchair = 304.8 [MILLI METRE]
    Additional Table Width = 203.2 [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Chair Depth = 457.2 [MILLI METRE]
    Chair Height = 838.2 [MILLI METRE]
    Chair Width = 406.4 [MILLI METRE]
    Chair-Table Distance = 38.1 [MILLI METRE]
    Depth for Wheelchair = 863.6 [MILLI METRE]
    Depth per Chair = 800.1 [MILLI METRE]
    Dimension 1 = 1219.2 [MILLI METRE]
    Dimension 2 = 1752.6 [MILLI METRE]
    Distance behind Chair = 304.8 [MILLI METRE]
    Distance behind Wheelchair = 304.8 [MILLI METRE]
    Distance next to Wheelchair = 304.8 [MILLI METRE]
    Height = 838.2 [MILLI METRE]
    Leg Width = 38.1 [MILLI METRE]
    Min. Chair-Chair Distance = 50.8 [MILLI METRE]
    Real Chair Distance Horizontal = 203.2 [MILLI METRE]
    Real Chair Distance Vertical = 355.6 [MILLI METRE]
    Seat Height = 406.4 [MILLI METRE]
    Table Half Length = 609.6 [MILLI METRE]
    Table Half Width = 381. [MILLI METRE]
    Table Height = 762. [MILLI METRE]
    Table Length = 1219.2 [MILLI METRE]
    Table Width = 762. [MILLI METRE]
    Table Width for Chairs = 1422.4 [MILLI METRE]
    Tabletop Overhang X = 100. [MILLI METRE]
    Tabletop Overhang Y = 100. [MILLI METRE]
    Tabletop Thickness = 38.1 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Wheelchair Depth = 558.8 [MILLI METRE]
    Wheelchair Height = 838.2 [MILLI METRE]
    Wheelchair Width = 508. [MILLI METRE]
    Width for Wheelchair = 1117.6 [MILLI METRE]
    Width per Chair = 609.6 [MILLI METRE]
  AC_Equantity_Designer_Chair_11_21 | quantities | on 36 objects (36 IFCFURNISHINGELEMENT)
    Bottom Level = 1000. [MILLI METRE]
    Dimension 1 = 508. [MILLI METRE]
    Dimension 2 = 609.6 [MILLI METRE]
    Height = 838.2 [MILLI METRE]
    Minimal Space Behind = 304.8 [MILLI METRE]
    Minimal Space in Front = 31.75 [MILLI METRE]
    Minimal Space on Sides = 152.4 [MILLI METRE]
    Seat Height = 428.2 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Equantity_Coffee_Table_01_21 | quantities | on 12 objects (12 IFCFURNISHINGELEMENT)
    Bottom Level = 1000. [MILLI METRE]
    Dimension 1 = 304.8 [MILLI METRE]
    Dimension 2 = 304.8 [MILLI METRE]
    Minimal Space = 609.6 [MILLI METRE]
    Tabletop Height = 457.2 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Equantity_Zone_Stamp_01_21 | quantities | on 2 objects (2 IFCSPACE)
    Combined Width of Doors = 6996.72770097 [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Floor Level = 203.2 [MILLI METRE]
    Font Size for Detail Text (model) = 304.8 [MILLI METRE]
    Height = 3454.4 [MILLI METRE]
    Length of Perimeter Walls = 25425.3734666 [MILLI METRE]
    Net Perimeter = 89706.3491219 [MILLI METRE]
    Perimeter = 89706.3491219 [MILLI METRE]
    Perimeter of Holes = 3031.24 [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
  AC_Equantity_Zone_Stamp_01_21 | quantities | on 2 objects (2 IFCSPACE)
    Combined Width of Doors = 1015.59042916 [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Floor Level = 203.2 [MILLI METRE]
    Font Size for Detail Text (model) = 304.8 [MILLI METRE]
    Height = 3454.4 [MILLI METRE]
    Length of Perimeter Walls = 7171.11193931 [MILLI METRE]
    Net Perimeter = 7171.11193931 [MILLI METRE]
    Perimeter = 7171.11193931 [MILLI METRE]
    Perimeter of Holes = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
  AC_Equantity_Zone_Stamp_01_21 | quantities | on 2 objects (2 IFCSPACE)
    Combined Width of Doors = 1700.2125 [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Floor Level = 203.2 [MILLI METRE]
    Font Size for Detail Text (model) = 304.8 [MILLI METRE]
    Height = 3454.4 [MILLI METRE]
    Length of Perimeter Walls = 8273.35595789 [MILLI METRE]
    Net Perimeter = 8273.35595789 [MILLI METRE]
    Perimeter = 8273.35595789 [MILLI METRE]
    Perimeter of Holes = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
  AC_Equantity_Zone_Stamp_01_21 | quantities | on 2 objects (2 IFCSPACE)
    Combined Width of Doors = 850.10625 [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Floor Level = 203.2 [MILLI METRE]
    Font Size for Detail Text (model) = 304.8 [MILLI METRE]
    Height = 3454.4 [MILLI METRE]
    Length of Perimeter Walls = 10093.6072866 [MILLI METRE]
    Net Perimeter = 10093.6072866 [MILLI METRE]
    Perimeter = 10093.6072866 [MILLI METRE]
    Perimeter of Holes = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
  AC_Equantity_Zone_Stamp_01_21 | quantities | on 2 objects (2 IFCSPACE)
    Combined Width of Doors = 1700.2125 [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Floor Level = 203.2 [MILLI METRE]
    Font Size for Detail Text (model) = 304.8 [MILLI METRE]
    Height = 3454.4 [MILLI METRE]
    Length of Perimeter Walls = 8352.92126152 [MILLI METRE]
    Net Perimeter = 8352.92126152 [MILLI METRE]
    Perimeter = 8352.92126152 [MILLI METRE]
    Perimeter of Holes = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
  AC_Equantity_Zone_Stamp_01_21 | quantities | on 2 objects (2 IFCSPACE)
    Combined Width of Doors = 7836.46688258 [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Floor Level = 203.2 [MILLI METRE]
    Font Size for Detail Text (model) = 304.8 [MILLI METRE]
    Height = 3454.4 [MILLI METRE]
    Length of Perimeter Walls = 25425.3734666 [MILLI METRE]
    Net Perimeter = 89706.3491217 [MILLI METRE]
    Perimeter = 89706.3491217 [MILLI METRE]
    Perimeter of Holes = 3031.24 [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
  AC_Equantity_Zone_Stamp_01_21 | quantities | on 1 object (1 IFCSPACE)
    Combined Width of Doors = 850.10625 [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Floor Level = 263.525 [MILLI METRE]
    Font Size for Detail Text (model) = 304.8 [MILLI METRE]
    Height = 3394.075 [MILLI METRE]
    Length of Perimeter Walls = 10237.7699668 [MILLI METRE]
    Net Perimeter = 10723.8185818 [MILLI METRE]
    Perimeter = 10723.8185818 [MILLI METRE]
    Perimeter of Holes = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
  AC_Equantity_Zone_Stamp_01_21 | quantities | on 1 object (1 IFCSPACE)
    Combined Width of Doors = 850.10625 [MILLI METRE]
    Combined Width of Windows = 0. [MILLI METRE]
    Floor Level = 263.525 [MILLI METRE]
    Font Size for Detail Text (model) = 304.8 [MILLI METRE]
    Height = 3394.075 [MILLI METRE]
    Length of Perimeter Walls = 11944.6328128 [MILLI METRE]
    Net Perimeter = 10093.6072866 [MILLI METRE]
    Perimeter = 10093.6072866 [MILLI METRE]
    Perimeter of Holes = 0. [MILLI METRE]
    Subfloor Thickness = 0. [MILLI METRE]
  AC_Equantity_Zone_Stamp_01_21: 6 more contents on 6 objects not shown
  AC_Equantity_Curved_Beam | quantities | on 6 objects (6 IFCBEAM)
    Bottom Level = 1000. [MILLI METRE]
    Dimension 1 = 3880.81455231 [MILLI METRE]
    Dimension 2 = 190.500259399 [MILLI METRE]
    Height = 7759.73138213 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Equantity_Kitchen_Layout_21 | quantities | on 2 objects (2 IFCFURNISHINGELEMENT)
    Bottom Level = 1000. [MILLI METRE]
    Counter Depth = 609.6 [MILLI METRE]
    Countertop Height = 914.4 [MILLI METRE]
    Countertop Thickness = 50.8 [MILLI METRE]
    Dimension 1 = 3000. [MILLI METRE]
    Dimension 2 = 609.6 [MILLI METRE]
    Font Size = 120. [MILLI METRE]
    Height = 2286. [MILLI METRE]
    Hood Top Height = 2286. [MILLI METRE]
    Last Point = 0. [MILLI METRE]
    Minimal Space in Front = 914.4 [MILLI METRE]
    Refrigerators Depth = 762. [MILLI METRE]
    Refrigerators Height = 1828.8 [MILLI METRE]
    Sinks Width = 304.7 [MILLI METRE]
    Toe Height = 101.6 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Wall Cabinet Clearance = 609.6 [MILLI METRE]
    Wall Cabinet Depth = 304.8 [MILLI METRE]
    Wall Cabinet Height = 762. [MILLI METRE]
  AC_Equantity_Office_Layout_Linear_21 | quantities | on 8 objects (8 IFCFURNISHINGELEMENT)
    Base Height (gs_baseHeight) = 38.1 [MILLI METRE]
    Base Height (partitionBaseHeight) = 0. [MILLI METRE]
    Bottom Drawer Height = 350. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Cabinet Depth = 508. [MILLI METRE]
    Cabinet Height = 1066.8 [MILLI METRE]
    Cabinet Width = 609.6 [MILLI METRE]
    Chair Depth = 609.6 [MILLI METRE]
    Chair Height = 1140. [MILLI METRE]
    Chair Width = 609.6 [MILLI METRE]
    Desk Cabinet Width = 406.4 [MILLI METRE]
    Dimension 1 = 3048. [MILLI METRE]
    Dimension 2 = 1219.2 [MILLI METRE]
    Dimension 3 = 762. [MILLI METRE]
    Drawer Height = 203.2 [MILLI METRE]
    Drawer Thickness = 12.7 [MILLI METRE]
    Extension Cabinet Base Height = 38.1 [MILLI METRE]
    Extra Desk Chair Distance = 508. [MILLI METRE]
    Extra Desk Chair Distance X = 0. [MILLI METRE]
    Extra Desk Depth = 609.6 [MILLI METRE]
    Extra Desk Width = 1219.2 [MILLI METRE]
    Front Panel Height = 711.2 [MILLI METRE]
    Front Panel Top Height = 736.6 [MILLI METRE]
    Half Extra Desk Width for Hotspot Editing = 609.6 [MILLI METRE]
    Horizontal Knob Position = 0. [MILLI METRE]
    Inner Arc End Position = 914.4 [MILLI METRE]
    Inner Arc Start X Position = 900. [MILLI METRE]
    Inner Corner X Position = 600. [MILLI METRE]
    Length Left = 0. [MILLI METRE]
    Length Right = 4242.64068712 [MILLI METRE]
    Minimal Space in front of Desks = 1219.2 [MILLI METRE]
    Minimal Space on Side 1 = 762. [MILLI METRE]
    Minimal Space on Side 2 = 762. [MILLI METRE]
    Partition Height = 406.4 [MILLI METRE]
    Radius = 304.8 [MILLI METRE]
    Real Table-Chair Distance 1 = 0. [MILLI METRE]
    Seat Height = 400. [MILLI METRE]
    Table Depth 1 = 609.6 [MILLI METRE]
    Table Depth 2 = 609.6 [MILLI METRE]
    Table Length 1 = 1524. [MILLI METRE]
    Table Length 2 = 1524. [MILLI METRE]
    Table-Chair Distance 1 = 0. [MILLI METRE]
    Table-Chair Distance 2 = 508. [MILLI METRE]
    Tabletop Height = 762. [MILLI METRE]
    Tabletop Thickness = 19.05 [MILLI METRE]
    Top Drawer Height = 100. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Total Height of Drawers = 647.7 [MILLI METRE]
    Total Length of Workstations = 3048. [MILLI METRE]
    Upper Cabinet Height = 419.1 [MILLI METRE]
  AC_Equantity_Office_Layout_Linear_21 | quantities | on 4 objects (4 IFCFURNISHINGELEMENT)
    Base Height (gs_baseHeight) = 38.1 [MILLI METRE]
    Base Height (partitionBaseHeight) = 0. [MILLI METRE]
    Bottom Drawer Height = 350. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Cabinet Depth = 508. [MILLI METRE]
    Cabinet Height = 1066.8 [MILLI METRE]
    Cabinet Width = 609.6 [MILLI METRE]
    Chair Depth = 609.6 [MILLI METRE]
    Chair Height = 1140. [MILLI METRE]
    Chair Width = 609.6 [MILLI METRE]
    Desk Cabinet Width = 406.4 [MILLI METRE]
    Dimension 1 = 1524. [MILLI METRE]
    Dimension 2 = 1219.2 [MILLI METRE]
    Dimension 3 = 762. [MILLI METRE]
    Drawer Height = 203.2 [MILLI METRE]
    Drawer Thickness = 12.7 [MILLI METRE]
    Extension Cabinet Base Height = 38.1 [MILLI METRE]
    Extra Desk Chair Distance = 508. [MILLI METRE]
    Extra Desk Chair Distance X = 0. [MILLI METRE]
    Extra Desk Depth = 609.6 [MILLI METRE]
    Extra Desk Width = 1219.2 [MILLI METRE]
    Front Panel Height = 711.2 [MILLI METRE]
    Front Panel Top Height = 736.6 [MILLI METRE]
    Half Extra Desk Width for Hotspot Editing = 609.6 [MILLI METRE]
    Horizontal Knob Position = 0. [MILLI METRE]
    Inner Arc End Position = 914.4 [MILLI METRE]
    Inner Arc Start X Position = 900. [MILLI METRE]
    Inner Corner X Position = 600. [MILLI METRE]
    Length Left = 0. [MILLI METRE]
    Length Right = 4242.64068712 [MILLI METRE]
    Minimal Space in front of Desks = 1219.2 [MILLI METRE]
    Minimal Space on Side 1 = 762. [MILLI METRE]
    Minimal Space on Side 2 = 762. [MILLI METRE]
    Partition Height = 406.4 [MILLI METRE]
    Radius = 304.8 [MILLI METRE]
    Real Table-Chair Distance 1 = 0. [MILLI METRE]
    Seat Height = 400. [MILLI METRE]
    Table Depth 1 = 609.6 [MILLI METRE]
    Table Depth 2 = 609.6 [MILLI METRE]
    Table Length 1 = 1524. [MILLI METRE]
    Table Length 2 = 1524. [MILLI METRE]
    Table-Chair Distance 1 = 0. [MILLI METRE]
    Table-Chair Distance 2 = 508. [MILLI METRE]
    Tabletop Height = 762. [MILLI METRE]
    Tabletop Thickness = 19.05 [MILLI METRE]
    Top Drawer Height = 100. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Total Height of Drawers = 647.7 [MILLI METRE]
    Total Length of Workstations = 1524. [MILLI METRE]
    Upper Cabinet Height = 419.1 [MILLI METRE]
  AC_Equantity_D1_Combi_Commercial_21 | quantities | on 1 object (1 IFCDOOR)
    3D Closed Height = 0. [MILLI METRE]
    3D Closed Length = 0. [MILLI METRE]
    3D Opening Height = 1500. [MILLI METRE]
    3D Opening Length 1 = 560. [MILLI METRE]
    3D Opening Length 2 = 140. [MILLI METRE]
    3D Opening Length = 1500. [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Box Axis Height from Header = 0. [MILLI METRE]
    Box Depth (gs_shutLam_boxWidth) = 150. [MILLI METRE]
    Box Depth (gs_shutRoll_boxWidth) = 150. [MILLI METRE]
    Box Height (gs_shutLam2_boxHeight) = 60. [MILLI METRE]
    Box Height (gs_shutLam_boxHeight) = 200. [MILLI METRE]
    Box Height (gs_shutRoll_boxHeight) = 200. [MILLI METRE]
    Box Left Offset = 0. [MILLI METRE]
    Box Right Offset = 0. [MILLI METRE]
    Box Width = 60. [MILLI METRE]
    Brick Thickness (gs_brick_sill_br_thk) = 65. [MILLI METRE]
    Brick Thickness (gs_masonry_arch_brick_thk) = 66.675 [MILLI METRE]
    Closer Thickness = 100. [MILLI METRE]
    Closer Width = 38. [MILLI METRE]
    Closing Depth = 0. [MILLI METRE]
    Cover Width = 0. [MILLI METRE]
    Custom Thickness = 15. [MILLI METRE]
    Dead Bolt Height = 1066.8 [MILLI METRE]
    Depth of Rails = 72.5 [MILLI METRE]
    Distance between Arch and Door = 0. [MILLI METRE]
    Distance from Header (gs_shutLam2_distFromHead) = 60. [MILLI METRE]
    Distance from Header (gs_shutLam_distFromHead) = 0. [MILLI METRE]
    Distance from Header (gs_shutRoll_distFromHead) = 0. [MILLI METRE]
    Distance from Wall (gs_shutLam_distFromWall) = 0. [MILLI METRE]
    Distance from Wall (gs_shutRoll_distFromWall) = 0. [MILLI METRE]
    Distance from Window = 60. [MILLI METRE]
    Distance of Skin from Closer = 0. [MILLI METRE]
    Door Panel Overlap Width = 50.8 [MILLI METRE]
    Door Stop Projection = 44.45 [MILLI METRE]
    Door Stop Thickness = 50.8 [MILLI METRE]
    Door Stop Width = 25.4 [MILLI METRE]
    Egress Height = 2006.6 [MILLI METRE]
    Egress Width = 863.6 [MILLI METRE]
    Ext. Threshold Overhang Inside = 50.8 [MILLI METRE]
    Ext. Threshold Overhang Outside = 50.8 [MILLI METRE]
    Extra Frame Thickness = 30. [MILLI METRE]
    Extra Frame Width = 40. [MILLI METRE]
    Frame Thickness = 101.6 [MILLI METRE]
    Frame Thickness Inside = 101.6 [MILLI METRE]
    Frame Width = 50.8 [MILLI METRE]
    Frame Width Bottom = 50. [MILLI METRE]
    Frame Width Left = 50.8 [MILLI METRE]
    Frame Width Right = 50.8 [MILLI METRE]
    Frame Width Upper = 50.8 [MILLI METRE]
    Glass Thickness = 12.7 [MILLI METRE]
    Grid Thickness = 19.05 [MILLI METRE]
    Grid Width = 12.7 [MILLI METRE]
    Handle Height = 914.4 [MILLI METRE]
    Handle Position = 50.8 [MILLI METRE]
    Hanging Stick Length = 20. [MILLI METRE]
    Hanging Stick Radius = 5. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_left_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_right_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_left_out) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_right_out) = 0. [MILLI METRE]
    Head Jamb Depth = 31.75 [MILLI METRE]
    Head Width Inside = 63.5 [MILLI METRE]
    Head Width Outside = 63.5 [MILLI METRE]
    Hole Radius = 10. [MILLI METRE]
    Horizontal Boards Approximate Width = 115. [MILLI METRE]
    Horizontal Boards Thickness = 25. [MILLI METRE]
    Horizontal Frame Divider Width = 50. [MILLI METRE]
    Inner Head Depth (gs_reveal_double_innerTop) = 101.6 [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 101.6 [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 101.6 [MILLI METRE]
    Inner Offset = 20. [MILLI METRE]
    Inner Panel Width = 120. [MILLI METRE]
    Inner Sill Depth (gs_reveal_double_innerBottom) = 101.6 [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 101.6 [MILLI METRE]
    Jamb Depth = 31.75 [MILLI METRE]
    Jamb Depth Side 2 = 31.75 [MILLI METRE]
    Jamb Extension Width = 12.7 [MILLI METRE]
    Jamb Extension Width Outside = 0. [MILLI METRE]
    Keystone Oversize = 0. [MILLI METRE]
    Keystone Projection = 10. [MILLI METRE]
    Keystone Width = 100. [MILLI METRE]
    Leaf Frame Width Internal = 25.4 [MILLI METRE]
    Leaf Frame Width Left = 101.6 [MILLI METRE]
    Leaf Frame Width Lower = 101.6 [MILLI METRE]
    Leaf Frame Width Right = 101.6 [MILLI METRE]
    Leaf Frame Width Side = 101.6 [MILLI METRE]
    Leaf Frame Width Upper = 101.6 [MILLI METRE]
    Leaf Height = 2032. [MILLI METRE]
    Leaf Thickness = 44.45 [MILLI METRE]
    Leaf Width = 914.4 [MILLI METRE]
    Left Opening Oversize = 0. [MILLI METRE]
    Left Panel Width = 254. [MILLI METRE]
    Louver Thickness = 10. [MILLI METRE]
    Louver Width = 40. [MILLI METRE]
    Lower Opening Oversize = 0. [MILLI METRE]
    Main Door Panel Width = 457.2 [MILLI METRE]
    Masonry Arch Depth = 101.6 [MILLI METRE]
    Masonry Arch Height = 203.2 [MILLI METRE]
    Masonry Arch Overhang Left = 0. [MILLI METRE]
    Masonry Arch Overhang Right = 0. [MILLI METRE]
    Masonry Arch Projection = 0. [MILLI METRE]
    Masonry Arch Rise = 50.8 [MILLI METRE]
    Middle Frame Width = 101.6 [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 15. [MILLI METRE]
    Mortar Thickness (gs_masonry_arch_mort_thk) = 9.525 [MILLI METRE]
    Offset Inside = 0. [MILLI METRE]
    Offset Outside = 25.4 [MILLI METRE]
    Offset from Edge if not Center = 152.4 [MILLI METRE]
    Opening Side Depth = 1524. [MILLI METRE]
    Opening Side Width 1 = 0. [MILLI METRE]
    Opening Side Width 2 = 457.2 [MILLI METRE]
    Opening Width in 2D = 0. [MILLI METRE]
    Opening Width in 3D = 0. [MILLI METRE]
    Outer Jamb Depth = 80. [MILLI METRE]
    Outside Overhang = 0. [MILLI METRE]
    Overhang 1 Left = 22.225 [MILLI METRE]
    Overhang 1 Right = 22.225 [MILLI METRE]
    Overhang 1 Upper = 22.225 [MILLI METRE]
    Panel Distance = 6. [MILLI METRE]
    Panel Fill Thickness = 10. [MILLI METRE]
    Panel Frame Width = 50.8 [MILLI METRE]
    Panel Height = 1500. [MILLI METRE]
    Panel Thickness = 50.8 [MILLI METRE]
    Panel Width = 0. [MILLI METRE]
    Plaster Thickness Limit = 38.1 [MILLI METRE]
    Profile Width = 150. [MILLI METRE]
    Rail Height = 914.4 [MILLI METRE]
    Rail Width = 38.1 [MILLI METRE]
    Rear Hole Depth = 0. [MILLI METRE]
    Rebate Width = 12.7 [MILLI METRE]
    Reveal Depth (AC_wido_sill) = 0. [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 0. [MILLI METRE]
    Reveal Height = 2387.6 [MILLI METRE]
    Reveal Width = 1320.8 [MILLI METRE]
    Reveal to Wall Core = 0. [MILLI METRE]
    Right Opening Oversize = 0. [MILLI METRE]
    Right Panel Width = 254. [MILLI METRE]
    Segment Width (gs_shutLam2_segmentWidth) = 60. [MILLI METRE]
    Segment Width (gs_shutLam_segmentWidth) = 60. [MILLI METRE]
    Side Width Inside = 63.5 [MILLI METRE]
    Side Width Outside = 63.5 [MILLI METRE]
    Sidelight Frame Thickness = 38.1 [MILLI METRE]
    Sidelight Frame Width = 50.8 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left) = 355.6 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_half) = 177.8 [MILLI METRE]
    Sidelight Width Left (gs_sidelight_width_left_orig) = 355.6 [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right) = 355.6 [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_half) = 177.8 [MILLI METRE]
    Sidelight Width Right (gs_sidelight_width_right_orig) = 355.6 [MILLI METRE]
    Sill Height to Current Story = 212.725055714 [MILLI METRE]
    Sill Jamb Depth = 60. [MILLI METRE]
    Sill Nosing = 31.75 [MILLI METRE]
    Sill Overhang Left = 0. [MILLI METRE]
    Sill Overhang Right = 0. [MILLI METRE]
    Sill Slip-in Depth = 25.4 [MILLI METRE]
    Sill Thickness = 100. [MILLI METRE]
    Sill Top Height = 10. [MILLI METRE]
    Sill Top Width = 10. [MILLI METRE]
    Skin Overhang to Frame Depth = 0. [MILLI METRE]
    Slat Width = 50. [MILLI METRE]
    Strip Thickness = 25. [MILLI METRE]
    Thickness Inside = 31.75 [MILLI METRE]
    Thickness Outside = 31.75 [MILLI METRE]
    Threshold External Thickness = 5.80737765736 [MILLI METRE]
    Threshold Nosing Inside = 25.4 [MILLI METRE]
    Threshold Nosing Outside = 25.4 [MILLI METRE]
    Threshold Thickness = 12.7 [MILLI METRE]
    Threshold Width = 10. [MILLI METRE]
    Tolerance Left = 0. [MILLI METRE]
    Tolerance Lower = 0. [MILLI METRE]
    Tolerance Right = 0. [MILLI METRE]
    Tolerance Upper = 0. [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Transom Frame Thickness = 38.1 [MILLI METRE]
    Transom Frame Width = 50.8 [MILLI METRE]
    Transom Height (gs_transom_height) = 355.6 [MILLI METRE]
    Transom Height (gs_transom_height_top) = 355.6 [MILLI METRE]
    Unit Height = 2387.6 [MILLI METRE]
    Unit Width = 1320.8 [MILLI METRE]
    Upper Opening Oversize = 0. [MILLI METRE]
    Vertical Board Width = 100. [MILLI METRE]
    Vertical Boards Approximate Width = 80. [MILLI METRE]
    Vertical Boards Thickness = 25. [MILLI METRE]
    Vertical Frame Divider Width = 50. [MILLI METRE]
    Vertical Grid Height = 914.4 [MILLI METRE]
    Wallhole Height = 2387.6 [MILLI METRE]
    Wallhole Width = 1320.8 [MILLI METRE]
    Width Side (gs_tw_left_in) = 63.5 [MILLI METRE]
    Width Side (gs_tw_left_out) = 63.5 [MILLI METRE]
    Width of Sill = 0. [MILLI METRE]
    Window Height = 304.8 [MILLI METRE]
    Window Sill Height = 1524. [MILLI METRE]
    Window Width = 304.8 [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
    Z Frame Thickness = 25. [MILLI METRE]
    Z Frame Width = 50. [MILLI METRE]
  AC_Equantity_W_Round_Pivot_21 | quantities | on 1 object (1 IFCWINDOW)
    3D Closed Height = 0. [MILLI METRE]
    3D Closed Length = 0. [MILLI METRE]
    3D Opening Height = 1500. [MILLI METRE]
    3D Opening Length 1 = 560. [MILLI METRE]
    3D Opening Length 2 = 140. [MILLI METRE]
    3D Opening Length = 1500. [MILLI METRE]
    AC Left Opening Oversize = 44.45 [MILLI METRE]
    AC Lower Opening Oversize = -0. [MILLI METRE]
    AC Right Opening Oversize = 44.45 [MILLI METRE]
    AC Upper Opening Oversize = 88.9 [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Bottom Overhang = 0. [MILLI METRE]
    Bottom Width Inside = 63.5 [MILLI METRE]
    Bottom Width Outside = 63.5 [MILLI METRE]
    Box Axis Height from Header = 0. [MILLI METRE]
    Box Depth (gs_shutLam_boxWidth) = 150. [MILLI METRE]
    Box Depth (gs_shutRoll_boxWidth) = 150. [MILLI METRE]
    Box Height (gs_shutLam2_boxHeight) = 60. [MILLI METRE]
    Box Height (gs_shutLam_boxHeight) = 200. [MILLI METRE]
    Box Height (gs_shutRoll_boxHeight) = 200. [MILLI METRE]
    Box Left Offset = 0. [MILLI METRE]
    Box Right Offset = 0. [MILLI METRE]
    Box Width = 60. [MILLI METRE]
    Brick Thickness (gs_brick_sill_br_thk) = 65. [MILLI METRE]
    Brick Thickness (gs_masonry_arch_brick_thk) = 66.675 [MILLI METRE]
    Casing Thickness = 50.8 [MILLI METRE]
    Casing Width = 25. [MILLI METRE]
    Closer Thickness = 100. [MILLI METRE]
    Closer Width = 38. [MILLI METRE]
    Closing Depth = 0. [MILLI METRE]
    Cover Width = 0. [MILLI METRE]
    Custom Thickness = 15. [MILLI METRE]
    Depth of Inset = 50. [MILLI METRE]
    Depth of Rails = 72.5 [MILLI METRE]
    Distance between Arch and Window = 0. [MILLI METRE]
    Distance from Header (gs_shutLam2_distFromHead) = 60. [MILLI METRE]
    Distance from Header (gs_shutLam_distFromHead) = 0. [MILLI METRE]
    Distance from Header (gs_shutRoll_distFromHead) = 0. [MILLI METRE]
    Distance from Wall (gs_shutLam_distFromWall) = 0. [MILLI METRE]
    Distance from Wall (gs_shutRoll_distFromWall) = 0. [MILLI METRE]
    Distance from Window = 60. [MILLI METRE]
    Distance of Skin from Closer = 0. [MILLI METRE]
    Extra Frame Thickness = 30. [MILLI METRE]
    Extra Frame Width = 40. [MILLI METRE]
    Frame Thickness = 114.3 [MILLI METRE]
    Frame Width = 38.1 [MILLI METRE]
    Frame Width Bottom = 50. [MILLI METRE]
    Glass Thickness = 6.35 [MILLI METRE]
    Grill Thickness = 25. [MILLI METRE]
    Grill Width = 20. [MILLI METRE]
    Hanging Stick Length = 20. [MILLI METRE]
    Hanging Stick Radius = 5. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_left_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Inside (gs_trimov_top_right_in) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_left_out) = 0. [MILLI METRE]
    Head Casing Side Overhang Outside (gs_trimov_top_right_out) = 0. [MILLI METRE]
    Head Jamb Depth = 31.75 [MILLI METRE]
    Head Width Inside = 63.5 [MILLI METRE]
    Head Width Outside = 38.1 [MILLI METRE]
    Height = 1398.40769111 [MILLI METRE]
    Hole Radius = 10. [MILLI METRE]
    Horizontal Boards Approximate Width = 115. [MILLI METRE]
    Horizontal Boards Thickness = 25. [MILLI METRE]
    Horizontal Frame Divider Width = 50. [MILLI METRE]
    Inner Head Depth (gs_reveal_double_innerTop) = 60. [MILLI METRE]
    Inner Head Depth (gs_reveal_splayed_innerTop) = 60. [MILLI METRE]
    Inner Jamb Depth (gs_reveal_double_innerRight) = 60. [MILLI METRE]
    Inner Jamb Depth (gs_reveal_splayed_innerRight) = 60. [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_double_innerLeft) = 60. [MILLI METRE]
    Inner Jamb Depth Side 2 (gs_reveal_splayed_innerLeft) = 60. [MILLI METRE]
    Inner Offset = 12.7 [MILLI METRE]
    Inner Panel Width = 120. [MILLI METRE]
    Inner Sill Depth (gs_reveal_double_innerBottom) = 60. [MILLI METRE]
    Inner Sill Depth (gs_reveal_splayed_innerBottom) = 60. [MILLI METRE]
    Jamb Depth = 31.75 [MILLI METRE]
    Jamb Depth Side 2 = 31.75 [MILLI METRE]
    Jamb Extension Width = 12.7 [MILLI METRE]
    Jamb Extension Width Outside = 0. [MILLI METRE]
    Keystone Oversize = 0. [MILLI METRE]
    Keystone Projection = 10. [MILLI METRE]
    Keystone Width = 101.6 [MILLI METRE]
    Left Opening Oversize = 0. [MILLI METRE]
    Louver Thickness = 10. [MILLI METRE]
    Louver Width = 40. [MILLI METRE]
    Lower Opening Oversize = 0. [MILLI METRE]
    Masonry Arch Depth = 101.6 [MILLI METRE]
    Masonry Arch Height = 203.2 [MILLI METRE]
    Masonry Arch Overhang Left = 0. [MILLI METRE]
    Masonry Arch Overhang Right = 0. [MILLI METRE]
    Masonry Arch Projection = 0. [MILLI METRE]
    Masonry Arch Rise = 50.8 [MILLI METRE]
    Maximal Tolerance = 100. [MILLI METRE]
    Modified Frame Thickness = 114.3 [MILLI METRE]
    Mortar Thickness (gs_brick_sill_mort_thk) = 15. [MILLI METRE]
    Mortar Thickness (gs_masonry_arch_mort_thk) = 9.525 [MILLI METRE]
    Offset Inside = 0. [MILLI METRE]
    Offset Outside = -38.1 [MILLI METRE]
    Outer Jamb Depth = 80. [MILLI METRE]
    Outside Overhang = 0. [MILLI METRE]
    Overhang Side 1 = 0. [MILLI METRE]
    Overhang Side 2 = 0. [MILLI METRE]
    Panel Distance = 6. [MILLI METRE]
    Panel Fill Thickness = 10. [MILLI METRE]
    Panel Frame Width = 50.8 [MILLI METRE]
    Panel Height = 1500. [MILLI METRE]
    Panel Thickness = 38.1 [MILLI METRE]
    Panel Width = 0. [MILLI METRE]
    Parapet Height = 900. [MILLI METRE]
    Parapet Width = 1000. [MILLI METRE]
    Plaster Thickness Limit = 38.1 [MILLI METRE]
    Profile Width = 76.2 [MILLI METRE]
    Rail Width = 30. [MILLI METRE]
    Rear Hole Depth (gs_masonry_arch_rearHoleDepth) = 0. [MILLI METRE]
    Rear Hole Depth (gs_sill_holeDepthBehind) = 0. [MILLI METRE]
    Reveal Depth (AC_wido_sill) = 15.875 [MILLI METRE]
    Reveal Depth (gs_wido_sill) = 15.875 [MILLI METRE]
    Reveal Height = 1487.30769111 [MILLI METRE]
    Reveal Width = 1487.30769111 [MILLI METRE]
    Reveal to Wall Core = 15.875 [MILLI METRE]
    Right Opening Oversize = 0. [MILLI METRE]
    Sash Frame Thickness = 44.45 [MILLI METRE]
    Sash Frame Width = 57.15 [MILLI METRE]
    Sash Setback = 25.4 [MILLI METRE]
    Segment Width (gs_shutLam2_segmentWidth) = 60. [MILLI METRE]
    Segment Width (gs_shutLam_segmentWidth) = 60. [MILLI METRE]
    Side Casing Bottom Overhang Inside (gs_trimov_bot_left_in) = 0. [MILLI METRE]
    Side Casing Bottom Overhang Inside (gs_trimov_bot_right_in) = 0. [MILLI METRE]
    Side Casing Bottom Overhang Outside (gs_trimov_bot_left_out) = 0. [MILLI METRE]
    Side Casing Bottom Overhang Outside (gs_trimov_bot_right_out) = 0. [MILLI METRE]
    Side Width Inside = 63.5 [MILLI METRE]
    Side Width Outside = 38.1 [MILLI METRE]
    Sill Drip Overlap = 20. [MILLI METRE]
    Sill Drip Width = 30. [MILLI METRE]
    Sill Elevation = 0. [MILLI METRE]
    Sill Front Side Thickness = 15. [MILLI METRE]
    Sill Height to Current Story = 1039.99230889 [MILLI METRE]
    Sill Jamb Depth = 31.75 [MILLI METRE]
    Sill Nosing = 30. [MILLI METRE]
    Sill Overhang Left = 0. [MILLI METRE]
    Sill Overhang Right = 0. [MILLI METRE]
    Sill Slip-in Depth = 20. [MILLI METRE]
    Sill Thickness = 25. [MILLI METRE]
    Sill Top Height = 10. [MILLI METRE]
    Sill Top Width = 10. [MILLI METRE]
    Skin Overhang to Frame Depth = 0. [MILLI METRE]
    Slat Width = 50. [MILLI METRE]
    Stool Nosing = 30. [MILLI METRE]
    Stool Overhang Left = 0. [MILLI METRE]
    Stool Overhang Right = 0. [MILLI METRE]
    Stool Slip-in Depth = 0. [MILLI METRE]
    Stool Thickness = 25. [MILLI METRE]
    Stool Width = 101.6 [MILLI METRE]
    Strip Thickness = 25.4 [MILLI METRE]
    Thickness Inside = 12.7 [MILLI METRE]
    Thickness Outside = 31.75 [MILLI METRE]
    Tolerance (gs_tolerance) = 0. [MILLI METRE]
    Tolerance (gs_tolerance_left) = 44.45 [MILLI METRE]
    Tolerance Lower = 44.45 [MILLI METRE]
    Tolerance Right = 44.45 [MILLI METRE]
    Tolerance Upper = 44.45 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Unit Height = 1398.40769111 [MILLI METRE]
    Unit Width = 1398.40769111 [MILLI METRE]
    Upper Opening Oversize = 0. [MILLI METRE]
    Vertical Board Width = 100. [MILLI METRE]
    Vertical Boards Approximate Width = 80. [MILLI METRE]
    Vertical Boards Thickness = 25. [MILLI METRE]
    Vertical Frame Divider Width = 50. [MILLI METRE]
    Wallhole Height = 1487.30769111 [MILLI METRE]
    Wallhole Width = 1487.30769111 [MILLI METRE]
    Width = 1398.40769111 [MILLI METRE]
    Width Side (gs_tw_left_in) = 63.5 [MILLI METRE]
    Width Side (gs_tw_left_out) = 38.1 [MILLI METRE]
    Width of Sill = 0. [MILLI METRE]
    Z Dimension = 1000. [MILLI METRE]
    Z Frame Thickness = 25. [MILLI METRE]
    Z Frame Width = 50. [MILLI METRE]
  AC_Equantity_Office_Workstation_Solo_21 | quantities | on 1 object (1 IFCFURNISHINGELEMENT)
    Base Height (gs_baseHeight) = 38.1 [MILLI METRE]
    Base Height (partitionBaseHeight) = 0. [MILLI METRE]
    Bottom Drawer Height = 355.6 [MILLI METRE]
    Bottom Level = 1000. [MILLI METRE]
    Chair Depth = 609.6 [MILLI METRE]
    Chair Height = 1040. [MILLI METRE]
    Chair Width = 609.6 [MILLI METRE]
    Custom Length = 1524. [MILLI METRE]
    Custom Offset = 0. [MILLI METRE]
    Desk Cabinet Width = 406.4 [MILLI METRE]
    Dimension 1 = 2743.2 [MILLI METRE]
    Dimension 2 = 914.4 [MILLI METRE]
    Dimension 3 = 762. [MILLI METRE]
    Drawer Thickness = 12.7 [MILLI METRE]
    Front Panel Height = 762. [MILLI METRE]
    Front Panel Top Height = 762. [MILLI METRE]
    Horizontal Knob Position = 0. [MILLI METRE]
    Inner Arc End Position = 527.929086147 [MILLI METRE]
    Inner Arc Start X Position = 527.929086147 [MILLI METRE]
    Inner Corner X Position = 351.952724098 [MILLI METRE]
    Minimal Space Length = 1400. [MILLI METRE]
    Minimal Space in front of Desks = 1219.2 [MILLI METRE]
    Minimal Space on Side 1 = 1524. [MILLI METRE]
    Minimal Space on Side 2 = 1524. [MILLI METRE]
    Partition Height = 1150. [MILLI METRE]
    Radius = 304.8 [MILLI METRE]
    Real Table-Chair Distance 1 = 288.675134595 [MILLI METRE]
    Seat Height = 400. [MILLI METRE]
    Table Depth 1 = 914.4 [MILLI METRE]
    Table Depth 2 = 609.6 [MILLI METRE]
    Table Length 1 = 2743.2 [MILLI METRE]
    Table Length 2 = 1524. [MILLI METRE]
    Table-Chair Distance 1 = 0. [MILLI METRE]
    Table-Chair Distance 2 = 500. [MILLI METRE]
    Tabletop Height = 762. [MILLI METRE]
    Tabletop Thickness = 19.05 [MILLI METRE]
    Top Drawer Height = 152.4 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
  AC_Equantity_Street_Lamp_04_21 | quantities | on 8 objects (8 IFCFLOWTERMINAL)
    Bottom Level = 1000. [MILLI METRE]
    Depth = 660.4 [MILLI METRE]
    Height = 3962.4 [MILLI METRE]
    Light Distance = 4000. [MILLI METRE]
    Post Diameter = 82.5 [MILLI METRE]
    Top Level = 0. [MILLI METRE]
    Width (A) = 660.4 [MILLI METRE]
    Width (A2) = 325. [MILLI METRE]
  Window Lining Properties | predefined | on 1 type object
  Window Panel Properties - Panel 1 | predefined | on 1 type object
  Door Lining Properties | predefined | on 6 type objects
  Door Panel Properties - Panel 1 | predefined | on 6 type objects
  Door Panel Properties - Panel 2 | predefined | on 1 type object